{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["CalculateurRE2020","drop down content & text","FDES (EPD)","results ready","climate zones"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":17,"comments":2,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"CalculateurRE2020","index":0,"n_rows":56,"n_cols":13,"rows_kept":56,"cut":false,"hidden":false,"merged":[[16,7,20,9],[16,1,18,3],[37,1,44,3],[45,1,46,3],[19,1,19,5],[6,2,6,3],[3,2,4,4],[47,1,55,3],[9,1,15,3],[8,1,8,5],[20,1,36,3]]}
[]
[]
[]
[null,null,"       Calculateur RE2020"]
[null,null,null,null,null,"Note concernant le PDF"]
[]
[null,null,"Valide jusqu'au:",null,"2026-07-06","Vers. 1.02 /04-2026             "]
[null,null,null,"Dernière version:","link"]
[null,"Configuration du produit (cliquez sur les menus déroulants)"]
[null,"Choisissez une configuration de solutions VELUX",null,null,"Fenêtre:","GGLS (3-en-1, rotation)"]
[null,null,null,null,"Taille:","FFKF08 (1.880m x 1.398m)"]
[null,null,null,null,"Vitrage:","Tout confort (57)"]
[null,null,null,null,"Gestion d'ouverture des fenêtres:","Manuelle"]
[null,null,null,null,"Installation:","Standard"]
[null,null,null,null,"Protections solaires:","Volet roulant (SML, SSL, SSLS, SMG)"]
[null,null,null,null,"Gestion d'ouverture des protections solaires:","Aucun"]
[null,"Renseignez les informations ci-dessous concernant votre projet pour vérifier la conformité des solutions choisies aux exigences de facteur solaire (Sws) maximum de la RE2020",null,null,"Zone climatique et altitude:","H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m"]
[null,null,null,null,"Exposition au bruit et usage de la pièce:","Exposition BR1 - locaux destinés au sommeil"]
[null,null,null,null,"Pente et orientation:","Pente < 60°"]
[null,"Résultats"]
[null,"Fenêtre",null,null,"Description du produit",{"$f":"\"Fenêtre de toit \" &F10&\", \"&F11&\" avec vitrage \"&F12&\". \"&F13&\". En pose \"&F14& IF(F15='drop down content & text'!K2,\"\",\" avec \"&F15&IF(F16='drop down content & text'!G8,\"\",\" \"&F16))","v":"Fenêtre de toit GGLS (3-en-1, rotation), FFKF08 (1.880m x 1.398m) avec vitrage Tout confort (57). Manuelle. En pose Standard avec Volet roulant (SML, SSL, SSLS, SMG)"}]
[null,null,null,null,"Product name short",{"$f":"VLOOKUP(F10,Product,2,FALSE)& \" \" & VLOOKUP(F11,Size,2,FALSE) & \" \" &VLOOKUP(F12,Glazing,2,FALSE) & \" \" & VLOOKUP(F14,Installation,2,FALSE)","v":"GGLS FFKF08 57 Standard"},"Hide later",null,null,null,null,null,"XML download funktion"]
[null,null,null,null,"Product",{"$f":"VLOOKUP(F15,Assessories,2,FALSE)","v":"Shutter"},"Hide later",null,null,null,null,null,"PDF conversion"]
[null,null,null,null,"TestID",{"$f":"VLOOKUP(F22,Results_all,53,FALSE)","v":1242},"Hide later"]
[null,null,null,null,"Valeur max de Sws autorisée",{"$f":"VLOOKUP(F17&\" \"&F18&\" \"&F19,climate_zones_Sws_max,5,FALSE)","v":0.25}]
[null,null,null,null,"Gestion d'ouverture de la fenêtre",{"$f":"VLOOKUP(F13,Operation,2,FALSE)","v":"Ouverture manuelle"}]
[null,null,null,null,"Gestion d'ouverture de la protection mobile",{"$f":"VLOOKUP(F16,A_operation,2,FALSE)","v":"-"}]
[null,null,null,null,"Uw (90°)",{"$f":"_xlfn.IFNA(VLOOKUP(F22,Results_all,14,FALSE),'drop down content & text'!S2)","v":1.3}]
[null,null,null,null,"Uw (0°)",{"$f":"_xlfn.IFNA(VLOOKUP(F22,Results_all,15,FALSE),'drop down content & text'!S2)","v":1.8}]
[null,null,null,null,"Swc1",{"$f":"_xlfn.IFNA(VLOOKUP(F22,Results_all,26,FALSE),'drop down content & text'!S2)","v":0.19}]
[null,null,null,null,"Swc2",{"$f":"_xlfn.IFNA(VLOOKUP(F22,Results_all,27,FALSE),'drop down content & text'!S2)","v":0.04}]
[null,null,null,null,"Swc3",{"$f":"_xlfn.IFNA(VLOOKUP(F22,Results_all,28,FALSE),'drop down content & text'!S2)","v":0}]
[null,null,null,null,"Swe1",{"$f":"_xlfn.IFNA(VLOOKUP(F22,Results_all,29,FALSE),'drop down content & text'!S2)","v":0.19}]
[null,null,null,null,"Swe2",{"$f":"_xlfn.IFNA(VLOOKUP(F22,Results_all,30,FALSE),'drop down content & text'!S2)","v":0.05}]
[null,null,null,null,"Swe3",{"$f":"_xlfn.IFNA(VLOOKUP(F22,Results_all,31,FALSE),'drop down content & text'!S2)","v":0}]
[null,null,null,null,"TLw",{"$f":"_xlfn.IFNA(VLOOKUP(F22,Results_all,44,FALSE),'drop down content & text'!S2)","v":0.44}]
[null,null,null,null,"TLw diff",{"$f":"_xlfn.IFNA(VLOOKUP(F22,Results_all,45,FALSE),'drop down content & text'!S2)","v":0}]
[null,"Fenêtre avec protection solaire",null,null,"Uws (90°)",{"$f":"_xlfn.IFNA(IF(F23='drop down content & text'!L2,F28,VLOOKUP(F22,Results_all,IF(F23='drop down content & text'!L3,\"16\",IF(OR(F23='drop down content & text'!L4,F23='drop down content & text'!L5),\"18\",IF(F23='drop down content & text'!L6,\"20\",IF(F23='drop down content & text'!L7,\"22\",IF(OR(F23='drop down content & text'!L8,F23='drop down content & text'!L9),\"24\"))))),FALSE)),'drop down content & text'!S2)","v":1.2}]
[null,null,null,null,"Uws(0°)",{"$f":"_xlfn.IFNA(IF(F23='drop down content & text'!L2,F29,VLOOKUP(F22,Results_all,IF(F23='drop down content & text'!L3,\"17\",IF(OR(F23='drop down content & text'!L4,F23='drop down content & text'!L5),\"19\",IF(F23='drop down content & text'!L6,\"21\",IF(F23='drop down content & text'!L7,\"23\",IF(OR(F23='drop down content & text'!L8,F23='drop down content & text'!L9),\"25\"))))),FALSE)),'drop down content & text'!S2)","v":1.5}]
[null,null,null,null,"Sws1",{"$f":"_xlfn.IFNA(IF(OR(F23='drop down content & text'!L2,F23='drop down content & text'!L6),F33,VLOOKUP(F22,Results_all,IF(OR(F23='drop down content & text'!L3,F23='drop down content & text'!L7),\"32\",IF(OR(F23='drop down content & text'!L4,F23='drop down content & text'!L8),\"40\",IF(OR(F23='drop down content & text'!L5,F23='drop down content & text'!L9),\"36\",))),FALSE)),'drop down content & text'!S2)","v":0}]
[null,null,null,null,"Sws2",{"$f":"_xlfn.IFNA(IF(OR(F23='drop down content & text'!L2,F23='drop down content & text'!L6),F34,VLOOKUP(F22,Results_all,IF(OR(F23='drop down content & text'!L3,F23='drop down content & text'!L7),\"33\",IF(OR(F23='drop down content & text'!L4,F23='drop down content & text'!L8),\"41\",IF(OR(F23='drop down content & text'!L5,F23='drop down content & text'!L9),\"37\",))),FALSE)),'drop down content & text'!S2)","v":7.0000000000000007E-2}]
[null,null,null,null,"Sws3",{"$f":"_xlfn.IFNA(IF(OR(F23='drop down content & text'!L2,F23='drop down content & text'!L6),F35,VLOOKUP(F22,Results_all,IF(OR(F23='drop down content & text'!L3,F23='drop down content & text'!L7),\"34\",IF(OR(F23='drop down content & text'!L4,F23='drop down content & text'!L8),\"42\",IF(OR(F23='drop down content & text'!L5,F23='drop down content & text'!L9),\"38\",))),FALSE)),'drop down content & text'!S2)","v":0}]
[null,null,null,null,"Sws (Sws1+Sws2+Sws3)",{"$f":"_xlfn.IFNA(IF(OR(F23='drop down content & text'!L2,F23='drop down content & text'!L6,F23='drop down content & text'!L7,F23='drop down content & text'!L8,F23='drop down content & text'!L9),SUM(F40:F42),VLOOKUP(F22,Results_all,IF(F23='drop down content & text'!L3,\"35\",IF(F23='drop down content & text'!L4,\"43\",IF(F23='drop down content & text'!L5,\"39\",))),FALSE)),'drop down content & text'!S2)","v":7.0000000000000007E-2}]
[null,null,null,null,"TLws",{"$f":"_xlfn.IFNA(IF(OR(F23='drop down content & text'!L2,F23='drop down content & text'!L6),F36,VLOOKUP(F22,Results_all,IF(OR(F23='drop down content & text'!L3,F23='drop down content & text'!L7),\"46\",IF(OR(F23='drop down content & text'!L4,F23='drop down content & text'!L8),\"50\",IF(OR(F23='drop down content & text'!L5,F23='drop down content & text'!L9),\"48\",))),FALSE)),'drop down content & text'!S2)","v":0}]
[null,null,null,null,"TLws diff",{"$f":"_xlfn.IFNA(IF(OR(F23='drop down content & text'!L2,F23='drop down content & text'!L6),F37,VLOOKUP(F22,Results_all,IF(OR(F23='drop down content & text'!L3,F23='drop down content & text'!L7),\"47\",IF(OR(F23='drop down content & text'!L4,F23='drop down content & text'!L8),\"51\",IF(OR(F23='drop down content & text'!L5,F23='drop down content & text'!L9),\"49\",))),FALSE)),'drop down content & text'!S2)","v":0}]
[null,"FDES",null,null,"Fenêtre",{"$f":"_xlfn.IFNA(VLOOKUP(F22,Results_all,52,FALSE)&IF(NOT(OR(F13=\"Fixe\",F13=\"Manuelle\")),\" (fenêtre)\n\"&'FDES (EPD)'!C10,\" \"),'drop down content & text'!S2)","v":"https://base-inies.fr/consultation/infos-produit/42364 "}]
[null,null,null,null,"Protections solaires",{"$f":"_xlfn.IFNA(VLOOKUP(F23,Assessories_FDES,2,FALSE),'drop down content & text'!S2)","v":"N.A"}]
[null,"Dimensions",null,null,"Largeur hors tout de la baie (m)",{"$f":"_xlfn.IFNA(VLOOKUP(F22,Results_all,54,FALSE),'drop down content & text'!S2)","v":1.88}]
[null,null,null,null,"Hauteur hors tout de la baie (m)",{"$f":"_xlfn.IFNA(VLOOKUP(F22,Results_all,55,FALSE),'drop down content & text'!S2)","v":1.4}]
[null,null,null,null,"Surface hors tout de la baie (m²)",{"$f":"_xlfn.IFNA(VLOOKUP(F22,Results_all,56,FALSE),'drop down content & text'!S2)","v":2.63}]
[null,null,null,null,"Largeur du vitrage (m)",{"$f":"_xlfn.IFNA(VLOOKUP(F22,Results_all,57,FALSE),'drop down content & text'!S2)","v":1.444}]
[null,null,null,null,"Hauteur du vitrage (m)",{"$f":"_xlfn.IFNA(VLOOKUP(F22,Results_all,58,FALSE),'drop down content & text'!S2)","v":1.2}]
[null,null,null,null,"Périmètre du vitrage (m)",{"$f":"_xlfn.IFNA(VLOOKUP(F22,Results_all,59,FALSE),'drop down content & text'!S2)","v":10.11}]
[null,null,null,null,"Surface du vitrage (m²)",{"$f":"_xlfn.IFNA(VLOOKUP(F22,Results_all,60,FALSE),'drop down content & text'!S2)","v":1.74}]
[null,null,null,null,"Surface de cadre (m²)",{"$f":"_xlfn.IFNA(VLOOKUP(F22,Results_all,61,FALSE),'drop down content & text'!S2)","v":0.8899999999999999}]
[null,null,null,null,"RCL",{"$f":"_xlfn.IFNA(VLOOKUP(F22,Results_all,62,FALSE),'drop down content & text'!S2)","v":0.66}]

{"sheet":"drop down content & text","index":1,"n_rows":28,"n_cols":19,"rows_kept":28,"cut":false,"hidden":true,"merged":[[14,12,14,13],[14,14,14,15],[14,16,14,17],[14,18,14,19],[14,20,14,21]]}
["Product type alias","Product type","Size alias","Size","Glazing alias","Glazing","Operation 1","Operation 2","Installation alias","Installation","Assessories alias","Assesories","Zone climatique et altitude","Exposition au bruit et usage de la pièce","Pente et orientation",null,"Exipration warning EN","Exipration warning FR","Error text"]
["GGL (Rotation, Bois)","GGL","CK01 (0.550m x 0.698m)","CK01","Standard (54F)","54F","Manuelle","Ouverture manuelle","Standard","Standard","Aucun","None","H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m","Exposition BR1 - locaux destinés au sommeil","Pente < 60°",null,"WARNING: Data expired","AVERTISSEMENT : Données expirées","La combinaison de produits choisie n'est pas vendue en France ou n'est pas intégrée au calculateur"]
["GGU (Rotation, Polyurethane)","GGU","CK02 (0.550m x 0.778m)","CK02","Tout confort (57)","57","Motorisée","Ouverture manuelle","Standard + bloc isolant BDX","Standard + BDX","Store pare-soleil extérieur (MHL, MSL, MML, MSLS, MAG, MSI, MIE,MAD)","Awning","H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m","Exposition BR2 ou BR3 - locaux destinés au sommeil","Pente>60° orientation autre que Nord",null,"Please refresh the data","Veuillez actualiser les données"]
["GIL (verrière d'angle, bois)","GIL","CK04 (0.550m x 0.978m)","CK04","Triple vitrage acoustique (62)",62,"Motorisée et automatisée avec VELUX Active ou Somfy Tahoma","Gestion automatique en fonction de la température intérieure","Encastrée","Flush","Volet roulant souple (SSS, SSSS)","Softshutter","H2d ou H3 altitude <= 400 m","Exposition BR1 - hors locaux destinés au sommeil","Pente>60° orientation Nord",null,"WARNING: Data will expire on","AVERTISSEMENT : Les données expireront le"]
["GIU (verrière d'angle, polyurethane)","GIU","FFKF06 (1.880m x 1.178m)","FFKF06","Triple vitrage (66)","66","Fixe","Non ouvrable","Encastrée + bloc isolant BDX","Flush + BDX","Volet roulant (SML, SSL, SSLS, SMG)","Shutter",null,"Exposition BR2 ou BR3 - hors locaux destinés au sommeil",null,null,"Please prepare to refresh","Veuillez vous préparer à actualiser"]
["GPL (Projection, bois)","GPL","FFKF08 (1.880m x 1.398m)","FFKF08","Isolant (70)","70",null,null,null,null,"Store intérieur (DKL)","DKL"]
["GPU (Projection, bois)","GPU","MK04 (0.780m x 0.978m)","MK04","Isolant (70Q)","70Q","A operation 1","A operation 2",null,null,"Store intérieur + Store pare-soleil extérieur","Awning + DKL"]
["GFL (Fenêtre essentielle à rotation, bois)","GFL","MK06 (0.780m x 1.178m)","MK06","Confort (76F)","76F","Aucun","-",null,null,"Store intérieur + Volet roulant souple","Softshutter + DKL"]
["VFE (verrière d'angle, bois)","VFE","MK08 (0.780m x 1.398m )","MK08",null,null,"Manuelle ou motorisée sans automatisation","Ouverture manuelle",null,null,"Store intérieur + Volet roulant","Shutter + DKL"]
["VIU (verrière d'angle, polyurethane)","VIU","MK31 (0.780m x 0.601m )","MK31",null,null,"Motorisée et automatisée avec VELUX Active ou Somfy Tahoma","Gestion crépusculaire sans détecteur de présence"]
["GGLS (3-en-1, rotation)","GGLS","MK34 (0.780m x 0.920m)","MK34"]
["GPLS (3-en-1, projection)","GPLS","MK35 (0.780m x 0.955m)","MK35"]
[null,null,"PK06 (0.942m x 1.178m)","PK06"]
[null,null,"PK08 (0.942m x 1.398m)","PK08"]
[null,null,"PK10 (0.942m x 1.600m)","PK10"]
[null,null,"PK31 (0.942m x 0.601m)","PK31"]
[null,null,"PK34 (0.942m x 0.920m)","PK34"]
[null,null,"PK35 (0.942m x 0.955m)","PK35"]
[null,null,"SK06 (1.140m x 1.178m)","SK06"]
[null,null,"SK08 (1.140m x 1.398m)","SK08"]
[null,null,"SK31 (1.140m x 0.601m)","SK31"]
[null,null,"SK34 (1.140m x 0.920m)","SK34"]
[null,null,"SK35 (1.140m x 0.955m )","SK35"]
[null,null,"UK04 (1.340m x 0.978m)","UK04"]
[null,null,"UK08 (1.340m x 1.398m)","UK08"]
[null,null,"UK31 (1.340m x 0.601m)","UK31"]
[null,null,"UK34 (1.340m x 0.920m)","UK34"]
[null,null,"UK35 (1.340m x 0.955m)","UK35"]

{"sheet":"FDES (EPD)","index":2,"n_rows":155,"n_cols":4,"rows_kept":155,"cut":false,"hidden":true,"merged":[]}
[]
[null,"NB: EPDs for windows are manually maps to the tab \"Product list (sale) w values\""]
[]
[]
[null,"Links to EPDs, used in the calculator (via references)"]
[null,"GGU","https://base-inies.fr/consultation/infos-produit/42366 ","link to our EPD in INIES"]
[null,"GPL","https://base-inies.fr/consultation/infos-produit/42365  ","link to our EPD in INIES"]
[null,"GPU","https://base-inies.fr/consultation/infos-produit/42367 ","link to our EPD in INIES"]
[null,"GGL, GFL, GGLS","https://base-inies.fr/consultation/infos-produit/42364","link to our EPD in INIES"]
[null,"Window operator","https://base-inies.fr/consultation/infos-produit/31433 (moteur)","link to industry EPD"]
[null,"Assessories_FDES"]
[null,"None","-"]
[null,"Awning","https://base-inies.fr/consultation/infos-produit/27007","link to industry EPD"]
[null,"Softshutter","N.A"]
[null,"Shutter","N.A"]
[null,"DKL","https://base-inies.fr/consultation/infos-produit/26740","link to industry EPD"]
[null,"Awning + DKL","1) Store intérieur: https://base-inies.fr/consultation/infos-produit/2674\n2) Store pare-soleil extérieur: https://base-inies.fr/consultation/infos-produit/27007"]
[null,"Softshutter + DKL","1) Store intérieur: https://base-inies.fr/consultation/infos-produit/2674\n2) Volet roulant: N.A"]
[null,"Shutter + DKL","1) Store intérieur: https://base-inies.fr/consultation/infos-produit/2674\n2) Volet roulant: N.A"]
[null,"No results","Pas de FDES en ligne pour la solution choisie"]
[]
[]
[]
[]
[]
[]
[]
[null,"Zobber, zink versions excluded"]
[]
[]
[]
[null,"GPL CK04 57","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GPL MK04 57","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GPL MK06 57","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GPL MK08 57","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GPL PK06 57","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GPL PK08 57","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GPL PK10 57","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GPL SK06 57","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GPL SK08 57","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GPL UK04 57","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GPL UK08 57","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GPL CK04 76F","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GPL MK04 76F","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GPL MK06 76F","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GPL MK08 76F","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GPL PK06 76F","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GPL PK08 76F","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GPL PK10 76F","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GPL SK06 76F","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GPL SK08 76F","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GPL UK04 76F","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GPL UK08 76F","https://base-inies.fr/consultation/infos-produit/42365  "]
[null,"GGL CK01 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL CK02 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL CK04 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL MK04 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL MK06 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL MK08 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL PK06 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL PK08 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL PK10 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL SK06 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL SK08 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL UK04 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL UK08 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL CK01 57","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL CK02 57","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL CK04 57","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL MK04 57","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL MK06 57","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL MK08 57","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL PK06 57","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL PK08 57","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL PK10 57","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL SK06 57","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL SK08 57","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL UK04 57","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL UK08 57","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL CK01 76F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL CK02 76F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL CK04 76F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL MK04 76F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL MK06 76F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL MK08 76F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL PK06 76F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL PK08 76F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL PK10 76F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL SK06 76F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL SK08 76F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL UK04 76F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGL UK08 76F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GFL CK01 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GFL CK02 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GFL CK04 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GFL MK04 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GFL MK06 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GFL MK08 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GFL PK06 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GFL PK08 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GFL PK10 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GFL SK06 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GFL SK08 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GFL UK04 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GFL UK08 54F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGLS FFKF08 57","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGLS FFKF06 57","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGLS FFKF08 76F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGLS FFKF06 76F","https://base-inies.fr/consultation/infos-produit/42364"]
[null,"GGU CK02 57","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU CK04 57","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU MK04 57","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU MK06 57","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU MK08 57","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU PK06 57","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU PK08 57","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU PK10 57","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU SK06 57","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU SK08 57","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU UK04 57","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU UK08 57","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU CK02 76F","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU CK04 76F","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU MK04 76F","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU MK06 76F","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU MK08 76F","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU PK06 76F","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU PK08 76F","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU PK10 76F","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU SK06 76F","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU SK08 76F","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU UK04 76F","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GGU UK08 76F","https://base-inies.fr/consultation/infos-produit/42366 "]
[null,"GPU CK04 57","https://base-inies.fr/consultation/infos-produit/42367 "]
[null,"GPU MK04 57","https://base-inies.fr/consultation/infos-produit/42367 "]
[null,"GPU MK06 57","https://base-inies.fr/consultation/infos-produit/42367 "]
[null,"GPU MK08 57","https://base-inies.fr/consultation/infos-produit/42367 "]
[null,"GPU PK06 57","https://base-inies.fr/consultation/infos-produit/42367 "]
[null,"GPU PK08 57","https://base-inies.fr/consultation/infos-produit/42367 "]
[null,"GPU PK10 57","https://base-inies.fr/consultation/infos-produit/42367 "]
[null,"GPU SK06 57","https://base-inies.fr/consultation/infos-produit/42367 "]
[null,"GPU SK08 57","https://base-inies.fr/consultation/infos-produit/42367 "]
[null,"GPU UK04 57","https://base-inies.fr/consultation/infos-produit/42367 "]
[null,"GPU UK08 57","https://base-inies.fr/consultation/infos-produit/42367 "]
[null,"GPU CK04 76F","https://base-inies.fr/consultation/infos-produit/42367 "]
[null,"GPU MK04 76F","https://base-inies.fr/consultation/infos-produit/42367 "]
[null,"GPU MK06 76F","https://base-inies.fr/consultation/infos-produit/42367 "]
[null,"GPU MK08 76F","https://base-inies.fr/consultation/infos-produit/42367 "]
[null,"GPU PK06 76F","https://base-inies.fr/consultation/infos-produit/42367 "]
[null,"GPU PK08 76F","https://base-inies.fr/consultation/infos-produit/42367 "]
[null,"GPU PK10 76F","https://base-inies.fr/consultation/infos-produit/42367 "]
[null,"GPU SK06 76F","https://base-inies.fr/consultation/infos-produit/42367 "]
[null,"GPU SK08 76F","https://base-inies.fr/consultation/infos-produit/42367 "]
[null,"GPU UK04 76F","https://base-inies.fr/consultation/infos-produit/42367 "]
[null,"GPU UK08 76F","https://base-inies.fr/consultation/infos-produit/42367 "]

{"sheet":"results ready","index":3,"n_rows":2507,"n_cols":62,"rows_kept":1125,"cut":true,"hidden":true,"merged":[[3782,13,3782,14],[3782,15,3782,16],[3782,17,3782,18],[3782,19,3782,20],[3782,21,3782,22],[3782,25,3782,30],[3782,35,3782,38],[3782,39,3782,42],[3782,31,3782,34],[3782,23,3782,24]],"bounds":{"rows_first":500,"rows_last":125,"rows_between":500,"halvings":2}}
[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,42,43,44,45,46,47,48,49,50,51,52,53,54,55,56,57,58,59,60,61,62]
["Product defintion_lookup features",null,null,null,null,null,null,null,null,null,null,null,null,"Window",null,"Window + awning",null,"Window + shutter",null,"Window + DKL",null,"Window + awning + DKL",null,"Window + shutter + DKL",null,"Window",null,null,null,null,null,"Awning",null,null,null,"Shutter",null,null,null,"Soft shutter",null,null,null,"Window",null,"Awning",null,"Shutter",null,"Soft shutter",null,"FDES",null,"Geometry"]
["Product lookup","Extra colum (don't delete)","Variant","Size","PaneVariantCode","Operation","Installation","ID","Product mother","Status","Product mother variant","Glazing mother Uw","Glazing mother Sw etc","Uw (90°)","Uw (0°)","Uws (90°)","Uws(0°)","Uw (90°)","Uw (0°)","Uws (90°)","Uws(0°)","Uw (90°)","Uw (0°)","Uws (90°)","Uws(0°)","Swc1","Swc2","Swc3","Swe1","Swe2","Swe3","Sws1","Sws2","Sws3","Sws (Sws1+Sws2+Sws3)","Sws1","Sws2","Sws3","Sws (Sws1+Sws2+Sws3)","Sws1","Sws2","Sws3","Sws (Sws1+Sws2+Sws3)","TLw","TLw diff","Tlws","Tlws diff","Tlws","Tlws diff","Tlws","Tlws diff","FDES window","TestID","Lw","Lh","Aw","Lg,w","Lg,h","Lg","Ag","Af","RCL"]
["GFL CK02 54F Standard","GFL","CK02","54F","MANUAL","Standard","GFL 54F","GFL 54F","ok","GFL","54F","GFL CK02 54F Standard","54F",1.6,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.27,0.05,0,0.27,0.05,0,0.05,0.1,0,0.15,0,0.08,0,0.08,0,0.09,0,0.09,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",933,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GFL CK04 54F Standard","GFL","CK04","54F","MANUAL","Standard","GFL 54F","GFL 54F","ok","GFL","54F","GFL CK04 54F Standard","54F",1.6,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.28999999999999998,0.05,0,0.28999999999999998,0.05,0,0.05,0.1,0,0.15,0,0.08,0,0.08,0,0.09,0,0.09,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",934,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GFL MK04 54F Standard","GFL","MK04","54F","MANUAL","Standard","GFL 54F","GFL 54F","ok","GFL","54F","GFL MK04 54F Standard","54F",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.34,0.05,0,0.34,0.05,0,0.06,0.09,0,0.15,0,0.08,0,0.08,0,0.08,0,0.08,0.49,0,0.09,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",935,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GFL MK06 54F Standard","GFL","MK06","54F","MANUAL","Standard","GFL 54F","GFL 54F","ok","GFL","54F","GFL MK06 54F Standard","54F",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.35,0.05,0,0.35,0.05,0,0.06,0.09,0,0.15,0,0.08,0,0.08,0,0.08,0,0.08,0.52,0,0.09,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",936,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GFL MK08 54F Standard","GFL","MK08","54F","MANUAL","Standard","GFL 54F","GFL 54F","ok","GFL","54F","GFL MK08 54F Standard","54F",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.36,0.05,0,0.36,0.05,0,7.0000000000000007E-2,0.09,0,0.15,0,0.08,0,0.08,0,0.08,0,0.08,0.53,0,0.09,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",937,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GFL SK06 54F Standard","GFL","SK06","54F","MANUAL","Standard","GFL 54F","GFL 54F","ok","GFL","54F","GFL SK06 54F Standard","54F",1.4,1.8,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.39,0.05,0,0.39,0.05,0,7.0000000000000007E-2,0.08,0,0.15,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.56999999999999995,0,0.1,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",938,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GFL SK08 54F Standard","GFL","SK08","54F","MANUAL","Standard","GFL 54F","GFL 54F","ok","GFL","54F","GFL SK08 54F Standard","54F",1.4,1.8,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.4,0.05,0,0.4,0.05,0,7.0000000000000007E-2,0.08,0,0.15,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.59,0,0.1,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",939,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GFL UK04 54F Standard","GFL","UK04","54F","MANUAL","Standard","GFL 54F","GFL 54F","ok","GFL","54F","GFL UK04 54F Standard","54F",1.4,1.8,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.38,0.05,0,0.38,0.05,0,7.0000000000000007E-2,0.08,0,0.15,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.56000000000000005,0,0.1,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",940,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GFL UK08 54F Standard","GFL","UK08","54F","MANUAL","Standard","GFL 54F","GFL 54F","ok","GFL","54F","GFL UK08 54F Standard","54F",1.4,1.8,1.3,1.6,1.2,1.5,1.1000000000000001,1.4,1.6,1.3,1,1.2,0.41,0.05,0,0.41,0.05,0,7.0000000000000007E-2,0.08,0,0.15,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.6,0,0.1,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",941,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGL CK01 57 Standard","GGL","CK01",57,"MANUAL","Standard","GGL 57","GPL 70","ok","GPL","70","GPL CK01 70 Standard",57,1.6,1.9,1.5,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.1,0.05,0,0.1,0.06,0,0.02,0.1,0,0.12,0,0.08,0,0.08,0,0.08,0,0.08,0.3,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",942,0.55000000000000004,0.7,0.38,0.37000000000000005,0.5,1.75,0.18,0.2,0.47]
["GGL CK01 66 Standard","GGL","CK01","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL CK01 66 Standard","66",1.4,1.6,1.3,1.4,1.2,1.3,1.2,1.3,1.4,1.2,1,1.1000000000000001,0.15,0.08,0,0.15,0.08,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.3,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",943,0.55000000000000004,0.7,0.38,0.37000000000000005,0.5,1.75,0.18,0.2,0.47]
["GGL CK01 76F Standard","GGL","CK01","76F","MANUAL","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL CK01 70 Standard","76",1.6,1.9,1.5,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.1,0.05,0,0.1,0.05,0,0.02,0.1,0,0.12,0,0.08,0,0.08,0,0.08,0,0.08,0.3,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",944,0.55000000000000004,0.7,0.38,0.37000000000000005,0.5,1.75,0.18,0.2,0.47]
["GGL CK02 54F Standard","GGL","CK02","54F","MANUAL","Standard","GGL 54F","GPL 54F","ok","GPL","54F","GPL CK02 54F Standard","54F",1.7,2,1.5,1.8,1.4,1.6,1.3,1.5,1.8,1.4,1.1000000000000001,1.3,0.28000000000000003,0.05,0,0.28000000000000003,0.05,0,0.05,0.1,0,0.15,0,0.08,0,0.08,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",946,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGL CK02 57 Standard","GGL","CK02",57,"ELECTRIC","Standard","GGL 57","GPL 70","ok","GPL","70","GPL CK02 70 Standard",57,1.6,1.9,1.5,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.06,0,0.02,0.1,0,0.12,0,0.08,0,0.08,0,0.08,0,0.08,0.31,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",947,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGL CK02 57 Standard","GGL","CK02",57,"MANUAL","Standard","GGL 57","GPL 70","ok","GPL","70","GPL CK02 70 Standard",57,1.6,1.9,1.5,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.06,0,0.02,0.1,0,0.12,0,0.08,0,0.08,0,0.08,0,0.08,0.31,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",948,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGL CK02 62 Standard","GGL","CK02","62","MANUAL","Standard","GGL 62","GPL 62","ok","GPL","62","GPL CK02 62 Standard","62",1.4,1.5,1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.99,1.1000000000000001,0.19,7.0000000000000007E-2,0,0.19,0.08,0,0.03,0.09,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",949,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGL CK02 62 Standard","GGL","CK02","62","ELECTRIC","Standard","GGL 62","GPL 62","ok","GPL","62","GPL CK02 62 Standard","62",1.4,1.5,1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.99,1.1000000000000001,0.19,7.0000000000000007E-2,0,0.19,0.08,0,0.03,0.09,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",950,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGL CK02 66 Standard","GGL","CK02","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL CK02 66 Standard","66",1.4,1.5,1.3,1.4,1.2,1.3,1.1000000000000001,1.3,1.4,1.2,1,1.1000000000000001,0.15,0.08,0,0.15,0.08,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.31,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",951,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGL CK02 66 Standard","GGL","CK02","66","ELECTRIC","Standard","GGL 66","GPL 66","ok","GPL","66","GPL CK02 66 Standard","66",1.4,1.5,1.3,1.4,1.2,1.3,1.1000000000000001,1.3,1.4,1.2,1,1.1000000000000001,0.15,0.08,0,0.15,0.08,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.31,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",945,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGL CK02 66 Standard","GGL","CK02","66","SOLAR","Standard","GGL 66","GPL 66","ok","GPL","66","GPL CK02 66 Standard","66",1.4,1.5,1.3,1.4,1.2,1.3,1.1000000000000001,1.3,1.4,1.2,1,1.1000000000000001,0.15,0.08,0,0.15,0.08,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.31,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",952,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGL CK02 70 Standard","GGL","CK02","70","MANUAL","Standard","GGL 70","GPL 70","ok","GPL","70","GPL CK02 70 Standard","70",1.6,1.9,1.5,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.19,0.06,0,0.19,0.06,0,0.04,0.1,0,0.14000000000000001,0,0.08,0,0.08,0,0.08,0,0.08,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",957,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGL CK02 70 Standard","GGL","CK02","70","MANUALBOTTOM","Standard","GGL 70","GPL 70","ok","GPL","70","GPL CK02 70 Standard","70",1.6,1.9,1.5,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.19,0.06,0,0.19,0.06,0,0.04,0.1,0,0.14000000000000001,0,0.08,0,0.08,0,0.08,0,0.08,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",958,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGL CK02 70Q Standard","GGL","CK02","70Q","MANUAL","Standard","GGL 70Q","GPL 70","ok","GPL","70","GPL CK02 70 Standard",70,1.6,1.9,1.5,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.19,0.06,0,0.19,0.06,0,0.04,0.1,0,0.14000000000000001,0,0.08,0,0.08,0,0.08,0,0.08,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",959,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGL CK02 76F Standard","GGL","CK02","76F","ELECTRIC","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL CK02 70 Standard","76",1.6,1.9,1.5,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.05,0,0.02,0.1,0,0.12,0,0.08,0,0.08,0,0.08,0,0.08,0.31,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",954,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGL CK02 76F Standard","GGL","CK02","76F","MANUAL","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL CK02 70 Standard","76",1.6,1.9,1.5,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.05,0,0.02,0.1,0,0.12,0,0.08,0,0.08,0,0.08,0,0.08,0.31,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",962,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGL CK02 76F Standard","GGL","CK02","76F","SOLAR","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL CK02 70 Standard","76",1.6,1.9,1.5,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.05,0,0.02,0.1,0,0.12,0,0.08,0,0.08,0,0.08,0,0.08,0.31,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",960,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGL CK04 54F Standard","GGL","CK04","54F","MANUAL","Standard","GGL 54F","GPL 54F","ok","GPL","54F","GPL CK04 54F Standard","54F",1.6,2,1.5,1.8,1.4,1.6,1.3,1.5,1.8,1.4,1.1000000000000001,1.3,0.3,0.05,0,0.3,0.05,0,0.05,0.1,0,0.15,0,0.08,0,0.08,0,0.08,0,0.08,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",963,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGL CK04 57 Standard","GGL","CK04",57,"ELECTRIC","Standard","GGL 57","GPL 70","ok","GPL","70","GPL CK04 70 Standard",57,1.6,1.9,1.4,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.06,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.33,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",964,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGL CK04 57 Standard","GGL","CK04",57,"MANUAL","Standard","GGL 57","GPL 70","ok","GPL","70","GPL CK04 70 Standard",57,1.6,1.9,1.4,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.06,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.33,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",965,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGL CK04 62 Standard","GGL","CK04","62","MANUAL","Standard","GGL 62","GPL 62","ok","GPL","62","GPL CK04 62 Standard","62",1.3,1.5,1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.97,1.1000000000000001,0.2,0.08,0,0.2,0.08,0,0.03,0.09,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",966,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGL CK04 62 Standard","GGL","CK04","62","ELECTRIC","Standard","GGL 62","GPL 62","ok","GPL","62","GPL CK04 62 Standard","62",1.3,1.5,1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.97,1.1000000000000001,0.2,0.08,0,0.2,0.08,0,0.03,0.09,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",967,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGL CK04 66 Standard","GGL","CK04","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL CK04 66 Standard","66",1.3,1.5,1.2,1.4,1.2,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.99,1.1000000000000001,0.16,0.08,0,0.16,0.08,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",968,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGL CK04 66 Standard","GGL","CK04","66","ELECTRIC","Standard","GGL 66","GPL 66","ok","GPL","66","GPL CK04 66 Standard","66",1.3,1.5,1.2,1.4,1.2,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.99,1.1000000000000001,0.16,0.08,0,0.16,0.08,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",969,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGL CK04 66 Standard","GGL","CK04","66","SOLAR","Standard","GGL 66","GPL 66","ok","GPL","66","GPL CK04 66 Standard","66",1.3,1.5,1.2,1.4,1.2,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.99,1.1000000000000001,0.16,0.08,0,0.16,0.08,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",970,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGL CK04 70 Standard","GGL","CK04","70","MANUAL","Standard","GGL 70","GPL 70","ok","GPL","70","GPL CK04 70 Standard","70",1.6,1.9,1.4,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.21,0.06,0,0.21,0.06,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",973,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGL CK04 70Q Standard","GGL","CK04","70Q","MANUAL","Standard","GGL 70Q","GPL 70","ok","GPL","70","GPL CK04 70 Standard",70,1.6,1.9,1.4,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.21,0.06,0,0.21,0.06,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",974,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGL CK04 76F Standard","GGL","CK04","76F","MANUAL","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL CK04 70 Standard","76",1.6,1.9,1.4,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.05,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.34,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",977,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGL CK04 76F Standard","GGL","CK04","76F","SOLAR","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL CK04 70 Standard","76",1.6,1.9,1.4,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.05,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.34,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",975,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGL CK04 70H Standard","GGL","CK04","70H","MANUAL","Standard","GGL 70H","GPL 70","ok","GPL","70","GPL CK04 70 Standard",70,1.6,1.9,1.4,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.21,0.06,0,0.21,0.06,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",976,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGL CK06 62 Standard","GGL","CK06","62","MANUAL","Standard","GGL 62","GPL 62","ok","GPL","62","GPL CK06 62 Standard","62",1.3,1.5,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.96,1,0.21,0.08,0,0.21,0.08,0,0.04,0.09,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",979,0.55000000000000004,1.18,0.65,0.37000000000000005,0.98,2.71,0.37,0.28000000000000003,0.56999999999999995]
["GGL CK06 62 Standard","GGL","CK06","62","ELECTRIC","Standard","GGL 62","GPL 62","ok","GPL","62","GPL CK06 62 Standard","62",1.3,1.5,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.96,1,0.21,0.08,0,0.21,0.08,0,0.04,0.09,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",980,0.55000000000000004,1.18,0.65,0.37000000000000005,0.98,2.71,0.37,0.28000000000000003,0.56999999999999995]
["GGL CK06 66 Standard","GGL","CK06","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL CK06 66 Standard","66",1.3,1.5,1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.97,1.1000000000000001,0.17,0.08,0,0.17,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",982,0.55000000000000004,1.18,0.65,0.37000000000000005,0.98,2.71,0.37,0.28000000000000003,0.56999999999999995]
["GGL CK06 66 Standard","GGL","CK06","66","ELECTRIC","Standard","GGL 66","GPL 66","ok","GPL","66","GPL CK06 66 Standard","66",1.3,1.5,1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.97,1.1000000000000001,0.17,0.08,0,0.17,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",983,0.55000000000000004,1.18,0.65,0.37000000000000005,0.98,2.71,0.37,0.28000000000000003,0.56999999999999995]
["GGL CK06 66 Standard","GGL","CK06","66","SOLAR","Standard","GGL 66","GPL 66","ok","GPL","66","GPL CK06 66 Standard","66",1.3,1.5,1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.97,1.1000000000000001,0.17,0.08,0,0.17,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",984,0.55000000000000004,1.18,0.65,0.37000000000000005,0.98,2.71,0.37,0.28000000000000003,0.56999999999999995]
["GGL CK06 70 Standard","GGL","CK06","70","SOLAR","Standard","GGL 70","GPL 70","ok","GPL","70","GPL CK06 70 Standard","70",1.5,1.9,1.4,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.21,0.06,0,0.21,0.06,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",987,0.55000000000000004,1.18,0.65,0.37000000000000005,0.98,2.71,0.37,0.28000000000000003,0.56999999999999995]
["GGL CK06 70H Standard","GGL","CK06","70H","MANUAL","Standard","GGL 70H","GPL 70","ok","GPL","70","GPL CK06 70 Standard",70,1.5,1.9,1.4,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.21,0.06,0,0.21,0.06,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",981,0.55000000000000004,1.18,0.65,0.37000000000000005,0.98,2.71,0.37,0.28000000000000003,0.56999999999999995]
["GGL FK04 62 Standard","GGL","FK04","62","MANUAL","Standard","GGL 62","GPL 62","ok","GPL","62","GPL FK04 62 Standard","62",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.93,1,0.22,0.08,0,0.22,0.08,0,0.04,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",988,0.66,0.98,0.65,0.48000000000000004,0.78,2.5299999999999998,0.38,0.27,0.57999999999999996]
["GGL FK04 62 Standard","GGL","FK04","62","ELECTRIC","Standard","GGL 62","GPL 62","ok","GPL","62","GPL FK04 62 Standard","62",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.93,1,0.22,0.08,0,0.22,0.08,0,0.04,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",989,0.66,0.98,0.65,0.48000000000000004,0.78,2.5299999999999998,0.38,0.27,0.57999999999999996]
["GGL FK04 66 Standard","GGL","FK04","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL FK04 66 Standard","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.95,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",991,0.66,0.98,0.65,0.48000000000000004,0.78,2.5299999999999998,0.38,0.27,0.57999999999999996]
["GGL FK04 66 Standard","GGL","FK04","66","ELECTRIC","Standard","GGL 66","GPL 66","ok","GPL","66","GPL FK04 66 Standard","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.95,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",992,0.66,0.98,0.65,0.48000000000000004,0.78,2.5299999999999998,0.38,0.27,0.57999999999999996]
["GGL FK04 70Q Standard","GGL","FK04","70Q","MANUAL","Standard","GGL 70Q","GPL 70","ok","GPL","70","GPL FK04 70 Standard",70,1.5,1.9,1.4,1.7,1.3,1.6,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.22,0.06,0,0.22,0.06,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",994,0.66,0.98,0.65,0.48000000000000004,0.78,2.5299999999999998,0.38,0.27,0.57999999999999996]
["GGL FK06 62 Standard","GGL","FK06","62","MANUAL","Standard","GGL 62","GPL 62","ok","GPL","62","GPL FK06 62 Standard","62",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.91,1,0.23,0.08,0,0.23,0.08,0,0.04,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",995,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GGL FK06 62 Standard","GGL","FK06","62","ELECTRIC","Standard","GGL 62","GPL 62","ok","GPL","62","GPL FK06 62 Standard","62",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.91,1,0.23,0.08,0,0.23,0.08,0,0.04,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",996,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GGL FK06 66 Standard","GGL","FK06","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL FK06 66 Standard","66",1.2,1.4,1.2,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.93,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",990,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GGL FK06 66 Standard","GGL","FK06","66","ELECTRIC","Standard","GGL 66","GPL 66","ok","GPL","66","GPL FK06 66 Standard","66",1.2,1.4,1.2,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.93,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",999,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GGL FK06 66 Standard","GGL","FK06","66","SOLAR","Standard","GGL 66","GPL 66","ok","GPL","66","GPL FK06 66 Standard","66",1.2,1.4,1.2,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.93,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",997,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GGL FK06 70Q Standard","GGL","FK06","70Q","MANUAL","Standard","GGL 70Q","GPL 70","ok","GPL","70","GPL FK06 70 Standard",70,1.5,1.9,1.4,1.7,1.3,1.6,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.23,0.06,0,0.23,0.06,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1002,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GGL FK06 76F Standard","GGL","FK06","76F","MANUAL","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL FK06 70 Standard","76",1.5,1.9,1.4,1.7,1.3,1.6,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.13,0.05,0,0.13,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1003,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GGL FK06 70H Standard","GGL","FK06","70H","MANUAL","Standard","GGL 70H","GPL 70","ok","GPL","70","GPL FK06 70 Standard",70,1.5,1.9,1.4,1.7,1.3,1.6,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.23,0.06,0,0.23,0.06,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1004,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GGL FK08 62 Standard","GGL","FK08","62","MANUAL","Standard","GGL 62","GPL 62","ok","GPL","62","GPL FK08 62 Standard","62",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.89,0.99,0.23,0.08,0,0.23,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1005,0.66,1.4,0.92,0.48000000000000004,1.2,3.37,0.57999999999999996,0.34000000000000008,0.63]
["GGL FK08 62 Standard","GGL","FK08","62","ELECTRIC","Standard","GGL 62","GPL 62","ok","GPL","62","GPL FK08 62 Standard","62",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.89,0.99,0.23,0.08,0,0.23,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1006,0.66,1.4,0.92,0.48000000000000004,1.2,3.37,0.57999999999999996,0.34000000000000008,0.63]
["GGL FK08 66 Standard","GGL","FK08","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL FK08 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.92,1,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1000,0.66,1.4,0.92,0.48000000000000004,1.2,3.37,0.57999999999999996,0.34000000000000008,0.63]
["GGL FK08 66 Standard","GGL","FK08","66","ELECTRIC","Standard","GGL 66","GPL 66","ok","GPL","66","GPL FK08 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.92,1,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1009,0.66,1.4,0.92,0.48000000000000004,1.2,3.37,0.57999999999999996,0.34000000000000008,0.63]
["GGL FK08 66 Standard","GGL","FK08","66","SOLAR","Standard","GGL 66","GPL 66","ok","GPL","66","GPL FK08 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.92,1,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1007,0.66,1.4,0.92,0.48000000000000004,1.2,3.37,0.57999999999999996,0.34000000000000008,0.63]
["GGL MK04 54F Standard","GGL","MK04","54F","MANUAL","Standard","GGL 54F","GPL 54F","ok","GPL","54F","GPL MK04 54F Standard","54F",1.5,1.9,1.4,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.37,0.05,0,0.37,0.05,0,7.0000000000000007E-2,0.09,0,0.15,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.5,0,0.09,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1010,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGL MK04 57 Standard","GGL","MK04",57,"ELECTRIC","Standard","GGL 57","GPL 70","ok","GPL","70","GPL MK04 70 Standard",57,1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.13,0.05,0,0.13,0.06,0,0.02,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1011,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGL MK04 57 Standard","GGL","MK04",57,"MANUAL","Standard","GGL 57","GPL 70","ok","GPL","70","GPL MK04 70 Standard",57,1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.13,0.05,0,0.13,0.06,0,0.02,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1012,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGL MK04 62 Standard","GGL","MK04","62","MANUAL","Standard","GGL 62","GPL 62","ok","GPL","62","GPL MK04 62 Standard","62",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.89,0.99,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1015,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGL MK04 62 Standard","GGL","MK04","62","ELECTRIC","Standard","GGL 62","GPL 62","ok","GPL","62","GPL MK04 62 Standard","62",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.89,0.99,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1013,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGL MK04 66 Standard","GGL","MK04","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL MK04 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.92,1,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1014,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGL MK04 66 Standard","GGL","MK04","66","ELECTRIC","Standard","GGL 66","GPL 66","ok","GPL","66","GPL MK04 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.92,1,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1016,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGL MK04 66 Standard","GGL","MK04","66","SOLAR","Standard","GGL 66","GPL 66","ok","GPL","66","GPL MK04 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.92,1,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1017,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGL MK04 70 Standard","GGL","MK04","70","MANUAL","Standard","GGL 70","GPL 70","ok","GPL","70","GPL MK04 70 Standard","70",1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.24,0.06,0,0.24,0.06,0,0.04,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1022,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGL MK04 70 Standard","GGL","MK04","70","MANUALBOTTOM","Standard","GGL 70","GPL 70","ok","GPL","70","GPL MK04 70 Standard","70",1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.24,0.06,0,0.24,0.06,0,0.04,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1023,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGL MK04 70Q Standard","GGL","MK04","70Q","MANUAL","Standard","GGL 70Q","GPL 70","ok","GPL","70","GPL MK04 70 Standard",70,1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.24,0.06,0,0.24,0.06,0,0.04,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1024,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGL MK04 76F Standard","GGL","MK04","76F","ELECTRIC","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL MK04 70 Standard","76",1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1025,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGL MK04 76F Standard","GGL","MK04","76F","MANUAL","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL MK04 70 Standard","76",1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1026,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGL MK04 76F Standard","GGL","MK04","76F","SOLAR","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL MK04 70 Standard","76",1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1027,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGL MK04 57 Standard","GGL","MK04",57,"SOLAR","Standard","GGL 57","GPL 70","ok","GPL","70","GPL MK04 70 Standard",57,1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.13,0.05,0,0.13,0.06,0,0.02,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1028,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGL MK06 54F Standard","GGL","MK06","54F","MANUAL","Standard","GGL 54F","GPL 54F","ok","GPL","54F","GPL MK06 54F Standard","54F",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.38,0.05,0,0.38,0.05,0,7.0000000000000007E-2,0.09,0,0.15,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.52,0,0.09,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1029,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGL MK06 57 Standard","GGL","MK06",57,"ELECTRIC","Standard","GGL 57","GPL 70","ok","GPL","70","GPL MK06 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1030,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGL MK06 57 Standard","GGL","MK06",57,"MANUAL","Standard","GGL 57","GPL 70","ok","GPL","70","GPL MK06 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1031,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGL MK06 62 Standard","GGL","MK06","62","MANUAL","Standard","GGL 62","GPL 62","ok","GPL","62","GPL MK06 62 Standard","62",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.97,1.1000000000000001,1.2,1,0.87,0.98,0.24,0.08,0,0.24,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1032,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGL MK06 62 Standard","GGL","MK06","62","ELECTRIC","Standard","GGL 62","GPL 62","ok","GPL","62","GPL MK06 62 Standard","62",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.97,1.1000000000000001,1.2,1,0.87,0.98,0.24,0.08,0,0.24,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1033,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGL MK06 66 Standard","GGL","MK06","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL MK06 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.9,1,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1034,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGL MK06 66 Standard","GGL","MK06","66","ELECTRIC","Standard","GGL 66","GPL 66","ok","GPL","66","GPL MK06 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.9,1,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1035,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGL MK06 66 Standard","GGL","MK06","66","SOLAR","Standard","GGL 66","GPL 66","ok","GPL","66","GPL MK06 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.9,1,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1036,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGL MK06 70 Standard","GGL","MK06","70","MANUAL","Standard","GGL 70","GPL 70","ok","GPL","70","GPL MK06 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.24,0.06,0,0.24,0.06,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1041,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGL MK06 70 Standard","GGL","MK06","70","MANUALBOTTOM","Standard","GGL 70","GPL 70","ok","GPL","70","GPL MK06 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.24,0.06,0,0.24,0.06,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1042,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGL MK06 70Q Standard","GGL","MK06","70Q","MANUAL","Standard","GGL 70Q","GPL 70","ok","GPL","70","GPL MK06 70 Standard",70,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.24,0.06,0,0.24,0.06,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1043,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGL MK06 76F Standard","GGL","MK06","76F","MANUAL","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL MK06 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1044,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGL MK06 76F Standard","GGL","MK06","76F","SOLAR","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL MK06 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1045,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGL MK06 70H Standard","GGL","MK06","70H","MANUAL","Standard","GGL 70H","GPL 70","ok","GPL","70","GPL MK06 70 Standard",70,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.24,0.06,0,0.24,0.06,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1046,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGL MK06 57 Standard","GGL","MK06",57,"SOLAR","Standard","GGL 57","GPL 70","ok","GPL","70","GPL MK06 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1047,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGL MK08 54F Standard","GGL","MK08","54F","MANUAL","Standard","GGL 54F","GPL 54F","ok","GPL","54F","GPL MK08 54F Standard","54F",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.38,0.05,0,0.38,0.05,0,7.0000000000000007E-2,0.08,0,0.15,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.54,0,0.09,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1048,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGL MK08 57 Standard","GGL","MK08",57,"ELECTRIC","Standard","GGL 57","GPL 70","ok","GPL","70","GPL MK08 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1049,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGL MK08 57 Standard","GGL","MK08",57,"MANUAL","Standard","GGL 57","GPL 70","ok","GPL","70","GPL MK08 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1050,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGL MK08 62 Standard","GGL","MK08","62","MANUAL","Standard","GGL 62","GPL 62","ok","GPL","62","GPL MK08 62 Standard","62",1.1000000000000001,1.3,1,1.2,0.98,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.85,0.96,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1051,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGL MK08 62 Standard","GGL","MK08","62","ELECTRIC","Standard","GGL 62","GPL 62","ok","GPL","62","GPL MK08 62 Standard","62",1.1000000000000001,1.3,1,1.2,0.98,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.85,0.96,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1052,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGL MK08 66 Standard","GGL","MK08","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL MK08 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1,1.2,0.99,1.1000000000000001,1.3,1.1000000000000001,0.88,0.99,0.2,0.09,0,0.2,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1053,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGL MK08 66 Standard","GGL","MK08","66","ELECTRIC","Standard","GGL 66","GPL 66","ok","GPL","66","GPL MK08 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1,1.2,0.99,1.1000000000000001,1.3,1.1000000000000001,0.88,0.99,0.2,0.09,0,0.2,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1054,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGL MK08 66 Standard","GGL","MK08","66","SOLAR","Standard","GGL 66","GPL 66","ok","GPL","66","GPL MK08 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1,1.2,0.99,1.1000000000000001,1.3,1.1000000000000001,0.88,0.99,0.2,0.09,0,0.2,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1055,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGL MK08 70 Standard","GGL","MK08","70","MANUAL","Standard","GGL 70","GPL 70","ok","GPL","70","GPL MK08 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.25,7.0000000000000007E-2,0,0.25,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1061,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGL MK08 70 Standard","GGL","MK08","70","MANUALBOTTOM","Standard","GGL 70","GPL 70","ok","GPL","70","GPL MK08 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.25,7.0000000000000007E-2,0,0.25,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1062,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGL MK08 70Q Standard","GGL","MK08","70Q","MANUAL","Standard","GGL 70Q","GPL 70","ok","GPL","70","GPL MK08 70 Standard",70,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.25,7.0000000000000007E-2,0,0.25,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1063,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGL MK08 76F Standard","GGL","MK08","76F","ELECTRIC","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL MK08 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1064,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGL MK08 76F Standard","GGL","MK08","76F","MANUAL","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL MK08 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1058,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGL MK08 76F Standard","GGL","MK08","76F","SOLAR","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL MK08 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1065,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGL MK08 70H Standard","GGL","MK08","70H","MANUAL","Standard","GGL 70H","GPL 70","ok","GPL","70","GPL MK08 70 Standard",70,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.25,7.0000000000000007E-2,0,0.25,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1066,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGL MK08 57 Standard","GGL","MK08",57,"SOLAR","Standard","GGL 57","GPL 70","ok","GPL","70","GPL MK08 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1068,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGL MK10 62 Standard","GGL","MK10","62","MANUAL","Standard","GGL 62","GPL 62","ok","GPL","62","GPL MK10 62 Standard","62",1.1000000000000001,1.3,1,1.2,0.96,1.1000000000000001,0.94,1.1000000000000001,1.2,1,0.84,0.96,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1069,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GGL MK10 62 Standard","GGL","MK10","62","ELECTRIC","Standard","GGL 62","GPL 62","ok","GPL","62","GPL MK10 62 Standard","62",1.1000000000000001,1.3,1,1.2,0.96,1.1000000000000001,0.94,1.1000000000000001,1.2,1,0.84,0.96,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1070,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GGL MK10 66 Standard","GGL","MK10","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL MK10 66 Standard","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,0.97,1.1000000000000001,1.2,1,0.87,0.98,0.2,0.09,0,0.2,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1071,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GGL MK10 66 Standard","GGL","MK10","66","ELECTRIC","Standard","GGL 66","GPL 66","ok","GPL","66","GPL MK10 66 Standard","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,0.97,1.1000000000000001,1.2,1,0.87,0.98,0.2,0.09,0,0.2,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1072,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GGL MK10 66 Standard","GGL","MK10","66","SOLAR","Standard","GGL 66","GPL 66","ok","GPL","66","GPL MK10 66 Standard","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,0.97,1.1000000000000001,1.2,1,0.87,0.98,0.2,0.09,0,0.2,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1067,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GGL MK10 70 Standard","GGL","MK10","70","MANUAL","Standard","GGL 70","GPL 70","ok","GPL","70","GPL MK10 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.2,0.26,7.0000000000000007E-2,0,0.26,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1075,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GGL MK10 70Q Standard","GGL","MK10","70Q","MANUAL","Standard","GGL 70Q","GPL 70","ok","GPL","70","GPL MK10 70 Standard",70,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.2,0.26,7.0000000000000007E-2,0,0.26,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1076,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GGL MK12 57 Standard","GGL","MK12","57","MANUAL","Standard","GGL 57","GPL 70","ok","GPL","70","GPL MK12 70 Standard","57",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1078,0.78,1.8,1.4,0.60000000000000009,1.61,4.41,0.96,0.43999999999999995,0.69]
["GGL MK12 66 Standard","GGL","MK12","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL MK12 66 Standard","66",1.1000000000000001,1.3,1.1000000000000001,1.2,0.99,1.1000000000000001,0.96,1.1000000000000001,1.2,1,0.86,0.98,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1079,0.78,1.8,1.4,0.60000000000000009,1.61,4.41,0.96,0.43999999999999995,0.69]
["GGL MK12 66 Standard","GGL","MK12","66","ELECTRIC","Standard","GGL 66","GPL 66","ok","GPL","66","GPL MK12 66 Standard","66",1.1000000000000001,1.3,1.1000000000000001,1.2,0.99,1.1000000000000001,0.96,1.1000000000000001,1.2,1,0.86,0.98,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1081,0.78,1.8,1.4,0.60000000000000009,1.61,4.41,0.96,0.43999999999999995,0.69]
["GGL MK12 70 Standard","GGL","MK12","70","MANUAL","Standard","GGL 70","GPL 70","ok","GPL","70","GPL MK12 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.26,7.0000000000000007E-2,0,0.26,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1083,0.78,1.8,1.4,0.60000000000000009,1.61,4.41,0.96,0.43999999999999995,0.69]
["GGL MK27 66 Standard","GGL","MK27","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL MK27 66 Standard","66",1.3,1.5,1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.98,1.1000000000000001,0.16,0.08,0,0.16,0.08,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1080,0.78,0.62,0.49,0.60000000000000009,0.43,2.06,0.26,0.22999999999999998,0.53]
["GGL PK04 57 Standard","GGL","PK04",57,"MANUAL","Standard","GGL 57","GPL 70","ok","GPL","70","GPL PK04 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1087,0.94199999999999995,0.98,0.92,0.76200000000000001,0.78,3.09,0.6,0.32000000000000006,0.65]
["GGL PK04 57 Standard","GGL","PK04",57,"ELECTRIC","Standard","GGL 57","GPL 70","ok","GPL","70","GPL PK04 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1085,0.94199999999999995,0.98,0.92,0.76200000000000001,0.78,3.09,0.6,0.32000000000000006,0.65]
["GGL PK04 62 Standard","GGL","PK04","62","MANUAL","Standard","GGL 62","GPL 62","ok","GPL","62","GPL PK04 62 Standard","62",1.1000000000000001,1.3,1,1.2,0.98,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.85,0.96,0.24,0.08,0,0.24,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1086,0.94199999999999995,0.98,0.92,0.76200000000000001,0.78,3.09,0.6,0.32000000000000006,0.65]
["GGL PK04 62 Standard","GGL","PK04","62","ELECTRIC","Standard","GGL 62","GPL 62","ok","GPL","62","GPL PK04 62 Standard","62",1.1000000000000001,1.3,1,1.2,0.98,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.85,0.96,0.24,0.08,0,0.24,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1089,0.94199999999999995,0.98,0.92,0.76200000000000001,0.78,3.09,0.6,0.32000000000000006,0.65]
["GGL PK04 66 Standard","GGL","PK04","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL PK04 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1,1.2,0.99,1.1000000000000001,1.3,1.1000000000000001,0.88,0.99,0.2,0.08,0,0.2,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1090,0.94199999999999995,0.98,0.92,0.76200000000000001,0.78,3.09,0.6,0.32000000000000006,0.65]
["GGL PK04 70Q Standard","GGL","PK04","70Q","MANUAL","Standard","GGL 70Q","GPL 70","ok","GPL","70","GPL PK04 70 Standard",70,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.25,0.06,0,0.25,0.06,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1092,0.94199999999999995,0.98,0.92,0.76200000000000001,0.78,3.09,0.6,0.32000000000000006,0.65]
["GGL PK06 57 Standard","GGL","PK06",57,"ELECTRIC","Standard","GGL 57","GPL 70","ok","GPL","70","GPL PK06 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1093,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGL PK06 57 Standard","GGL","PK06",57,"MANUAL","Standard","GGL 57","GPL 70","ok","GPL","70","GPL PK06 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1094,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGL PK06 62 Standard","GGL","PK06","62","MANUAL","Standard","GGL 62","GPL 62","ok","GPL","62","GPL PK06 62 Standard","62",1.1000000000000001,1.3,1,1.2,0.95,1.1000000000000001,0.92,1.1000000000000001,1.2,1,0.83,0.94,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1095,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGL PK06 62 Standard","GGL","PK06","62","ELECTRIC","Standard","GGL 62","GPL 62","ok","GPL","62","GPL PK06 62 Standard","62",1.1000000000000001,1.3,1,1.2,0.95,1.1000000000000001,0.92,1.1000000000000001,1.2,1,0.83,0.94,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1096,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGL PK06 66 Standard","GGL","PK06","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL PK06 66 Standard","66",1.1000000000000001,1.3,1.1000000000000001,1.2,0.99,1.1000000000000001,0.96,1.1000000000000001,1.2,1,0.86,0.98,0.2,0.09,0,0.2,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1097,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGL PK06 66 Standard","GGL","PK06","66","ELECTRIC","Standard","GGL 66","GPL 66","ok","GPL","66","GPL PK06 66 Standard","66",1.1000000000000001,1.3,1.1000000000000001,1.2,0.99,1.1000000000000001,0.96,1.1000000000000001,1.2,1,0.86,0.98,0.2,0.09,0,0.2,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1098,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGL PK06 70 Standard","GGL","PK06","70","MANUALBOTTOM","Standard","GGL 70","GPL 70","ok","GPL","70","GPL PK06 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.26,0.06,0,0.26,0.06,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1102,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGL PK06 70Q Standard","GGL","PK06","70Q","MANUAL","Standard","GGL 70Q","GPL 70","ok","GPL","70","GPL PK06 70 Standard",70,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.26,0.06,0,0.26,0.06,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1103,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGL PK06 76F Standard","GGL","PK06","76F","ELECTRIC","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL PK06 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.15,0.05,0,0.15,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.08,0,0.08,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1104,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGL PK06 76F Standard","GGL","PK06","76F","MANUAL","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL PK06 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.15,0.05,0,0.15,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.08,0,0.08,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1105,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGL PK08 57 Standard","GGL","PK08",57,"ELECTRIC","Standard","GGL 57","GPL 70","ok","GPL","70","GPL PK08 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.5,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1107,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGL PK08 57 Standard","GGL","PK08",57,"MANUAL","Standard","GGL 57","GPL 70","ok","GPL","70","GPL PK08 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.5,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1108,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGL PK08 62 Standard","GGL","PK08","62","MANUAL","Standard","GGL 62","GPL 62","ok","GPL","62","GPL PK08 62 Standard","62",1,1.2,0.98,1.2,0.93,1.1000000000000001,0.9,1.1000000000000001,1.2,0.99,0.81,0.93,0.26,0.08,0,0.26,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1109,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGL PK08 62 Standard","GGL","PK08","62","ELECTRIC","Standard","GGL 62","GPL 62","ok","GPL","62","GPL PK08 62 Standard","62",1,1.2,0.98,1.2,0.93,1.1000000000000001,0.9,1.1000000000000001,1.2,0.99,0.81,0.93,0.26,0.08,0,0.26,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1110,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGL PK08 66 Standard","GGL","PK08","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL PK08 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.97,1.1000000000000001,0.94,1.1000000000000001,1.2,1,0.85,0.97,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1111,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGL PK08 66 Standard","GGL","PK08","66","ELECTRIC","Standard","GGL 66","GPL 66","ok","GPL","66","GPL PK08 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.97,1.1000000000000001,0.94,1.1000000000000001,1.2,1,0.85,0.97,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1112,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGL PK08 66 Standard","GGL","PK08","66","SOLAR","Standard","GGL 66","GPL 66","ok","GPL","66","GPL PK08 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.97,1.1000000000000001,0.94,1.1000000000000001,1.2,1,0.85,0.97,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1113,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGL PK08 70 Standard","GGL","PK08","70","MANUAL","Standard","GGL 70","GPL 70","ok","GPL","70","GPL PK08 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.5,1.7,1.3,1,1.2,0.27,7.0000000000000007E-2,0,0.27,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1116,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGL PK08 70 Standard","GGL","PK08","70","MANUALBOTTOM","Standard","GGL 70","GPL 70","ok","GPL","70","GPL PK08 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.5,1.7,1.3,1,1.2,0.27,7.0000000000000007E-2,0,0.27,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1117,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGL PK08 70Q Standard","GGL","PK08","70Q","MANUAL","Standard","GGL 70Q","GPL 70","ok","GPL","70","GPL PK08 70 Standard",70,1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.5,1.7,1.3,1,1.2,0.27,7.0000000000000007E-2,0,0.27,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1118,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGL PK08 76F Standard","GGL","PK08","76F","MANUAL","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL PK08 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.5,1.7,1.3,1,1.2,0.13,0.05,0,0.13,0.05,0,0.02,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1119,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGL PK10 57 Standard","GGL","PK10",57,"ELECTRIC","Standard","GGL 57","GPL 70","ok","GPL","70","GPL PK10 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.5,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1120,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.71]
["GGL PK10 57 Standard","GGL","PK10",57,"MANUAL","Standard","GGL 57","GPL 70","ok","GPL","70","GPL PK10 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.5,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1121,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.71]
["GGL PK10 62 Standard","GGL","PK10","62","MANUAL","Standard","GGL 62","GPL 62","ok","GPL","62","GPL PK10 62 Standard","62",1,1.2,0.96,1.1000000000000001,0.91,1.1000000000000001,0.89,1,1.1000000000000001,0.98,0.8,0.92,0.27,0.08,0,0.27,0.09,0,0.05,0.08,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1122,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.71]
["GGL PK10 62 Standard","GGL","PK10","62","ELECTRIC","Standard","GGL 62","GPL 62","ok","GPL","62","GPL PK10 62 Standard","62",1,1.2,0.96,1.1000000000000001,0.91,1.1000000000000001,0.89,1,1.1000000000000001,0.98,0.8,0.92,0.27,0.08,0,0.27,0.09,0,0.05,0.08,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1123,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.71]
["GGL PK10 66 Standard","GGL","PK10","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL PK10 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.95,1.1000000000000001,0.93,1.1000000000000001,1.2,1,0.83,0.96,0.21,0.09,0,0.21,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1124,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.71]
["GGL PK10 66 Standard","GGL","PK10","66","ELECTRIC","Standard","GGL 66","GPL 66","ok","GPL","66","GPL PK10 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.95,1.1000000000000001,0.93,1.1000000000000001,1.2,1,0.83,0.96,0.21,0.09,0,0.21,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1125,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.71]
["GGL PK10 66 Standard","GGL","PK10","66","SOLAR","Standard","GGL 66","GPL 66","ok","GPL","66","GPL PK10 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.95,1.1000000000000001,0.93,1.1000000000000001,1.2,1,0.83,0.96,0.21,0.09,0,0.21,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1126,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.71]
["GGL PK10 70 Standard","GGL","PK10","70","ELECTRIC","Standard","GGL 70","GPL 70","ok","GPL","70","GPL PK10 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.5,1.7,1.3,1,1.2,0.27,7.0000000000000007E-2,0,0.27,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1130,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.71]
["GGL PK10 70 Standard","GGL","PK10","70","MANUALBOTTOM","Standard","GGL 70","GPL 70","ok","GPL","70","GPL PK10 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.5,1.7,1.3,1,1.2,0.27,7.0000000000000007E-2,0,0.27,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1131,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.71]
["GGL PK10 70Q Standard","GGL","PK10","70Q","MANUAL","Standard","GGL 70Q","GPL 70","ok","GPL","70","GPL PK10 70 Standard",70,1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.5,1.7,1.3,1,1.2,0.27,7.0000000000000007E-2,0,0.27,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1132,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.71]
["GGL PK10 76F Standard","GGL","PK10","76F","MANUAL","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL PK10 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1133,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.71]
["GGL PK25 62 Standard","GGL","PK25","62","MANUAL","Standard","GGL 62","GPL 62","ok","GPL","62","GPL PK25 62 Standard","62",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.96,1,0.19,7.0000000000000007E-2,0,0.19,0.08,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1135,0.94199999999999995,0.55000000000000004,0.52,0.76200000000000001,0.36,2.2400000000000002,0.27,0.25,0.52]
["GGL PK25 62 Standard","GGL","PK25","62","ELECTRIC","Standard","GGL 62","GPL 62","ok","GPL","62","GPL PK25 62 Standard","62",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.96,1,0.19,7.0000000000000007E-2,0,0.19,0.08,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1136,0.94199999999999995,0.55000000000000004,0.52,0.76200000000000001,0.36,2.2400000000000002,0.27,0.25,0.52]
["GGL PK25 66 Standard","GGL","PK25","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL PK25 66 Standard","66",1.3,1.5,1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.98,1.1000000000000001,0.16,0.08,0,0.16,0.08,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.32,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1137,0.94199999999999995,0.55000000000000004,0.52,0.76200000000000001,0.36,2.2400000000000002,0.27,0.25,0.52]
["GGL PK25 76F Standard","GGL","PK25","76F","MANUAL","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL PK25 70 Standard","76",1.5,1.9,1.4,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1138,0.94199999999999995,0.55000000000000004,0.52,0.76200000000000001,0.36,2.2400000000000002,0.27,0.25,0.52]
["GGL SK01 62 Standard","GGL","SK01","62","MANUAL","Standard","GGL 62","GPL 62","ok","GPL","62","GPL SK01 62 Standard","62",1.2,1.3,1.1000000000000001,1.2,1,1.2,0.99,1.1000000000000001,1.2,1,0.88,0.98,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1139,1.1399999999999999,0.7,0.8,0.96,0.5,2.93,0.49,0.31000000000000005,0.61]
["GGL SK01 62 Standard","GGL","SK01","62","ELECTRIC","Standard","GGL 62","GPL 62","ok","GPL","62","GPL SK01 62 Standard","62",1.2,1.3,1.1000000000000001,1.2,1,1.2,0.99,1.1000000000000001,1.2,1,0.88,0.98,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1140,1.1399999999999999,0.7,0.8,0.96,0.5,2.93,0.49,0.31000000000000005,0.61]
["GGL SK01 66 Standard","GGL","SK01","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL SK01 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.91,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1141,1.1399999999999999,0.7,0.8,0.96,0.5,2.93,0.49,0.31000000000000005,0.61]
["GGL SK01 70Q Standard","GGL","SK01","70Q","MANUAL","Standard","GGL 70Q","GPL 70","ok","GPL","70","GPL SK01 70 Standard",70,1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.23,0.06,0,0.23,0.06,0,0.04,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1142,1.1399999999999999,0.7,0.8,0.96,0.5,2.93,0.49,0.31000000000000005,0.61]
["GGL SK01 76F Standard","GGL","SK01","76F","MANUAL","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL SK01 70 Standard","76",1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.15,0.05,0,0.15,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.08,0,0.08,0.38,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1143,1.1399999999999999,0.7,0.8,0.96,0.5,2.93,0.49,0.31000000000000005,0.61]
["GGL SK06 54F Standard","GGL","SK06","54F","MANUAL","Standard","GGL 54F","GPL 54F","ok","GPL","54F","GPL SK06 54F Standard","54F",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.41,0.05,0,0.41,0.05,0,7.0000000000000007E-2,0.08,0,0.15,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.56999999999999995,0,0.1,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1144,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGL SK06 57 Standard","GGL","SK06",57,"ELECTRIC","Standard","GGL 57","GPL 70","ok","GPL","70","GPL SK06 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.99,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1145,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGL SK06 57 Standard","GGL","SK06",57,"MANUAL","Standard","GGL 57","GPL 70","ok","GPL","70","GPL SK06 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.99,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1146,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGL SK06 62 Standard","GGL","SK06","62","MANUAL","Standard","GGL 62","GPL 62","ok","GPL","62","GPL SK06 62 Standard","62",1,1.2,0.96,1.1000000000000001,0.91,1.1000000000000001,0.88,1,1.1000000000000001,0.98,0.8,0.92,0.26,0.08,0,0.26,0.09,0,0.05,0.08,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1147,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGL SK06 62 Standard","GGL","SK06","62","ELECTRIC","Standard","GGL 62","GPL 62","ok","GPL","62","GPL SK06 62 Standard","62",1,1.2,0.96,1.1000000000000001,0.91,1.1000000000000001,0.88,1,1.1000000000000001,0.98,0.8,0.92,0.26,0.08,0,0.26,0.09,0,0.05,0.08,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1148,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGL SK06 66 Standard","GGL","SK06","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL SK06 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.95,1.1000000000000001,0.93,1.1000000000000001,1.2,1,0.83,0.96,0.21,0.09,0,0.21,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1149,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGL SK06 66 Standard","GGL","SK06","66","ELECTRIC","Standard","GGL 66","GPL 66","ok","GPL","66","GPL SK06 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.95,1.1000000000000001,0.93,1.1000000000000001,1.2,1,0.83,0.96,0.21,0.09,0,0.21,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1150,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGL SK06 66 Standard","GGL","SK06","66","SOLAR","Standard","GGL 66","GPL 66","ok","GPL","66","GPL SK06 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.95,1.1000000000000001,0.93,1.1000000000000001,1.2,1,0.83,0.96,0.21,0.09,0,0.21,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1151,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGL SK06 70 Standard","GGL","SK06","70","MANUAL","Standard","GGL 70","GPL 70","ok","GPL","70","GPL SK06 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.99,1.2,0.27,7.0000000000000007E-2,0,0.27,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1155,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGL SK06 70 Standard","GGL","SK06","70","ELECTRIC","Standard","GGL 70","GPL 70","ok","GPL","70","GPL SK06 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.99,1.2,0.27,7.0000000000000007E-2,0,0.27,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1156,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGL SK06 70 Standard","GGL","SK06","70","MANUALBOTTOM","Standard","GGL 70","GPL 70","ok","GPL","70","GPL SK06 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.99,1.2,0.27,7.0000000000000007E-2,0,0.27,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1157,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGL SK06 70Q Standard","GGL","SK06","70Q","MANUAL","Standard","GGL 70Q","GPL 70","ok","GPL","70","GPL SK06 70 Standard",70,1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.99,1.2,0.27,7.0000000000000007E-2,0,0.27,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1158,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGL SK06 76F Standard","GGL","SK06","76F","ELECTRIC","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL SK06 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.99,1.2,0.16,0.05,0,0.16,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1159,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGL SK06 76F Standard","GGL","SK06","76F","MANUAL","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL SK06 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.99,1.2,0.16,0.05,0,0.16,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1160,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGL SK06 76F Standard","GGL","SK06","76F","SOLAR","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL SK06 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.99,1.2,0.16,0.05,0,0.16,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1161,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGL SK06 57 Standard","GGL","SK06",57,"SOLAR","Standard","GGL 57","GPL 70","ok","GPL","70","GPL SK06 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.99,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1162,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGL SK08 54F Standard","GGL","SK08","54F","MANUAL","Standard","GGL 54F","GPL 54F","ok","GPL","54F","GPL SK08 54F Standard","54F",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.39,0.05,0,0.39,0.05,0,7.0000000000000007E-2,0.08,0,0.15,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.59,0,0.1,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1163,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGL SK08 57 Standard","GGL","SK08",57,"MANUAL","Standard","GGL 57","GPL 70","ok","GPL","70","GPL SK08 70 Standard",57,1.3,1.8,1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.98,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.45,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1164,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGL SK08 62 Standard","GGL","SK08","62","MANUAL","Standard","GGL 62","GPL 62","ok","GPL","62","GPL SK08 62 Standard","62",0.99,1.2,0.93,1.1000000000000001,0.88,1.1000000000000001,0.86,1,1.1000000000000001,0.96,0.78,0.91,0.27,0.08,0,0.27,0.09,0,0.05,7.0000000000000007E-2,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.49,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1165,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGL SK08 62 Standard","GGL","SK08","62","ELECTRIC","Standard","GGL 62","GPL 62","ok","GPL","62","GPL SK08 62 Standard","62",0.99,1.2,0.93,1.1000000000000001,0.88,1.1000000000000001,0.86,1,1.1000000000000001,0.96,0.78,0.91,0.27,0.08,0,0.27,0.09,0,0.05,7.0000000000000007E-2,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.49,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1166,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGL SK08 66 Standard","GGL","SK08","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL SK08 66 Standard","66",1,1.3,0.98,1.2,0.93,1.1000000000000001,0.9,1.1000000000000001,1.2,1,0.82,0.94,0.22,0.09,0,0.22,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1167,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGL SK08 66 Standard","GGL","SK08","66","ELECTRIC","Standard","GGL 66","GPL 66","ok","GPL","66","GPL SK08 66 Standard","66",1,1.3,0.98,1.2,0.93,1.1000000000000001,0.9,1.1000000000000001,1.2,1,0.82,0.94,0.22,0.09,0,0.22,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1168,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGL SK08 70 Standard","GGL","SK08","70","MANUAL","Standard","GGL 70","GPL 70","ok","GPL","70","GPL SK08 70 Standard","70",1.3,1.8,1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.98,1.2,0.28000000000000003,7.0000000000000007E-2,0,0.28000000000000003,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.49,0,0.09,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1170,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGL SK08 70Q Standard","GGL","SK08","70Q","MANUAL","Standard","GGL 70Q","GPL 70","ok","GPL","70","GPL SK08 70 Standard",70,1.3,1.8,1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.98,1.2,0.28000000000000003,7.0000000000000007E-2,0,0.28000000000000003,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.49,0,0.09,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1171,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGL SK08 76F Standard","GGL","SK08","76F","MANUAL","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL SK08 70 Standard","76",1.3,1.8,1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.98,1.2,0.15,0.05,0,0.15,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.45,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1172,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGL SK08 76F Standard","GGL","SK08","76F","SOLAR","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL SK08 70 Standard","76",1.3,1.8,1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.98,1.2,0.15,0.05,0,0.15,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.45,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1173,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGL SK08 57 Standard","GGL","SK08",57,"ELECTRIC","Standard","GGL 57","GPL 70","ok","GPL","70","GPL SK08 70 Standard",57,1.3,1.8,1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.98,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.45,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1174,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGL SK08 57 Standard","GGL","SK08",57,"SOLAR","Standard","GGL 57","GPL 70","ok","GPL","70","GPL SK08 70 Standard",57,1.3,1.8,1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.98,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.45,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1175,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGL SK10 66 Standard","GGL","SK10","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL SK10 66 Standard","66",1,1.2,0.97,1.2,0.91,1.1000000000000001,0.89,1.1000000000000001,1.2,0.99,0.8,0.93,0.22,0.09,0,0.22,0.1,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1176,1.1399999999999999,1.6,1.82,0.96,1.41,4.7300000000000004,1.35,0.47,0.74]
["GGL SK10 66 Standard","GGL","SK10","66","ELECTRIC","Standard","GGL 66","GPL 66","ok","GPL","66","GPL SK10 66 Standard","66",1,1.2,0.97,1.2,0.91,1.1000000000000001,0.89,1.1000000000000001,1.2,0.99,0.8,0.93,0.22,0.09,0,0.22,0.1,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1177,1.1399999999999999,1.6,1.82,0.96,1.41,4.7300000000000004,1.35,0.47,0.74]
["GGL SK10 70 Standard","GGL","SK10","70","MANUAL","Standard","GGL 70","GPL 70","ok","GPL","70","GPL SK10 70 Standard","70",1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.97,1.2,0.28000000000000003,7.0000000000000007E-2,0,0.28000000000000003,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.5,0,0.09,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1180,1.1399999999999999,1.6,1.82,0.96,1.41,4.7300000000000004,1.35,0.47,0.74]
["GGL SK10 70Q Standard","GGL","SK10","70Q","MANUAL","Standard","GGL 70Q","GPL 70","ok","GPL","70","GPL SK10 70 Standard",70,1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.97,1.2,0.28000000000000003,7.0000000000000007E-2,0,0.28000000000000003,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.5,0,0.09,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1181,1.1399999999999999,1.6,1.82,0.96,1.41,4.7300000000000004,1.35,0.47,0.74]
["GGL SK10 76F Standard","GGL","SK10","76F","MANUAL","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL SK10 70 Standard","76",1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.97,1.2,0.16,0.05,0,0.16,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1182,1.1399999999999999,1.6,1.82,0.96,1.41,4.7300000000000004,1.35,0.47,0.74]
["GGL UK04 54F Standard","GGL","UK04","54F","MANUAL","Standard","GGL 54F","GPL 54F","ok","GPL","54F","GPL UK04 54F Standard","54F",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.42,0.05,0,0.42,0.05,0,0.08,0.08,0,0.15,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.56000000000000005,0,0.1,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1183,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGL UK04 57 Standard","GGL","UK04",57,"ELECTRIC","Standard","GGL 57","GPL 70","ok","GPL","70","GPL UK04 70 Standard",57,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1184,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGL UK04 57 Standard","GGL","UK04",57,"MANUAL","Standard","GGL 57","GPL 70","ok","GPL","70","GPL UK04 70 Standard",57,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1185,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGL UK04 66 Standard","GGL","UK04","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL UK04 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.96,1.1000000000000001,0.93,1.1000000000000001,1.2,1,0.84,0.96,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1186,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGL UK04 66 Standard","GGL","UK04","66","ELECTRIC","Standard","GGL 66","GPL 66","ok","GPL","66","GPL UK04 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.96,1.1000000000000001,0.93,1.1000000000000001,1.2,1,0.84,0.96,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1187,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGL UK04 66 Standard","GGL","UK04","66","SOLAR","Standard","GGL 66","GPL 66","ok","GPL","66","GPL UK04 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.96,1.1000000000000001,0.93,1.1000000000000001,1.2,1,0.84,0.96,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1188,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGL UK04 70 Standard","GGL","UK04","70","MANUAL","Standard","GGL 70","GPL 70","ok","GPL","70","GPL UK04 70 Standard","70",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.26,7.0000000000000007E-2,0,0.26,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1192,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGL UK04 70Q Standard","GGL","UK04","70Q","MANUAL","Standard","GGL 70Q","GPL 70","ok","GPL","70","GPL UK04 70 Standard",70,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.26,7.0000000000000007E-2,0,0.26,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1193,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGL UK04 76F Standard","GGL","UK04","76F","ELECTRIC","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL UK04 70 Standard","76",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.16,0.05,0,0.16,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1194,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGL UK04 76F Standard","GGL","UK04","76F","MANUAL","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL UK04 70 Standard","76",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.16,0.05,0,0.16,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1195,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGL UK04 76F Standard","GGL","UK04","76F","SOLAR","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL UK04 70 Standard","76",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.16,0.05,0,0.16,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1196,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGL UK04 70H Standard","GGL","UK04","70H","MANUAL","Standard","GGL 70H","GPL 70","ok","GPL","70","GPL UK04 70 Standard",70,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.26,7.0000000000000007E-2,0,0.26,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1197,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGL UK04 57 Standard","GGL","UK04",57,"SOLAR","Standard","GGL 57","GPL 70","ok","GPL","70","GPL UK04 70 Standard",57,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1198,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGL UK04 70 Standard","GGL","UK04","70","ELECTRIC","Standard","GGL 70","GPL 70","ok","GPL","70","GPL UK04 70 Standard","70",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.26,7.0000000000000007E-2,0,0.26,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1199,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGL UK08 54F Standard","GGL","UK08","54F","MANUAL","Standard","GGL 54F","GPL 54F","ok","GPL","54F","GPL UK08 54F Standard","54F",1.4,1.8,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.28999999999999998,0.05,0,0.28999999999999998,0.05,0,0.05,0.1,0,0.15,0,0.08,0,0.08,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.61,0,0.1,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1200,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGL UK08 57 Standard","GGL","UK08",57,"MANUAL","Standard","GGL 57","GPL 70","ok","GPL","70","GPL UK08 70 Standard",57,1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.97,1.2,0.16,0.05,0,0.16,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1201,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGL UK08 66 Standard","GGL","UK08","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL UK08 66 Standard","66",1,1.2,0.95,1.2,0.9,1.1000000000000001,0.88,1,1.2,0.98,0.79,0.93,0.22,0.09,0,0.22,0.1,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1202,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGL UK08 66 Standard","GGL","UK08","66","ELECTRIC","Standard","GGL 66","GPL 66","ok","GPL","66","GPL UK08 66 Standard","66",1,1.2,0.95,1.2,0.9,1.1000000000000001,0.88,1,1.2,0.98,0.79,0.93,0.22,0.09,0,0.22,0.1,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1203,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGL UK08 66 Standard","GGL","UK08","66","SOLAR","Standard","GGL 66","GPL 66","ok","GPL","66","GPL UK08 66 Standard","66",1,1.2,0.95,1.2,0.9,1.1000000000000001,0.88,1,1.2,0.98,0.79,0.93,0.22,0.09,0,0.22,0.1,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1204,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGL UK08 70 Standard","GGL","UK08","70","MANUAL","Standard","GGL 70","GPL 70","ok","GPL","70","GPL UK08 70 Standard","70",1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.97,1.2,0.28000000000000003,7.0000000000000007E-2,0,0.28000000000000003,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.51,0,0.09,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1207,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGL UK08 70 Standard","GGL","UK08","70","ELECTRIC","Standard","GGL 70","GPL 70","ok","GPL","70","GPL UK08 70 Standard","70",1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.97,1.2,0.28000000000000003,7.0000000000000007E-2,0,0.28000000000000003,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.51,0,0.09,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1208,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGL UK08 70Q Standard","GGL","UK08","70Q","MANUAL","Standard","GGL 70Q","GPL 70","ok","GPL","70","GPL UK08 70 Standard",70,1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.97,1.2,0.28000000000000003,7.0000000000000007E-2,0,0.28000000000000003,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.51,0,0.09,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1209,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGL UK08 76F Standard","GGL","UK08","76F","ELECTRIC","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL UK08 70 Standard","76",1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.97,1.2,0.11,0.05,0,0.11,0.05,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1210,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGL UK08 76F Standard","GGL","UK08","76F","MANUAL","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL UK08 70 Standard","76",1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.97,1.2,0.11,0.05,0,0.11,0.05,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1211,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGL UK08 76F Standard","GGL","UK08","76F","SOLAR","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL UK08 70 Standard","76",1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.97,1.2,0.11,0.05,0,0.11,0.05,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1212,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGL UK08 57 Standard","GGL","UK08",57,"ELECTRIC","Standard","GGL 57","GPL 70","ok","GPL","70","GPL UK08 70 Standard",57,1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.97,1.2,0.16,0.05,0,0.16,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1213,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGL UK08 57 Standard","GGL","UK08",57,"SOLAR","Standard","GGL 57","GPL 70","ok","GPL","70","GPL UK08 70 Standard",57,1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.97,1.2,0.16,0.05,0,0.16,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1214,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGL UK10 66 Standard","GGL","UK10","66","MANUAL","Standard","GGL 66","GPL 66","ok","GPL","66","GPL UK10 66 Standard","66",0.99,1.2,0.93,1.1000000000000001,0.89,1.1000000000000001,0.86,1,1.1000000000000001,0.97,0.78,0.92,0.23,0.09,0,0.23,0.1,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1216,1.34,1.6,2.14,1.1600000000000001,1.41,5.13,1.63,0.51000000000000023,0.76]
["GGL UK10 66 Standard","GGL","UK10","66","ELECTRIC","Standard","GGL 66","GPL 66","ok","GPL","66","GPL UK10 66 Standard","66",0.99,1.2,0.93,1.1000000000000001,0.89,1.1000000000000001,0.86,1,1.1000000000000001,0.97,0.78,0.92,0.23,0.09,0,0.23,0.1,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1217,1.34,1.6,2.14,1.1600000000000001,1.41,5.13,1.63,0.51000000000000023,0.76]
["GGL UK10 70Q Standard","GGL","UK10","70Q","MANUAL","Standard","GGL 70Q","GPL 70","ok","GPL","70","GPL UK10 70 Standard",70,1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.96,1.2,0.28999999999999998,7.0000000000000007E-2,0,0.28999999999999998,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.52,0,0.09,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1220,1.34,1.6,2.14,1.1600000000000001,1.41,5.13,1.63,0.51000000000000023,0.76]
["GGL UK10 76F Standard","GGL","UK10","76F","MANUAL","Standard","GGL 76F","GPL 70","ok","GPL","70","GPL UK10 70 Standard","76",1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.96,1.2,0.13,0.05,0,0.13,0.05,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1221,1.34,1.6,2.14,1.1600000000000001,1.41,5.13,1.63,0.51000000000000023,0.76]
["GPLS FFKF06 66 Standard","GPLS","FFKF06","66","MANUAL","Standard","GPLS 66","GPLS 66 3in1","ok","GPLS",66,"GPLS FFKF06 66 Standard","66",1.3,1.3,1.2,1.2,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1,1,0.97,0.97,0.21,7.0000000000000007E-2,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1616,1.88,1.18,2.21,1.444,0.98,8.7899999999999991,1.42,0.79,0.64]
["GGLS FFKF06 66 Standard + BDX","GGLS","FFKF06","66","MANUAL","Standard + BDX","GGLS 66","GGLS 66 3in1","ok","GGLS",66,"GGLS FFKF06 66 Standard + BDX","66",1.1000000000000001,1.3,1,1.2,0.97,1.1000000000000001,0.94,1.1000000000000001,0.89,1,0.85,0.96,0.2,7.0000000000000007E-2,0,0.2,0.09,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",159,1.9419999999999999,1.28,2.4900000000000002,1.444,0.98,8.7899999999999991,1.42,0.79,0.56999999999999995]
["GGLS FFKF06 66 Standard + BDX","GGLS","FFKF06","66","SOLAR","Standard + BDX","GGLS 66","GGLS 66 3in1","ok","GGLS",66,"GGLS FFKF06 66 Standard + BDX","66",1.1000000000000001,1.3,1,1.2,0.97,1.1000000000000001,0.94,1.1000000000000001,0.89,1,0.85,0.96,0.2,7.0000000000000007E-2,0,0.2,0.09,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",160,1.9419999999999999,1.28,2.4900000000000002,1.444,0.98,8.7899999999999991,1.42,0.79,0.56999999999999995]
["GPLS FFKF06 66 Standard + BDX","GPLS","FFKF06","66","MANUAL","Standard + BDX","GPLS 66","GPLS 66 3in1","ok","GPLS",66,"GPLS FFKF06 66 Standard + BDX","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,0.98,1.1000000000000001,0.93,1,0.88,0.99,0.2,7.0000000000000007E-2,0,0.2,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.9419999999999999,1.28,2.4900000000000002,1.444,0.98,8.7899999999999991,1.42,0.79,0.56999999999999995]
["GGU CK02 57 Standard","GGU","CK02",57,"MANUAL","Standard","GGU 57","GPU 70","ok","GPU","70","GPU CK02 70 Standard",57,1.6,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.06,0,0.02,0.1,0,0.13,0,0.08,0,0.08,0,0.09,0,0.09,0.31,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1286,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGU CK02 57 Standard","GGU","CK02",57,"ELECTRIC","Standard","GGU 57","GPU 70","ok","GPU","70","GPU CK02 70 Standard",57,1.6,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.06,0,0.02,0.1,0,0.13,0,0.08,0,0.08,0,0.09,0,0.09,0.31,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1288,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGU CK02 62 Standard","GGU","CK02","62","MANUAL","Standard","GGU 62","GPU 62","ok","GPU","62","GPU CK02 62 Standard","62",1.3,1.5,1.2,1.4,1.2,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.98,1.1000000000000001,0.19,7.0000000000000007E-2,0,0.19,0.08,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1287,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGU CK02 62 Standard","GGU","CK02","62","ELECTRIC","Standard","GGU 62","GPU 62","ok","GPU","62","GPU CK02 62 Standard","62",1.3,1.5,1.2,1.4,1.2,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.98,1.1000000000000001,0.19,7.0000000000000007E-2,0,0.19,0.08,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1289,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGU CK02 66 Standard","GGU","CK02","66","MANUAL","Standard","GGU 66","GPU 66","ok","GPU","66","GPU CK02 66 Standard","66",1.4,1.5,1.3,1.4,1.2,1.3,1.2,1.3,1.4,1.2,1,1.1000000000000001,0.15,0.08,0,0.15,0.08,0,0.03,0.1,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.31,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1290,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGU CK02 66 Standard","GGU","CK02","66","ELECTRIC","Standard","GGU 66","GPU 66","ok","GPU","66","GPU CK02 66 Standard","66",1.4,1.5,1.3,1.4,1.2,1.3,1.2,1.3,1.4,1.2,1,1.1000000000000001,0.15,0.08,0,0.15,0.08,0,0.03,0.1,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.31,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1291,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGU CK02 66 Standard","GGU","CK02","66","SOLAR","Standard","GGU 66","GPU 66","ok","GPU","66","GPU CK02 66 Standard","66",1.4,1.5,1.3,1.4,1.2,1.3,1.2,1.3,1.4,1.2,1,1.1000000000000001,0.15,0.08,0,0.15,0.08,0,0.03,0.1,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.31,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1292,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGU CK02 70 Standard","GGU","CK02","70","MANUAL","Standard","GGU 70","GPU 70","ok","GPU","70","GPU CK02 70 Standard","70",1.6,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.19,0.06,0,0.19,0.06,0,0.04,0.1,0,0.14000000000000001,0,0.08,0,0.08,0,0.09,0,0.09,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1297,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGU CK02 70Q Standard","GGU","CK02","70Q","MANUAL","Standard","GGU 70Q","GPU 70","ok","GPU","70","GPU CK02 70 Standard",70,1.6,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.19,0.06,0,0.19,0.06,0,0.04,0.1,0,0.14000000000000001,0,0.08,0,0.08,0,0.09,0,0.09,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1299,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGU CK02 76F Standard","GGU","CK02","76F","MANUAL","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU CK02 70 Standard","76",1.6,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.05,0,0.02,0.1,0,0.13,0,0.08,0,0.08,0,0.09,0,0.09,0.31,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1298,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGU CK02 76F Standard","GGU","CK02","76F","ELECTRIC","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU CK02 70 Standard","76",1.6,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.05,0,0.02,0.1,0,0.13,0,0.08,0,0.08,0,0.09,0,0.09,0.31,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1305,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGU CK04 57 Standard","GGU","CK04",57,"MANUAL","Standard","GGU 57","GPU 70","ok","GPU","70","GPU CK04 70 Standard",57,1.6,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.06,0,0.02,0.1,0,0.12,0,0.08,0,0.08,0,0.08,0,0.08,0.33,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1300,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGU CK04 57 Standard","GGU","CK04",57,"ELECTRIC","Standard","GGU 57","GPU 70","ok","GPU","70","GPU CK04 70 Standard",57,1.6,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.06,0,0.02,0.1,0,0.12,0,0.08,0,0.08,0,0.08,0,0.08,0.33,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1301,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGU CK04 62 Standard","GGU","CK04","62","MANUAL","Standard","GGU 62","GPU 62","ok","GPU","62","GPU CK04 62 Standard","62",1.3,1.5,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.96,1,0.2,0.08,0,0.2,0.08,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1302,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGU CK04 62 Standard","GGU","CK04","62","ELECTRIC","Standard","GGU 62","GPU 62","ok","GPU","62","GPU CK04 62 Standard","62",1.3,1.5,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.96,1,0.2,0.08,0,0.2,0.08,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1304,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGU CK04 66 Standard","GGU","CK04","66","MANUAL","Standard","GGU 66","GPU 66","ok","GPU","66","GPU CK04 66 Standard","66",1.4,1.5,1.3,1.4,1.2,1.3,1.2,1.2,1.4,1.1000000000000001,1,1.1000000000000001,0.16,0.08,0,0.16,0.09,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1303,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGU CK04 66 Standard","GGU","CK04","66","ELECTRIC","Standard","GGU 66","GPU 66","ok","GPU","66","GPU CK04 66 Standard","66",1.4,1.5,1.3,1.4,1.2,1.3,1.2,1.2,1.4,1.1000000000000001,1,1.1000000000000001,0.16,0.08,0,0.16,0.09,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1306,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGU CK04 66 Standard","GGU","CK04","66","SOLAR","Standard","GGU 66","GPU 66","ok","GPU","66","GPU CK04 66 Standard","66",1.4,1.5,1.3,1.4,1.2,1.3,1.2,1.2,1.4,1.1000000000000001,1,1.1000000000000001,0.16,0.08,0,0.16,0.09,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1307,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGU CK04 70 Standard","GGU","CK04","70","MANUAL","Standard","GGU 70","GPU 70","ok","GPU","70","GPU CK04 70 Standard","70",1.6,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.21,0.06,0,0.21,0.06,0,0.04,0.1,0,0.14000000000000001,0,0.08,0,0.08,0,0.08,0,0.08,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1311,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGU CK04 70Q Standard","GGU","CK04","70Q","MANUAL","Standard","GGU 70Q","GPU 70","ok","GPU","70","GPU CK04 70 Standard",70,1.6,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.21,0.06,0,0.21,0.06,0,0.04,0.1,0,0.14000000000000001,0,0.08,0,0.08,0,0.08,0,0.08,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1312,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGU CK04 76F Standard","GGU","CK04","76F","MANUAL","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU CK04 70 Standard","76",1.6,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.05,0,0.02,0.1,0,0.12,0,0.08,0,0.08,0,0.08,0,0.08,0.34,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1313,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGU CK04 76F Standard","GGU","CK04","76F","ELECTRIC","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU CK04 70 Standard","76",1.6,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.05,0,0.02,0.1,0,0.12,0,0.08,0,0.08,0,0.08,0,0.08,0.34,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1314,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGU CK06 62 Standard","GGU","CK06","62","MANUAL","Standard","GGU 62","GPU 62","ok","GPU","62","GPU CK06 62 Standard","62",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.95,1,0.21,0.08,0,0.21,0.08,0,0.04,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1315,0.55000000000000004,1.18,0.65,0.37000000000000005,0.98,2.71,0.36,0.29000000000000004,0.55000000000000004]
["GGU CK06 62 Standard","GGU","CK06","62","ELECTRIC","Standard","GGU 62","GPU 62","ok","GPU","62","GPU CK06 62 Standard","62",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.95,1,0.21,0.08,0,0.21,0.08,0,0.04,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1316,0.55000000000000004,1.18,0.65,0.37000000000000005,0.98,2.71,0.36,0.29000000000000004,0.55000000000000004]
["GGU CK06 66 Standard","GGU","CK06","66","MANUAL","Standard","GGU 66","GPU 66","ok","GPU","66","GPU CK06 66 Standard","66",1.4,1.5,1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,1,1.1000000000000001,0.17,0.08,0,0.17,0.09,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1317,0.55000000000000004,1.18,0.65,0.37000000000000005,0.98,2.71,0.36,0.29000000000000004,0.55000000000000004]
["GGU CK06 66 Standard","GGU","CK06","66","ELECTRIC","Standard","GGU 66","GPU 66","ok","GPU","66","GPU CK06 66 Standard","66",1.4,1.5,1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,1,1.1000000000000001,0.17,0.08,0,0.17,0.09,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1318,0.55000000000000004,1.18,0.65,0.37000000000000005,0.98,2.71,0.36,0.29000000000000004,0.55000000000000004]
["GGU CK06 66 Standard","GGU","CK06","66","SOLAR","Standard","GGU 66","GPU 66","ok","GPU","66","GPU CK06 66 Standard","66",1.4,1.5,1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,1,1.1000000000000001,0.17,0.08,0,0.17,0.09,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1319,0.55000000000000004,1.18,0.65,0.37000000000000005,0.98,2.71,0.36,0.29000000000000004,0.55000000000000004]
["GGU FK04 62 Standard","GGU","FK04","62","MANUAL","Standard","GGU 62","GPU 62","ok","GPU","62","GPU FK04 62 Standard","62",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.92,1,0.22,0.08,0,0.22,0.08,0,0.04,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1323,0.66,0.98,0.65,0.48000000000000004,0.78,2.5299999999999998,0.38,0.27,0.57999999999999996]
["GGU FK04 62 Standard","GGU","FK04","62","ELECTRIC","Standard","GGU 62","GPU 62","ok","GPU","62","GPU FK04 62 Standard","62",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.92,1,0.22,0.08,0,0.22,0.08,0,0.04,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1324,0.66,0.98,0.65,0.48000000000000004,0.78,2.5299999999999998,0.38,0.27,0.57999999999999996]
["GGU FK04 66 Standard","GGU","FK04","66","MANUAL","Standard","GGU 66","GPU 66","ok","GPU","66","GPU FK04 66 Standard","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.97,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1325,0.66,0.98,0.65,0.48000000000000004,0.78,2.5299999999999998,0.38,0.27,0.57999999999999996]
["GGU FK04 66 Standard","GGU","FK04","66","ELECTRIC","Standard","GGU 66","GPU 66","ok","GPU","66","GPU FK04 66 Standard","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.97,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1326,0.66,0.98,0.65,0.48000000000000004,0.78,2.5299999999999998,0.38,0.27,0.57999999999999996]
["GGU FK04 70Q Standard","GGU","FK04","70Q","MANUAL","Standard","GGU 70Q","GPU 70","ok","GPU","70","GPU FK04 70 Standard",70,1.5,1.9,1.4,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.22,7.0000000000000007E-2,0,0.22,7.0000000000000007E-2,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1329,0.66,0.98,0.65,0.48000000000000004,0.78,2.5299999999999998,0.38,0.27,0.57999999999999996]
["GGU FK06 62 Standard","GGU","FK06","62","MANUAL","Standard","GGU 62","GPU 62","ok","GPU","62","GPU FK06 62 Standard","62",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.9,1,0.22,0.08,0,0.22,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1330,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GGU FK06 62 Standard","GGU","FK06","62","ELECTRIC","Standard","GGU 62","GPU 62","ok","GPU","62","GPU FK06 62 Standard","62",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.9,1,0.22,0.08,0,0.22,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1331,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GGU FK06 66 Standard","GGU","FK06","66","MANUAL","Standard","GGU 66","GPU 66","ok","GPU","66","GPU FK06 66 Standard","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.95,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1332,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GGU FK06 66 Standard","GGU","FK06","66","ELECTRIC","Standard","GGU 66","GPU 66","ok","GPU","66","GPU FK06 66 Standard","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.95,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1333,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GGU FK06 66 Standard","GGU","FK06","66","SOLAR","Standard","GGU 66","GPU 66","ok","GPU","66","GPU FK06 66 Standard","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.95,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1334,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GGU FK06 70Q Standard","GGU","FK06","70Q","MANUAL","Standard","GGU 70Q","GPU 70","ok","GPU","70","GPU FK06 70 Standard",70,1.5,1.9,1.4,1.7,1.3,1.6,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.23,7.0000000000000007E-2,0,0.23,7.0000000000000007E-2,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1338,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GGU FK06 76F Standard","GGU","FK06","76F","MANUAL","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU FK06 70 Standard","76",1.5,1.9,1.4,1.7,1.3,1.6,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.13,0.05,0,0.13,0.05,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1339,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GGU FK08 62 Standard","GGU","FK08","62","MANUAL","Standard","GGU 62","GPU 62","ok","GPU","62","GPU FK08 62 Standard","62",1.2,1.3,1.1000000000000001,1.2,1,1.2,0.99,1.1000000000000001,1.2,1.1000000000000001,0.89,0.99,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1340,0.66,1.4,0.92,0.48000000000000004,1.2,3.37,0.57999999999999996,0.34000000000000008,0.63]
["GGU FK08 62 Standard","GGU","FK08","62","ELECTRIC","Standard","GGU 62","GPU 62","ok","GPU","62","GPU FK08 62 Standard","62",1.2,1.3,1.1000000000000001,1.2,1,1.2,0.99,1.1000000000000001,1.2,1.1000000000000001,0.89,0.99,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1341,0.66,1.4,0.92,0.48000000000000004,1.2,3.37,0.57999999999999996,0.34000000000000008,0.63]
["GGU FK08 66 Standard","GGU","FK08","66","MANUAL","Standard","GGU 66","GPU 66","ok","GPU","66","GPU FK08 66 Standard","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.94,1,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1342,0.66,1.4,0.92,0.48000000000000004,1.2,3.37,0.57999999999999996,0.34000000000000008,0.63]
["GGU FK08 66 Standard","GGU","FK08","66","ELECTRIC","Standard","GGU 66","GPU 66","ok","GPU","66","GPU FK08 66 Standard","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.94,1,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1343,0.66,1.4,0.92,0.48000000000000004,1.2,3.37,0.57999999999999996,0.34000000000000008,0.63]
["GGU FK08 66 Standard","GGU","FK08","66","SOLAR","Standard","GGU 66","GPU 66","ok","GPU","66","GPU FK08 66 Standard","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.94,1,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1344,0.66,1.4,0.92,0.48000000000000004,1.2,3.37,0.57999999999999996,0.34000000000000008,0.63]
["GGU MK04 57 Standard","GGU","MK04",57,"MANUAL","Standard","GGU 57","GPU 70","ok","GPU","70","GPU MK04 70 Standard",57,1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.13,0.05,0,0.13,7.0000000000000007E-2,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1348,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGU MK04 57 Standard","GGU","MK04",57,"ELECTRIC","Standard","GGU 57","GPU 70","ok","GPU","70","GPU MK04 70 Standard",57,1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.13,0.05,0,0.13,7.0000000000000007E-2,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1349,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGU MK04 57 Standard","GGU","MK04",57,"SOLAR","Standard","GGU 57","GPU 70","ok","GPU","70","GPU MK04 70 Standard",57,1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.13,0.05,0,0.13,7.0000000000000007E-2,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1350,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGU MK04 62 Standard","GGU","MK04","62","MANUAL","Standard","GGU 62","GPU 62","ok","GPU","62","GPU MK04 62 Standard","62",1.2,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.98,1.1000000000000001,1.2,1,0.88,0.98,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1351,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGU MK04 62 Standard","GGU","MK04","62","ELECTRIC","Standard","GGU 62","GPU 62","ok","GPU","62","GPU MK04 62 Standard","62",1.2,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.98,1.1000000000000001,1.2,1,0.88,0.98,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1352,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGU MK04 66 Standard","GGU","MK04","66","MANUAL","Standard","GGU 66","GPU 66","ok","GPU","66","GPU MK04 66 Standard","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.94,1,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1353,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGU MK04 66 Standard","GGU","MK04","66","ELECTRIC","Standard","GGU 66","GPU 66","ok","GPU","66","GPU MK04 66 Standard","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.94,1,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1354,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGU MK04 66 Standard","GGU","MK04","66","SOLAR","Standard","GGU 66","GPU 66","ok","GPU","66","GPU MK04 66 Standard","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.94,1,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1355,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGU MK04 70 Standard","GGU","MK04","70","MANUAL","Standard","GGU 70","GPU 70","ok","GPU","70","GPU MK04 70 Standard","70",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.23,7.0000000000000007E-2,0,0.23,7.0000000000000007E-2,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1360,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGU MK04 70Q Standard","GGU","MK04","70Q","MANUAL","Standard","GGU 70Q","GPU 70","ok","GPU","70","GPU MK04 70 Standard",70,1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.23,7.0000000000000007E-2,0,0.23,7.0000000000000007E-2,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1361,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGU MK04 76F Standard","GGU","MK04","76F","MANUAL","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU MK04 70 Standard","76",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1362,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGU MK04 76F Standard","GGU","MK04","76F","ELECTRIC","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU MK04 70 Standard","76",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1363,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGU MK06 57 Standard","GGU","MK06",57,"MANUAL","Standard","GGU 57","GPU 70","ok","GPU","70","GPU MK06 70 Standard",57,1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1364,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGU MK06 57 Standard","GGU","MK06",57,"ELECTRIC","Standard","GGU 57","GPU 70","ok","GPU","70","GPU MK06 70 Standard",57,1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1365,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGU MK06 57 Standard","GGU","MK06",57,"SOLAR","Standard","GGU 57","GPU 70","ok","GPU","70","GPU MK06 70 Standard",57,1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1366,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGU MK06 62 Standard","GGU","MK06","62","MANUAL","Standard","GGU 62","GPU 62","ok","GPU","62","GPU MK06 62 Standard","62",1.1000000000000001,1.3,1,1.2,0.99,1.1000000000000001,0.96,1.1000000000000001,1.2,1,0.86,0.97,0.24,0.08,0,0.24,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1367,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGU MK06 62 Standard","GGU","MK06","62","ELECTRIC","Standard","GGU 62","GPU 62","ok","GPU","62","GPU MK06 62 Standard","62",1.1000000000000001,1.3,1,1.2,0.99,1.1000000000000001,0.96,1.1000000000000001,1.2,1,0.86,0.97,0.24,0.08,0,0.24,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1368,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGU MK06 66 Standard","GGU","MK06","66","MANUAL","Standard","GGU 66","GPU 66","ok","GPU","66","GPU MK06 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.92,1,0.19,0.09,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1369,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGU MK06 66 Standard","GGU","MK06","66","ELECTRIC","Standard","GGU 66","GPU 66","ok","GPU","66","GPU MK06 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.92,1,0.19,0.09,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1370,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGU MK06 66 Standard","GGU","MK06","66","SOLAR","Standard","GGU 66","GPU 66","ok","GPU","66","GPU MK06 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.92,1,0.19,0.09,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1371,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGU MK06 70 Standard","GGU","MK06","70","MANUAL","Standard","GGU 70","GPU 70","ok","GPU","70","GPU MK06 70 Standard","70",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.24,7.0000000000000007E-2,0,0.24,7.0000000000000007E-2,0,0.05,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1376,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGU MK06 70Q Standard","GGU","MK06","70Q","MANUAL","Standard","GGU 70Q","GPU 70","ok","GPU","70","GPU MK06 70 Standard",70,1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.24,7.0000000000000007E-2,0,0.24,7.0000000000000007E-2,0,0.05,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1377,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGU MK06 76F Standard","GGU","MK06","76F","MANUAL","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU MK06 70 Standard","76",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1378,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGU MK06 76F Standard","GGU","MK06","76F","ELECTRIC","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU MK06 70 Standard","76",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1379,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGU MK08 57 Standard","GGU","MK08",57,"MANUAL","Standard","GGU 57","GPU 70","ok","GPU","70","GPU MK08 70 Standard",57,1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1380,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGU MK08 57 Standard","GGU","MK08",57,"ELECTRIC","Standard","GGU 57","GPU 70","ok","GPU","70","GPU MK08 70 Standard",57,1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1381,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGU MK08 57 Standard","GGU","MK08",57,"SOLAR","Standard","GGU 57","GPU 70","ok","GPU","70","GPU MK08 70 Standard",57,1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1382,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGU MK08 62 Standard","GGU","MK08","62","MANUAL","Standard","GGU 62","GPU 62","ok","GPU","62","GPU MK08 62 Standard","62",1.1000000000000001,1.3,1,1.2,0.97,1.1000000000000001,0.94,1.1000000000000001,1.2,1,0.85,0.96,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1383,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGU MK08 62 Standard","GGU","MK08","62","ELECTRIC","Standard","GGU 62","GPU 62","ok","GPU","62","GPU MK08 62 Standard","62",1.1000000000000001,1.3,1,1.2,0.97,1.1000000000000001,0.94,1.1000000000000001,1.2,1,0.85,0.96,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1384,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGU MK08 66 Standard","GGU","MK08","66","MANUAL","Standard","GGU 66","GPU 66","ok","GPU","66","GPU MK08 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.9,0.99,0.2,0.09,0,0.2,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1385,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGU MK08 66 Standard","GGU","MK08","66","ELECTRIC","Standard","GGU 66","GPU 66","ok","GPU","66","GPU MK08 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.9,0.99,0.2,0.09,0,0.2,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1386,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGU MK08 66 Standard","GGU","MK08","66","SOLAR","Standard","GGU 66","GPU 66","ok","GPU","66","GPU MK08 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.9,0.99,0.2,0.09,0,0.2,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1387,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGU MK08 70 Standard","GGU","MK08","70","MANUAL","Standard","GGU 70","GPU 70","ok","GPU","70","GPU MK08 70 Standard","70",1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.25,7.0000000000000007E-2,0,0.25,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1392,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGU MK08 70Q Standard","GGU","MK08","70Q","MANUAL","Standard","GGU 70Q","GPU 70","ok","GPU","70","GPU MK08 70 Standard",70,1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.25,7.0000000000000007E-2,0,0.25,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1393,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGU MK08 76F Standard","GGU","MK08","76F","MANUAL","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU MK08 70 Standard","76",1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1395,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGU MK08 76F Standard","GGU","MK08","76F","ELECTRIC","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU MK08 70 Standard","76",1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1394,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGU MK10 62 Standard","GGU","MK10","62","MANUAL","Standard","GGU 62","GPU 62","ok","GPU","62","GPU MK10 62 Standard","62",1.1000000000000001,1.3,1,1.2,0.96,1.1000000000000001,0.93,1.1000000000000001,1.2,1,0.84,0.95,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1396,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GGU MK10 62 Standard","GGU","MK10","62","ELECTRIC","Standard","GGU 62","GPU 62","ok","GPU","62","GPU MK10 62 Standard","62",1.1000000000000001,1.3,1,1.2,0.96,1.1000000000000001,0.93,1.1000000000000001,1.2,1,0.84,0.95,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1397,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GGU MK10 66 Standard","GGU","MK10","66","MANUAL","Standard","GGU 66","GPU 66","ok","GPU","66","GPU MK10 66 Standard","66",1.2,1.3,1.1000000000000001,1.2,1,1.2,1,1.1000000000000001,1.2,1,0.89,0.98,0.2,0.09,0,0.2,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1398,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GGU MK10 66 Standard","GGU","MK10","66","ELECTRIC","Standard","GGU 66","GPU 66","ok","GPU","66","GPU MK10 66 Standard","66",1.2,1.3,1.1000000000000001,1.2,1,1.2,1,1.1000000000000001,1.2,1,0.89,0.98,0.2,0.09,0,0.2,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1399,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GGU MK10 66 Standard","GGU","MK10","66","SOLAR","Standard","GGU 66","GPU 66","ok","GPU","66","GPU MK10 66 Standard","66",1.2,1.3,1.1000000000000001,1.2,1,1.2,1,1.1000000000000001,1.2,1,0.89,0.98,0.2,0.09,0,0.2,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1400,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GGU MK10 70 Standard","GGU","MK10","70","MANUAL","Standard","GGU 70","GPU 70","ok","GPU","70","GPU MK10 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.2,0.26,7.0000000000000007E-2,0,0.26,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1404,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GGU MK10 70 Standard","GGU","MK10","70","ELECTRIC","Standard","GGU 70","GPU 70","ok","GPU","70","GPU MK10 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.2,0.26,7.0000000000000007E-2,0,0.26,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1405,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GGU PK06 57 Standard","GGU","PK06",57,"MANUAL","Standard","GGU 57","GPU 70","ok","GPU","70","GPU PK06 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1406,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGU PK06 57 Standard","GGU","PK06",57,"ELECTRIC","Standard","GGU 57","GPU 70","ok","GPU","70","GPU PK06 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1407,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGU PK06 57 Standard","GGU","PK06",57,"SOLAR","Standard","GGU 57","GPU 70","ok","GPU","70","GPU PK06 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1408,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGU PK06 62 Standard","GGU","PK06","62","MANUAL","Standard","GGU 62","GPU 62","ok","GPU","62","GPU PK06 62 Standard","62",1,1.2,0.99,1.2,0.93,1.1000000000000001,0.91,1.1000000000000001,1.2,0.99,0.82,0.93,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1409,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGU PK06 62 Standard","GGU","PK06","62","ELECTRIC","Standard","GGU 62","GPU 62","ok","GPU","62","GPU PK06 62 Standard","62",1,1.2,0.99,1.2,0.93,1.1000000000000001,0.91,1.1000000000000001,1.2,0.99,0.82,0.93,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1410,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGU PK06 66 Standard","GGU","PK06","66","MANUAL","Standard","GGU 66","GPU 66","ok","GPU","66","GPU PK06 66 Standard","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.98,1.1000000000000001,1.2,1,0.88,0.98,0.2,0.09,0,0.2,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1411,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGU PK06 66 Standard","GGU","PK06","66","ELECTRIC","Standard","GGU 66","GPU 66","ok","GPU","66","GPU PK06 66 Standard","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.98,1.1000000000000001,1.2,1,0.88,0.98,0.2,0.09,0,0.2,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1412,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGU PK06 66 Standard","GGU","PK06","66","SOLAR","Standard","GGU 66","GPU 66","ok","GPU","66","GPU PK06 66 Standard","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.98,1.1000000000000001,1.2,1,0.88,0.98,0.2,0.09,0,0.2,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1413,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGU PK06 70 Standard","GGU","PK06","70","MANUAL","Standard","GGU 70","GPU 70","ok","GPU","70","GPU PK06 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.26,7.0000000000000007E-2,0,0.26,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1418,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGU PK06 70Q Standard","GGU","PK06","70Q","MANUAL","Standard","GGU 70Q","GPU 70","ok","GPU","70","GPU PK06 70 Standard",70,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.26,7.0000000000000007E-2,0,0.26,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1419,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGU PK06 76F Standard","GGU","PK06","76F","MANUAL","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU PK06 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.15,0.05,0,0.15,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1420,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGU PK08 57 Standard","GGU","PK08",57,"MANUAL","Standard","GGU 57","GPU 70","ok","GPU","70","GPU PK08 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1421,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGU PK08 57 Standard","GGU","PK08",57,"ELECTRIC","Standard","GGU 57","GPU 70","ok","GPU","70","GPU PK08 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1422,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGU PK08 57 Standard","GGU","PK08",57,"SOLAR","Standard","GGU 57","GPU 70","ok","GPU","70","GPU PK08 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1423,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGU PK08 62 Standard","GGU","PK08","62","MANUAL","Standard","GGU 62","GPU 62","ok","GPU","62","GPU PK08 62 Standard","62",1,1.2,0.97,1.1000000000000001,0.92,1.1000000000000001,0.89,1,1.1000000000000001,0.98,0.81,0.93,0.26,0.08,0,0.26,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1424,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGU PK08 62 Standard","GGU","PK08","62","ELECTRIC","Standard","GGU 62","GPU 62","ok","GPU","62","GPU PK08 62 Standard","62",1,1.2,0.97,1.1000000000000001,0.92,1.1000000000000001,0.89,1,1.1000000000000001,0.98,0.81,0.93,0.26,0.08,0,0.26,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1425,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGU PK08 66 Standard","GGU","PK08","66","MANUAL","Standard","GGU 66","GPU 66","ok","GPU","66","GPU PK08 66 Standard","66",1.1000000000000001,1.3,1.1000000000000001,1.2,0.99,1.1000000000000001,0.96,1.1000000000000001,1.2,1,0.86,0.97,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1426,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGU PK08 66 Standard","GGU","PK08","66","ELECTRIC","Standard","GGU 66","GPU 66","ok","GPU","66","GPU PK08 66 Standard","66",1.1000000000000001,1.3,1.1000000000000001,1.2,0.99,1.1000000000000001,0.96,1.1000000000000001,1.2,1,0.86,0.97,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1427,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGU PK08 66 Standard","GGU","PK08","66","SOLAR","Standard","GGU 66","GPU 66","ok","GPU","66","GPU PK08 66 Standard","66",1.1000000000000001,1.3,1.1000000000000001,1.2,0.99,1.1000000000000001,0.96,1.1000000000000001,1.2,1,0.86,0.97,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1428,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGU PK08 70 Standard","GGU","PK08","70","MANUAL","Standard","GGU 70","GPU 70","ok","GPU","70","GPU PK08 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.27,7.0000000000000007E-2,0,0.27,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1432,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGU PK08 70Q Standard","GGU","PK08","70Q","MANUAL","Standard","GGU 70Q","GPU 70","ok","GPU","70","GPU PK08 70 Standard",70,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.27,7.0000000000000007E-2,0,0.27,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1433,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGU PK08 76F Standard","GGU","PK08","76F","MANUAL","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU PK08 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.13,0.05,0,0.13,0.05,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1434,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGU PK10 57 Standard","GGU","PK10",57,"MANUAL","Standard","GGU 57","GPU 70","ok","GPU","70","GPU PK10 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1435,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.71]
["GGU PK10 57 Standard","GGU","PK10",57,"ELECTRIC","Standard","GGU 57","GPU 70","ok","GPU","70","GPU PK10 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1436,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.71]
["GGU PK10 57 Standard","GGU","PK10",57,"SOLAR","Standard","GGU 57","GPU 70","ok","GPU","70","GPU PK10 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1437,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.71]
["GGU PK10 62 Standard","GGU","PK10","62","MANUAL","Standard","GGU 62","GPU 62","ok","GPU","62","GPU PK10 62 Standard","62",1,1.2,0.95,1.1000000000000001,0.9,1.1000000000000001,0.88,1,1.1000000000000001,0.97,0.79,0.92,0.27,0.08,0,0.27,0.09,0,0.05,0.08,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1438,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.71]
["GGU PK10 62 Standard","GGU","PK10","62","ELECTRIC","Standard","GGU 62","GPU 62","ok","GPU","62","GPU PK10 62 Standard","62",1,1.2,0.95,1.1000000000000001,0.9,1.1000000000000001,0.88,1,1.1000000000000001,0.97,0.79,0.92,0.27,0.08,0,0.27,0.09,0,0.05,0.08,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1439,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.71]
["GGU PK10 66 Standard","GGU","PK10","66","MANUAL","Standard","GGU 66","GPU 66","ok","GPU","66","GPU PK10 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.98,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.85,0.96,0.21,0.09,0,0.21,0.1,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1440,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.71]
["GGU PK10 66 Standard","GGU","PK10","66","ELECTRIC","Standard","GGU 66","GPU 66","ok","GPU","66","GPU PK10 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.98,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.85,0.96,0.21,0.09,0,0.21,0.1,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1441,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.71]
["GGU PK10 66 Standard","GGU","PK10","66","SOLAR","Standard","GGU 66","GPU 66","ok","GPU","66","GPU PK10 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.98,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.85,0.96,0.21,0.09,0,0.21,0.1,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1442,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.71]
["GGU PK10 70 Standard","GGU","PK10","70","MANUAL","Standard","GGU 70","GPU 70","ok","GPU","70","GPU PK10 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.27,7.0000000000000007E-2,0,0.27,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1447,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.71]
["GGU PK10 70Q Standard","GGU","PK10","70Q","MANUAL","Standard","GGU 70Q","GPU 70","ok","GPU","70","GPU PK10 70 Standard",70,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.27,7.0000000000000007E-2,0,0.27,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1448,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.71]
["GGU PK10 76F Standard","GGU","PK10","76F","MANUAL","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU PK10 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1449,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.71]
["GGU SK06 57 Standard","GGU","SK06",57,"MANUAL","Standard","GGU 57","GPU 70","ok","GPU","70","GPU SK06 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1450,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGU SK06 57 Standard","GGU","SK06",57,"ELECTRIC","Standard","GGU 57","GPU 70","ok","GPU","70","GPU SK06 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1451,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGU SK06 57 Standard","GGU","SK06",57,"SOLAR","Standard","GGU 57","GPU 70","ok","GPU","70","GPU SK06 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1452,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGU SK06 62 Standard","GGU","SK06","62","MANUAL","Standard","GGU 62","GPU 62","ok","GPU","62","GPU SK06 62 Standard","62",1,1.2,0.95,1.1000000000000001,0.89,1.1000000000000001,0.87,1,1.1000000000000001,0.97,0.79,0.91,0.26,0.08,0,0.26,0.09,0,0.05,0.08,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1453,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGU SK06 62 Standard","GGU","SK06","62","ELECTRIC","Standard","GGU 62","GPU 62","ok","GPU","62","GPU SK06 62 Standard","62",1,1.2,0.95,1.1000000000000001,0.89,1.1000000000000001,0.87,1,1.1000000000000001,0.97,0.79,0.91,0.26,0.08,0,0.26,0.09,0,0.05,0.08,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1454,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGU SK06 66 Standard","GGU","SK06","66","MANUAL","Standard","GGU 66","GPU 66","ok","GPU","66","GPU SK06 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.97,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.85,0.96,0.21,0.09,0,0.21,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1455,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGU SK06 66 Standard","GGU","SK06","66","ELECTRIC","Standard","GGU 66","GPU 66","ok","GPU","66","GPU SK06 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.97,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.85,0.96,0.21,0.09,0,0.21,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1456,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGU SK06 66 Standard","GGU","SK06","66","SOLAR","Standard","GGU 66","GPU 66","ok","GPU","66","GPU SK06 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.97,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.85,0.96,0.21,0.09,0,0.21,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1457,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGU SK06 70 Standard","GGU","SK06","70","MANUAL","Standard","GGU 70","GPU 70","ok","GPU","70","GPU SK06 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.27,7.0000000000000007E-2,0,0.27,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1462,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGU SK06 70Q Standard","GGU","SK06","70Q","MANUAL","Standard","GGU 70Q","GPU 70","ok","GPU","70","GPU SK06 70 Standard",70,1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.27,7.0000000000000007E-2,0,0.27,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1464,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGU SK06 76F Standard","GGU","SK06","76F","MANUAL","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU SK06 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.16,0.05,0,0.16,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.08,0,0.08,0.44,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1465,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGU SK06 76F Standard","GGU","SK06","76F","ELECTRIC","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU SK06 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.16,0.05,0,0.16,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.08,0,0.08,0.44,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1466,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGU SK08 57 Standard","GGU","SK08",57,"MANUAL","Standard","GGU 57","GPU 70","ok","GPU","70","GPU SK08 70 Standard",57,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1467,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGU SK08 57 Standard","GGU","SK08",57,"ELECTRIC","Standard","GGU 57","GPU 70","ok","GPU","70","GPU SK08 70 Standard",57,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1468,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGU SK08 57 Standard","GGU","SK08",57,"SOLAR","Standard","GGU 57","GPU 70","ok","GPU","70","GPU SK08 70 Standard",57,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1469,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGU SK08 62 Standard","GGU","SK08","62","MANUAL","Standard","GGU 62","GPU 62","ok","GPU","62","GPU SK08 62 Standard","62",0.97,1.2,0.92,1.1000000000000001,0.87,1,0.85,1,1.1000000000000001,0.95,0.77,0.9,0.27,0.08,0,0.27,0.09,0,0.05,7.0000000000000007E-2,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.49,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1463,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGU SK08 62 Standard","GGU","SK08","62","ELECTRIC","Standard","GGU 62","GPU 62","ok","GPU","62","GPU SK08 62 Standard","62",0.97,1.2,0.92,1.1000000000000001,0.87,1,0.85,1,1.1000000000000001,0.95,0.77,0.9,0.27,0.08,0,0.27,0.09,0,0.05,7.0000000000000007E-2,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.49,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1470,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGU SK08 66 Standard","GGU","SK08","66","MANUAL","Standard","GGU 66","GPU 66","ok","GPU","66","GPU SK08 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.95,1.1000000000000001,0.92,1.1000000000000001,1.2,1,0.83,0.94,0.22,0.09,0,0.22,0.1,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1471,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGU SK08 66 Standard","GGU","SK08","66","ELECTRIC","Standard","GGU 66","GPU 66","ok","GPU","66","GPU SK08 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.95,1.1000000000000001,0.92,1.1000000000000001,1.2,1,0.83,0.94,0.22,0.09,0,0.22,0.1,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1473,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGU SK08 70 Standard","GGU","SK08","70","MANUAL","Standard","GGU 70","GPU 70","ok","GPU","70","GPU SK08 70 Standard","70",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.28000000000000003,7.0000000000000007E-2,0,0.28000000000000003,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.49,0,0.09,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1477,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGU SK08 70Q Standard","GGU","SK08","70Q","MANUAL","Standard","GGU 70Q","GPU 70","ok","GPU","70","GPU SK08 70 Standard",70,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.28000000000000003,7.0000000000000007E-2,0,0.28000000000000003,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.49,0,0.09,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1472,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGU SK08 76F Standard","GGU","SK08","76F","MANUAL","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU SK08 70 Standard","76",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.15,0.05,0,0.15,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.45,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1480,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGU SK08 76F Standard","GGU","SK08","76F","ELECTRIC","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU SK08 70 Standard","76",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.15,0.05,0,0.15,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.45,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1478,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGU SK10 66 Standard","GGU","SK10","66","MANUAL","Standard","GGU 66","GPU 66","ok","GPU","66","GPU SK10 66 Standard","66",1.1000000000000001,1.2,0.99,1.2,0.93,1.1000000000000001,0.91,1.1000000000000001,1.2,0.99,0.82,0.93,0.22,0.09,0,0.22,0.1,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1479,1.1399999999999999,1.6,1.82,0.96,1.41,4.7300000000000004,1.35,0.47,0.74]
["GGU SK10 66 Standard","GGU","SK10","66","ELECTRIC","Standard","GGU 66","GPU 66","ok","GPU","66","GPU SK10 66 Standard","66",1.1000000000000001,1.2,0.99,1.2,0.93,1.1000000000000001,0.91,1.1000000000000001,1.2,0.99,0.82,0.93,0.22,0.09,0,0.22,0.1,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1481,1.1399999999999999,1.6,1.82,0.96,1.41,4.7300000000000004,1.35,0.47,0.74]
["GGU SK10 66 Standard","GGU","SK10","66","SOLAR","Standard","GGU 66","GPU 66","ok","GPU","66","GPU SK10 66 Standard","66",1.1000000000000001,1.2,0.99,1.2,0.93,1.1000000000000001,0.91,1.1000000000000001,1.2,0.99,0.82,0.93,0.22,0.09,0,0.22,0.1,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1482,1.1399999999999999,1.6,1.82,0.96,1.41,4.7300000000000004,1.35,0.47,0.74]
["GGU UK04 57 Standard","GGU","UK04",57,"MANUAL","Standard","GGU 57","GPU 70","ok","GPU","70","GPU UK04 70 Standard",57,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1486,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGU UK04 57 Standard","GGU","UK04",57,"ELECTRIC","Standard","GGU 57","GPU 70","ok","GPU","70","GPU UK04 70 Standard",57,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1487,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGU UK04 57 Standard","GGU","UK04",57,"SOLAR","Standard","GGU 57","GPU 70","ok","GPU","70","GPU UK04 70 Standard",57,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1488,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGU UK04 66 Standard","GGU","UK04","66","MANUAL","Standard","GGU 66","GPU 66","ok","GPU","66","GPU UK04 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.98,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.85,0.96,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1489,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGU UK04 66 Standard","GGU","UK04","66","ELECTRIC","Standard","GGU 66","GPU 66","ok","GPU","66","GPU UK04 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.98,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.85,0.96,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1490,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGU UK04 66 Standard","GGU","UK04","66","SOLAR","Standard","GGU 66","GPU 66","ok","GPU","66","GPU UK04 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.98,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.85,0.96,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1491,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGU UK04 70 Standard","GGU","UK04","70","MANUAL","Standard","GGU 70","GPU 70","ok","GPU","70","GPU UK04 70 Standard","70",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.26,7.0000000000000007E-2,0,0.26,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1494,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGU UK04 70Q Standard","GGU","UK04","70Q","MANUAL","Standard","GGU 70Q","GPU 70","ok","GPU","70","GPU UK04 70 Standard",70,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.26,7.0000000000000007E-2,0,0.26,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1496,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGU UK04 76F Standard","GGU","UK04","76F","MANUAL","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU UK04 70 Standard","76",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.16,0.05,0,0.16,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.08,0,0.08,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1497,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGU UK04 76F Standard","GGU","UK04","76F","ELECTRIC","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU UK04 70 Standard","76",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.16,0.05,0,0.16,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.08,0,0.08,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1498,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGU UK08 57 Standard","GGU","UK08",57,"MANUAL","Standard","GGU 57","GPU 70","ok","GPU","70","GPU UK08 70 Standard",57,1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.98,1.2,0.16,0.05,0,0.16,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1500,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGU UK08 57 Standard","GGU","UK08",57,"ELECTRIC","Standard","GGU 57","GPU 70","ok","GPU","70","GPU UK08 70 Standard",57,1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.98,1.2,0.16,0.05,0,0.16,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1501,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGU UK08 57 Standard","GGU","UK08",57,"SOLAR","Standard","GGU 57","GPU 70","ok","GPU","70","GPU UK08 70 Standard",57,1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.98,1.2,0.16,0.05,0,0.16,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1502,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGU UK08 66 Standard","GGU","UK08","66","MANUAL","Standard","GGU 66","GPU 66","ok","GPU","66","GPU UK08 66 Standard","66",1,1.2,0.97,1.2,0.92,1.1000000000000001,0.9,1,1.2,0.98,0.81,0.93,0.22,0.09,0,0.22,0.1,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1503,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGU UK08 66 Standard","GGU","UK08","66","ELECTRIC","Standard","GGU 66","GPU 66","ok","GPU","66","GPU UK08 66 Standard","66",1,1.2,0.97,1.2,0.92,1.1000000000000001,0.9,1,1.2,0.98,0.81,0.93,0.22,0.09,0,0.22,0.1,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1504,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGU UK08 66 Standard","GGU","UK08","66","SOLAR","Standard","GGU 66","GPU 66","ok","GPU","66","GPU UK08 66 Standard","66",1,1.2,0.97,1.2,0.92,1.1000000000000001,0.9,1,1.2,0.98,0.81,0.93,0.22,0.09,0,0.22,0.1,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1505,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGU UK08 70 Standard","GGU","UK08","70","MANUAL","Standard","GGU 70","GPU 70","ok","GPU","70","GPU UK08 70 Standard","70",1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.98,1.2,0.28000000000000003,7.0000000000000007E-2,0,0.28000000000000003,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.51,0,0.09,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1509,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGU UK08 70Q Standard","GGU","UK08","70Q","MANUAL","Standard","GGU 70Q","GPU 70","ok","GPU","70","GPU UK08 70 Standard",70,1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.98,1.2,0.28000000000000003,7.0000000000000007E-2,0,0.28000000000000003,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.51,0,0.09,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1510,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGU UK08 76F Standard","GGU","UK08","76F","MANUAL","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU UK08 70 Standard","76",1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.98,1.2,0.11,0.05,0,0.11,0.05,0,0.02,0.1,0,0.12,0,0.08,0,0.08,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1511,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGU UK08 76F Standard","GGU","UK08","76F","ELECTRIC","Standard","GGU 76F","GPU 70","ok","GPU","70","GPU UK08 70 Standard","76",1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.98,1.2,0.11,0.05,0,0.11,0.05,0,0.02,0.1,0,0.12,0,0.08,0,0.08,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",1512,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGU UK10 66 Standard","GGU","UK10","66","MANUAL","Standard","GGU 66","GPU 66","ok","GPU","66","GPU UK10 66 Standard","66",1,1.2,0.95,1.1000000000000001,0.9,1.1000000000000001,0.88,1,1.1000000000000001,0.97,0.8,0.92,0.23,0.09,0,0.23,0.1,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1513,1.34,1.6,2.14,1.1600000000000001,1.41,5.13,1.63,0.51000000000000023,0.76]
["GGU UK10 66 Standard","GGU","UK10","66","ELECTRIC","Standard","GGU 66","GPU 66","ok","GPU","66","GPU UK10 66 Standard","66",1,1.2,0.95,1.1000000000000001,0.9,1.1000000000000001,0.88,1,1.1000000000000001,0.97,0.8,0.92,0.23,0.09,0,0.23,0.1,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1514,1.34,1.6,2.14,1.1600000000000001,1.41,5.13,1.63,0.51000000000000023,0.76]
["GGU UK10 66 Standard","GGU","UK10","66","SOLAR","Standard","GGU 66","GPU 66","ok","GPU","66","GPU UK10 66 Standard","66",1,1.2,0.95,1.1000000000000001,0.9,1.1000000000000001,0.88,1,1.1000000000000001,0.97,0.8,0.92,0.23,0.09,0,0.23,0.1,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1508,1.34,1.6,2.14,1.1600000000000001,1.41,5.13,1.63,0.51000000000000023,0.76]
["GIL MK34 57 Standard","GIL","MK34","57","FIXED","Standard","GIL 57","GPL 70","ok","GPL","70","GPL MK34 70 Standard","57",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.13,0.05,0,0.13,0.06,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1517,0.78,0.92,0.72,0.60000000000000009,0.73,2.65,0.44,0.27999999999999997,0.61]
["GIL MK34 62 Standard","GIL","MK34","62","FIXED","Standard","GIL 62","VFE 62","ok","VFE","62","VFE MK34 62 Standard","62",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.91,1,0.22,0.08,0,0.22,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1515,0.78,0.92,0.72,0.60000000000000009,0.73,2.65,0.44,0.27999999999999997,0.61]
["GIL MK34 66 Standard","GIL","MK34","66","FIXED","Standard","GIL 66","GPL 66","ok","GPL","66","GPL MK34 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.92,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1516,0.78,0.92,0.72,0.60000000000000009,0.73,2.65,0.44,0.27999999999999997,0.61]
["GIL MK34 70 Standard","GIL","MK34","70","FIXED","Standard","GIL 70","GPL 70","ok","GPL","70","GPL MK34 70 Standard","70",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.23,0.06,0,0.23,0.06,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1519,0.78,0.92,0.72,0.60000000000000009,0.73,2.65,0.44,0.27999999999999997,0.61]
["GIL PK34 57 Standard","GIL","PK34","57","FIXED","Standard","GIL 57","GPL 70","ok","GPL","70","GPL PK34 70 Standard","57",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.13,0.05,0,0.13,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1520,0.94199999999999995,0.92,0.87,0.76200000000000001,0.73,2.98,0.56000000000000005,0.30999999999999994,0.64]
["GIL PK34 62 Standard","GIL","PK34","62","FIXED","Standard","GIL 62","VFE 62","ok","VFE","62","VFE PK34 62 Standard","62",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.97,1.1000000000000001,1.2,1,0.87,0.97,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1521,0.94199999999999995,0.92,0.87,0.76200000000000001,0.73,2.98,0.56000000000000005,0.30999999999999994,0.64]
["GIL PK34 66 Standard","GIL","PK34","66","FIXED","Standard","GIL 66","GPL 66","ok","GPL","66","GPL PK34 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1,1.2,0.99,1.1000000000000001,1.3,1.1000000000000001,0.89,0.99,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1522,0.94199999999999995,0.92,0.87,0.76200000000000001,0.73,2.98,0.56000000000000005,0.30999999999999994,0.64]
["GIL PK34 70 Standard","GIL","PK34","70","FIXED","Standard","GIL 70","GPL 70","ok","GPL","70","GPL PK34 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.24,0.06,0,0.24,0.06,0,0.04,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1523,0.94199999999999995,0.92,0.87,0.76200000000000001,0.73,2.98,0.56000000000000005,0.30999999999999994,0.64]
["GIL SK34 57 Standard","GIL","SK34","57","FIXED","Standard","GIL 57","GPL 70","ok","GPL","70","GPL SK34 70 Standard","57",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1524,1.1399999999999999,0.92,1.05,0.96,0.73,3.37,0.7,0.35000000000000009,0.67]
["GIL SK34 62 Standard","GIL","SK34","62","FIXED","Standard","GIL 62","VFE 62","ok","VFE","62","VFE SK34 62 Standard","62",1.1000000000000001,1.3,1,1.2,0.97,1.1000000000000001,0.94,1.1000000000000001,1.2,1,0.84,0.95,0.24,0.08,0,0.24,0.08,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1518,1.1399999999999999,0.92,1.05,0.96,0.73,3.37,0.7,0.35000000000000009,0.67]
["GIL SK34 66 Standard","GIL","SK34","66","FIXED","Standard","GIL 66","GPL 66","ok","GPL","66","GPL SK34 66 Standard","66",1.1000000000000001,1.3,1.1000000000000001,1.2,0.99,1.1000000000000001,0.96,1.1000000000000001,1.2,1,0.86,0.98,0.2,0.08,0,0.2,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1527,1.1399999999999999,0.92,1.05,0.96,0.73,3.37,0.7,0.35000000000000009,0.67]
["GIL SK34 70 Standard","GIL","SK34","70","FIXED","Standard","GIL 70","GPL 70","ok","GPL","70","GPL SK34 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.25,0.06,0,0.25,0.06,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1525,1.1399999999999999,0.92,1.05,0.96,0.73,3.37,0.7,0.35000000000000009,0.67]
["GIL UK34 57 Standard","GIL","UK34","57","FIXED","Standard","GIL 57","GPL 70","ok","GPL","70","GPL UK34 70 Standard","57",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1526,1.34,0.92,1.23,1.1600000000000001,0.73,3.77,0.84,0.39,0.68]
["GIL UK34 66 Standard","GIL","UK34","66","FIXED","Standard","GIL 66","GPL 66","ok","GPL","66","GPL UK34 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.97,1.1000000000000001,0.94,1.1000000000000001,1.2,1,0.85,0.96,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1528,1.34,0.92,1.23,1.1600000000000001,0.73,3.77,0.84,0.39,0.68]
["GIL UK34 70 Standard","GIL","UK34","70","FIXED","Standard","GIL 70","GPL 70","ok","GPL","70","GPL UK34 70 Standard","70",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.26,0.06,0,0.26,0.06,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1529,1.34,0.92,1.23,1.1600000000000001,0.73,3.77,0.84,0.39,0.68]
["GIU FK34 62 Standard","GIU","FK34","62","FIXED","Standard","GIU 62","GIU 62","ok","GIU","62","GIU FK34 62 Standard","62",1.2,1.3,1.1000000000000001,1.2,1,1.2,1,1.1000000000000001,1.2,1,0.89,0.99,0.21,0.08,0,0.21,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1530,0.66,0.92,0.61,0.48000000000000004,0.73,2.41,0.35,0.26,0.56999999999999995]
["GIU FK34 66 Standard","GIU","FK34","66","FIXED","Standard","GIU 66","GPU 66","ok","GPU","66","GPU FK34 66 Standard","66",1.3,1.5,1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.98,1.1000000000000001,0.17,0.08,0,0.17,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1533,0.66,0.92,0.61,0.48000000000000004,0.73,2.41,0.35,0.26,0.56999999999999995]
["GIU MK34 57 Standard","GIU","MK34","57","FIXED","Standard","GIU 57","GPU 70","ok","GPU","70","GPU MK34 70 Standard","57",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.13,0.05,0,0.13,7.0000000000000007E-2,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1531,0.78,0.92,0.72,0.60000000000000009,0.73,2.65,0.44,0.27999999999999997,0.61]
["GIU MK34 62 Standard","GIU","MK34","62","FIXED","Standard","GIU 62","GIU 62","ok","GIU","62","GIU MK34 62 Standard","62",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.91,1,0.23,0.08,0,0.23,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1532,0.78,0.92,0.72,0.60000000000000009,0.73,2.65,0.44,0.27999999999999997,0.61]
["GIU MK34 66 Standard","GIU","MK34","66","FIXED","Standard","GIU 66","GPU 66","ok","GPU","66","GPU MK34 66 Standard","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.94,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1534,0.78,0.92,0.72,0.60000000000000009,0.73,2.65,0.44,0.27999999999999997,0.61]
["GIU PK34 57 Standard","GIU","PK34","57","FIXED","Standard","GIU 57","GPU 70","ok","GPU","70","GPU PK34 70 Standard","57",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.13,0.05,0,0.13,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1535,0.94199999999999995,0.92,0.87,0.76200000000000001,0.73,2.97,0.55000000000000004,0.31999999999999995,0.63]
["GIU PK34 62 Standard","GIU","PK34","62","FIXED","Standard","GIU 62","GIU 62","ok","GIU","62","GIU PK34 62 Standard","62",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,0.98,1.1000000000000001,1.2,1,0.88,0.98,0.24,0.08,0,0.24,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1536,0.94199999999999995,0.92,0.87,0.76200000000000001,0.73,2.97,0.55000000000000004,0.31999999999999995,0.63]
["GIU PK34 66 Standard","GIU","PK34","66","FIXED","Standard","GIU 66","GPU 66","ok","GPU","66","GPU PK34 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.9,0.99,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1538,0.94199999999999995,0.92,0.87,0.76200000000000001,0.73,2.97,0.55000000000000004,0.31999999999999995,0.63]
["GIU SK34 57 Standard","GIU","SK34","57","FIXED","Standard","GIU 57","GPU 70","ok","GPU","70","GPU SK34 70 Standard","57",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1537,1.1399999999999999,0.92,1.05,0.96,0.73,3.37,0.7,0.35000000000000009,0.67]
["GIU SK34 62 Standard","GIU","SK34","62","FIXED","Standard","GIU 62","GIU 62","ok","GIU","62","GIU SK34 62 Standard","62",1.1000000000000001,1.3,1,1.2,0.97,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.85,0.96,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1539,1.1399999999999999,0.92,1.05,0.96,0.73,3.37,0.7,0.35000000000000009,0.67]
["GIU SK34 66 Standard","GIU","SK34","66","FIXED","Standard","GIU 66","GPU 66","ok","GPU","66","GPU SK34 66 Standard","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.98,1.1000000000000001,1.2,1,0.88,0.98,0.2,0.09,0,0.2,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1540,1.1399999999999999,0.92,1.05,0.96,0.73,3.37,0.7,0.35000000000000009,0.67]
["GIU SK34 70 Standard","GIU","SK34","70","FIXED","Standard","GIU 70","GPU 70","ok","GPU","70","GPU SK34 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.25,7.0000000000000007E-2,0,0.25,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1541,1.1399999999999999,0.92,1.05,0.96,0.73,3.37,0.7,0.35000000000000009,0.67]
["GIU UK34 57 Standard","GIU","UK34","57","FIXED","Standard","GIU 57","GPU 70","ok","GPU","70","GPU UK34 70 Standard","57",1.4,1.8,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1542,1.34,0.92,1.23,1.1600000000000001,0.73,3.77,0.84,0.39,0.68]
["GIU UK34 66 Standard","GIU","UK34","66","FIXED","Standard","GIU 66","GPU 66","ok","GPU","66","GPU UK34 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.99,1.1000000000000001,0.96,1.1000000000000001,1.2,1,0.86,0.96,0.2,0.09,0,0.2,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1543,1.34,0.92,1.23,1.1600000000000001,0.73,3.77,0.84,0.39,0.68]
["GPL CK04 57 Standard","GPL","CK04",57,"MANUAL","Standard","GPL 57","GPL 70","ok","GPL","70","GPL CK04 70 Standard",57,1.6,1.9,1.4,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.06,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.33,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1544,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GPL CK04 66 Standard","GPL","CK04","66","MANUAL","Standard","GPL 66","GPL 66","ok","GPL","66","GPL CK04 66 Standard","66",1.3,1.5,1.2,1.4,1.2,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.99,1.1000000000000001,0.16,0.08,0,0.16,0.08,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1545,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GPL CK04 76F Standard","GPL","CK04","76F","MANUAL","Standard","GPL 76F","GPL 70","ok","GPL","70","GPL CK04 70 Standard","76",1.6,1.9,1.4,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.05,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.34,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1547,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GPL CK04 70 Standard","GPL","CK04","70","MANUAL","Standard","GPL 70","GPL 70","ok","GPL","70","GPL CK04 70 Standard","70",1.6,1.9,1.4,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.21,0.06,0,0.21,0.06,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1548,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GPL CK06 66 Standard","GPL","CK06","66","MANUAL","Standard","GPL 66","GPL 66","ok","GPL","66","GPL CK06 66 Standard","66",1.3,1.5,1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.97,1.1000000000000001,0.17,0.08,0,0.17,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1549,0.55000000000000004,1.18,0.65,0.37000000000000005,0.98,2.71,0.37,0.28000000000000003,0.56999999999999995]
["GPL FK06 66 Standard","GPL","FK06","66","MANUAL","Standard","GPL 66","GPL 66","ok","GPL","66","GPL FK06 66 Standard","66",1.2,1.4,1.2,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.93,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1551,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GPL FK06 76F Standard","GPL","FK06","76F","MANUAL","Standard","GPL 76F","GPL 70","ok","GPL","70","GPL FK06 70 Standard","76",1.5,1.9,1.4,1.7,1.3,1.6,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.13,0.05,0,0.13,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1553,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GPL FK08 66 Standard","GPL","FK08","66","MANUAL","Standard","GPL 66","GPL 66","ok","GPL","66","GPL FK08 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.92,1,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1554,0.66,1.4,0.92,0.48000000000000004,1.2,3.37,0.57999999999999996,0.34000000000000008,0.63]
["GPL MK04 57 Standard","GPL","MK04",57,"MANUAL","Standard","GPL 57","GPL 70","ok","GPL","70","GPL MK04 70 Standard",57,1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.13,0.05,0,0.13,0.06,0,0.02,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1555,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GPL MK04 66 Standard","GPL","MK04","66","MANUAL","Standard","GPL 66","GPL 66","ok","GPL","66","GPL MK04 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.92,1,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1556,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GPL MK04 76F Standard","GPL","MK04","76F","MANUAL","Standard","GPL 76F","GPL 70","ok","GPL","70","GPL MK04 70 Standard","76",1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1559,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GPL MK04 70 Standard","GPL","MK04","70","MANUAL","Standard","GPL 70","GPL 70","ok","GPL","70","GPL MK04 70 Standard","70",1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.24,0.06,0,0.24,0.06,0,0.04,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1560,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GPL MK06 57 Standard","GPL","MK06",57,"MANUAL","Standard","GPL 57","GPL 70","ok","GPL","70","GPL MK06 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1561,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GPL MK06 66 Standard","GPL","MK06","66","MANUAL","Standard","GPL 66","GPL 66","ok","GPL","66","GPL MK06 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.9,1,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1562,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GPL MK06 76F Standard","GPL","MK06","76F","MANUAL","Standard","GPL 76F","GPL 70","ok","GPL","70","GPL MK06 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1564,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GPL MK06 70 Standard","GPL","MK06","70","MANUAL","Standard","GPL 70","GPL 70","ok","GPL","70","GPL MK06 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.24,0.06,0,0.24,0.06,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1565,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GPL MK08 57 Standard","GPL","MK08",57,"MANUAL","Standard","GPL 57","GPL 70","ok","GPL","70","GPL MK08 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1566,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GPL MK08 66 Standard","GPL","MK08","66","MANUAL","Standard","GPL 66","GPL 66","ok","GPL","66","GPL MK08 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1,1.2,0.99,1.1000000000000001,1.3,1.1000000000000001,0.88,0.99,0.2,0.09,0,0.2,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1567,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GPL MK08 76F Standard","GPL","MK08","76F","MANUAL","Standard","GPL 76F","GPL 70","ok","GPL","70","GPL MK08 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1569,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GPL MK08 70 Standard","GPL","MK08","70","MANUAL","Standard","GPL 70","GPL 70","ok","GPL","70","GPL MK08 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.25,7.0000000000000007E-2,0,0.25,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1570,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GPL MK10 66 Standard","GPL","MK10","66","MANUAL","Standard","GPL 66","GPL 66","ok","GPL","66","GPL MK10 66 Standard","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,0.97,1.1000000000000001,1.2,1,0.87,0.98,0.2,0.09,0,0.2,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1571,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GPL MK10 70 Standard","GPL","MK10","70","MANUAL","Standard","GPL 70","GPL 70","ok","GPL","70","GPL MK10 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.2,0.26,7.0000000000000007E-2,0,0.26,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1573,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GPL PK04 66 Standard","GPL","PK04","66","MANUAL","Standard","GPL 66","GPL 66","ok","GPL","66","GPL PK04 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1,1.2,0.99,1.1000000000000001,1.3,1.1000000000000001,0.88,0.99,0.2,0.08,0,0.2,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1574,0.94199999999999995,0.98,0.92,0.76200000000000001,0.78,3.09,0.6,0.32000000000000006,0.65]
["GPL PK06 57 Standard","GPL","PK06",57,"MANUAL","Standard","GPL 57","GPL 70","ok","GPL","70","GPL PK06 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1577,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GPL PK06 66 Standard","GPL","PK06","66","MANUAL","Standard","GPL 66","GPL 66","ok","GPL","66","GPL PK06 66 Standard","66",1.1000000000000001,1.3,1.1000000000000001,1.2,0.99,1.1000000000000001,0.96,1.1000000000000001,1.2,1,0.86,0.98,0.2,0.09,0,0.2,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1578,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GPL PK06 76F Standard","GPL","PK06","76F","MANUAL","Standard","GPL 76F","GPL 70","ok","GPL","70","GPL PK06 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.15,0.05,0,0.15,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.08,0,0.08,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1580,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GPL PK08 57 Standard","GPL","PK08",57,"MANUAL","Standard","GPL 57","GPL 70","ok","GPL","70","GPL PK08 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.5,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1581,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GPL PK08 66 Standard","GPL","PK08","66","MANUAL","Standard","GPL 66","GPL 66","ok","GPL","66","GPL PK08 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.97,1.1000000000000001,0.94,1.1000000000000001,1.2,1,0.85,0.97,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1582,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GPL PK10 57 Standard","GPL","PK10",57,"MANUAL","Standard","GPL 57","GPL 70","ok","GPL","70","GPL PK10 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.5,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1583,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.71]
["GPL PK10 66 Standard","GPL","PK10","66","MANUAL","Standard","GPL 66","GPL 66","ok","GPL","66","GPL PK10 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.95,1.1000000000000001,0.93,1.1000000000000001,1.2,1,0.83,0.96,0.21,0.09,0,0.21,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1584,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.71]
["GPL PK10 76F Standard","GPL","PK10","76F","MANUAL","Standard","GPL 76F","GPL 70","ok","GPL","70","GPL PK10 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1587,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.71]
["GPL SK06 57 Standard","GPL","SK06",57,"MANUAL","Standard","GPL 57","GPL 70","ok","GPL","70","GPL SK06 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.99,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1588,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GPL SK06 66 Standard","GPL","SK06","66","MANUAL","Standard","GPL 66","GPL 66","ok","GPL","66","GPL SK06 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.95,1.1000000000000001,0.93,1.1000000000000001,1.2,1,0.83,0.96,0.21,0.09,0,0.21,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1589,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GPL SK06 76F Standard","GPL","SK06","76F","MANUAL","Standard","GPL 76F","GPL 70","ok","GPL","70","GPL SK06 70 Standard","76",1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.99,1.2,0.16,0.05,0,0.16,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1585,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GPL SK06 70 Standard","GPL","SK06","70","MANUAL","Standard","GPL 70","GPL 70","ok","GPL","70","GPL SK06 70 Standard","70",1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.99,1.2,0.27,7.0000000000000007E-2,0,0.27,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1591,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GPL SK08 57 Standard","GPL","SK08",57,"MANUAL","Standard","GPL 57","GPL 70","ok","GPL","70","GPL SK08 70 Standard",57,1.3,1.8,1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.98,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.45,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1592,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GPL SK08 66 Standard","GPL","SK08","66","MANUAL","Standard","GPL 66","GPL 66","ok","GPL","66","GPL SK08 66 Standard","66",1,1.3,0.98,1.2,0.93,1.1000000000000001,0.9,1.1000000000000001,1.2,1,0.82,0.94,0.22,0.09,0,0.22,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1593,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GPL SK08 76F Standard","GPL","SK08","76F","MANUAL","Standard","GPL 76F","GPL 70","ok","GPL","70","GPL SK08 70 Standard","76",1.3,1.8,1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.98,1.2,0.15,0.05,0,0.15,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.45,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1595,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GPL SK10 66 Standard","GPL","SK10","66","MANUAL","Standard","GPL 66","GPL 66","ok","GPL","66","GPL SK10 66 Standard","66",1,1.2,0.97,1.2,0.91,1.1000000000000001,0.89,1.1000000000000001,1.2,0.99,0.8,0.93,0.22,0.09,0,0.22,0.1,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1596,1.1399999999999999,1.6,1.82,0.96,1.41,4.7300000000000004,1.35,0.47,0.74]
["GPL UK04 57 Standard","GPL","UK04",57,"MANUAL","Standard","GPL 57","GPL 70","ok","GPL","70","GPL UK04 70 Standard",57,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1599,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GPL UK04 66 Standard","GPL","UK04","66","MANUAL","Standard","GPL 66","GPL 66","ok","GPL","66","GPL UK04 66 Standard","66",1.1000000000000001,1.3,1,1.2,0.96,1.1000000000000001,0.93,1.1000000000000001,1.2,1,0.84,0.96,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1600,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GPL UK04 76F Standard","GPL","UK04","76F","MANUAL","Standard","GPL 76F","GPL 70","ok","GPL","70","GPL UK04 70 Standard","76",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.16,0.05,0,0.16,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1602,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GPL UK04 70 Standard","GPL","UK04","70","MANUAL","Standard","GPL 70","GPL 70","ok","GPL","70","GPL UK04 70 Standard","70",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.26,7.0000000000000007E-2,0,0.26,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1598,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GPL UK08 57 Standard","GPL","UK08","57","MANUAL","Standard","GPL 57","GPL 70","ok","GPL","70","GPL UK08 70 Standard","57",1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.97,1.2,0.16,0.05,0,0.16,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1605,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GPL UK08 66 Standard","GPL","UK08","66","MANUAL","Standard","GPL 66","GPL 66","ok","GPL","66","GPL UK08 66 Standard","66",1,1.2,0.95,1.2,0.9,1.1000000000000001,0.88,1,1.2,0.98,0.79,0.93,0.22,0.09,0,0.22,0.1,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1603,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GPL UK08 76F Standard","GPL","UK08","76F","MANUAL","Standard","GPL 76F","GPL 70","ok","GPL","70","GPL UK08 70 Standard","76",1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.97,1.2,0.11,0.05,0,0.11,0.05,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1607,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GPL UK08 70 Standard","GPL","UK08","70","MANUAL","Standard","GPL 70","GPL 70","ok","GPL","70","GPL UK08 70 Standard","70",1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.97,1.2,0.28000000000000003,7.0000000000000007E-2,0,0.28000000000000003,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.51,0,0.09,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1608,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GPL UK08 57 Standard","GPL","UK08",57,"MANUAL","Standard","GPL 57","GPL 70","ok","GPL","70","GPL UK08 70 Standard",57,1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.97,1.2,0.16,0.05,0,0.16,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",1609,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGLS FFKF06 66 Flush","GGLS","FFKF06","66","MANUAL","Flush","GGLS 66","GGLS 66 3in1","ok","GGLS",66,"GGLS FFKF06 66 Flush","66",1,1.2,0.96,1.1000000000000001,0.91,1.1000000000000001,0.88,1,0.84,0.98,0.8,0.92,0.21,7.0000000000000007E-2,0,0.21,0.09,0,0.03,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.88,1.18,2.21,1.444,0.98,8.7899999999999991,1.42,0.79,0.64]
["GGLS FFKF06 66 Flush","GGLS","FFKF06","66","SOLAR","Flush","GGLS 66","GGLS 66 3in1","ok","GGLS",66,"GGLS FFKF06 66 Flush","66",1,1.2,0.96,1.1000000000000001,0.91,1.1000000000000001,0.88,1,0.84,0.98,0.8,0.92,0.21,7.0000000000000007E-2,0,0.21,0.09,0,0.03,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.88,1.18,2.21,1.444,0.98,8.7899999999999991,1.42,0.79,0.64]
["GPLS FFKF06 66 Flush","GPLS","FFKF06","66","MANUAL","Flush","GPLS 66","GPLS 66 3in1","ok","GPLS",66,"GPLS FFKF06 66 Flush","66",1.1000000000000001,1.3,1,1.2,0.95,1.1000000000000001,0.92,1.1000000000000001,0.87,1,0.83,0.95,0.21,7.0000000000000007E-2,0,0.21,0.09,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.88,1.18,2.21,1.444,0.98,8.7899999999999991,1.42,0.79,0.64]
["GGLS FFKF06 66 Flush + BDX","GGLS","FFKF06","66","MANUAL","Flush + BDX","GGLS 66","GGLS 66 3in1","ok","GGLS",66,"GGLS FFKF06 66 Flush + BDX","66",0.97,1.2,0.92,1.1000000000000001,0.87,1,0.85,1,0.81,0.94,0.77,0.89,0.2,7.0000000000000007E-2,0,0.2,0.08,0,0.03,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.9419999999999999,1.28,2.4900000000000002,1.444,0.98,8.7899999999999991,1.42,0.79,0.56999999999999995]
["GGLS FFKF06 66 Flush + BDX","GGLS","FFKF06","66","SOLAR","Flush + BDX","GGLS 66","GGLS 66 3in1","ok","GGLS",66,"GGLS FFKF06 66 Flush + BDX","66",0.97,1.2,0.92,1.1000000000000001,0.87,1,0.85,1,0.81,0.94,0.77,0.89,0.2,7.0000000000000007E-2,0,0.2,0.08,0,0.03,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.9419999999999999,1.28,2.4900000000000002,1.444,0.98,8.7899999999999991,1.42,0.79,0.56999999999999995]
["GPLS FFKF06 66 Flush + BDX","GPLS","FFKF06","66","MANUAL","Flush + BDX","GPLS 66","GPLS 66 3in1","ok","GPLS",66,"GPLS FFKF06 66 Flush + BDX","66",1,1.2,0.97,1.1000000000000001,0.91,1.1000000000000001,0.89,1,0.84,0.97,0.8,0.92,0.2,7.0000000000000007E-2,0,0.2,0.09,0,0.03,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.9419999999999999,1.28,2.4900000000000002,1.444,0.98,8.7899999999999991,1.42,0.79,0.56999999999999995]
["GPLS FFKF08 66 Standard","GPLS","FFKF08","66","MANUAL","Standard","GPLS 66","GPLS 66 3in1","ok","GPLS",66,"GPLS FFKF08 66 Standard","66",1.3,1.3,1.2,1.2,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.2,1,0.96,0.96,0.22,0.09,0,0.22,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1620,1.88,1.4,2.63,1.444,1.2,10.11,1.74,0.8899999999999999,0.66]
["GGLS FFKF08 66 Standard + BDX","GGLS","FFKF08","66","MANUAL","Standard + BDX","GGLS 66","GGLS 66 3in1","ok","GGLS",66,"GGLS FFKF08 66 Standard + BDX","66",1.1000000000000001,1.3,1,1.2,0.97,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.85,0.97,0.2,0.08,0,0.2,0.09,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",166,1.9419999999999999,1.5,2.91,1.444,1.2,10.11,1.74,0.8899999999999999,0.6]
["GGLS FFKF08 66 Standard + BDX","GGLS","FFKF08","66","SOLAR","Standard + BDX","GGLS 66","GGLS 66 3in1","ok","GGLS",66,"GGLS FFKF08 66 Standard + BDX","66",1.1000000000000001,1.3,1,1.2,0.97,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.85,0.97,0.2,0.08,0,0.2,0.09,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",167,1.9419999999999999,1.5,2.91,1.444,1.2,10.11,1.74,0.8899999999999999,0.6]
["GPLS FFKF08 66 Standard + BDX","GPLS","FFKF08","66","MANUAL","Standard + BDX","GPLS 66","GPLS 66 3in1","ok","GPLS",66,"GPLS FFKF08 66 Standard + BDX","66",1.2,1.4,1.1000000000000001,1.3,1,1.2,0.98,1.1000000000000001,1.3,1.1000000000000001,0.88,1,0.2,0.08,0,0.2,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.9419999999999999,1.5,2.91,1.444,1.2,10.11,1.74,0.8899999999999999,0.6]
["GGLS FFKF08 66 Flush","GGLS","FFKF08","66","MANUAL","Flush","GGLS 66","GGLS 66 3in1","ok","GGLS",66,"GGLS FFKF08 66 Flush","66",1,1.2,0.94,1.1000000000000001,0.89,1.1000000000000001,0.87,1,1.1000000000000001,0.97,0.79,0.92,0.22,0.08,0,0.22,0.09,0,0.04,0.08,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.88,1.4,2.63,1.444,1.2,10.11,1.74,0.8899999999999999,0.66]
["GGLS FFKF08 66 Flush","GGLS","FFKF08","66","SOLAR","Flush","GGLS 66","GGLS 66 3in1","ok","GGLS",66,"GGLS FFKF08 66 Flush","66",1,1.2,0.94,1.1000000000000001,0.89,1.1000000000000001,0.87,1,1.1000000000000001,0.97,0.79,0.92,0.22,0.08,0,0.22,0.09,0,0.04,0.08,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.88,1.4,2.63,1.444,1.2,10.11,1.74,0.8899999999999999,0.66]
["GPLS FFKF08 66 Flush","GPLS","FFKF08","66","MANUAL","Flush","GPLS 66","GPLS 66 3in1","ok","GPLS",66,"GPLS FFKF08 66 Flush","66",1,1.3,0.99,1.2,0.93,1.1000000000000001,0.91,1.1000000000000001,1.2,1,0.82,0.94,0.22,0.09,0,0.22,0.09,0,0.04,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.88,1.4,2.63,1.444,1.2,10.11,1.74,0.8899999999999999,0.66]
["GGLS FFKF08 66 Flush + BDX","GGLS","FFKF08","66","MANUAL","Flush + BDX","GGLS 66","GGLS 66 3in1","ok","GGLS",66,"GGLS FFKF08 66 Flush + BDX","66",0.99,1.2,0.93,1.1000000000000001,0.88,1,0.86,1,1.1000000000000001,0.96,0.78,0.91,0.2,0.08,0,0.2,0.09,0,0.03,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.9419999999999999,1.5,2.91,1.444,1.2,10.11,1.74,0.8899999999999999,0.6]
["GGLS FFKF08 66 Flush + BDX","GGLS","FFKF08","66","SOLAR","Flush + BDX","GGLS 66","GGLS 66 3in1","ok","GGLS",66,"GGLS FFKF08 66 Flush + BDX","66",0.99,1.2,0.93,1.1000000000000001,0.88,1,0.86,1,1.1000000000000001,0.96,0.78,0.91,0.2,0.08,0,0.2,0.09,0,0.03,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.9419999999999999,1.5,2.91,1.444,1.2,10.11,1.74,0.8899999999999999,0.6]
["GGLS FFKF08 66 Standard","GGLS","FFKF08","66","SOLAR","Standard","GGLS 66","GGLS 66 3in1","ok","GGLS",66,"GGLS FFKF08 66 Standard","66",1,1.3,0.98,1.2,0.93,1.1000000000000001,0.9,1.1000000000000001,1.2,1,0.81,0.94,0.22,0.09,0,0.22,0.09,0,0.04,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1244,1.88,1.4,2.63,1.444,1.2,10.11,1.74,0.8899999999999999,0.66]
["GGLS FFKF06 57 Flush","GGLS","FFKF06",57,"MANUAL","Flush","GGLS 57","GGLS 70 3in1","ok","GGLS",70,"GGLS FFKF06 70 Flush",57,1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,0.97,1.2,0.15,0.03,0,0.15,0.06,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.88,1.18,2.21,1.444,0.98,8.7899999999999991,1.42,0.79,0.64]
["GGLS FFKF06 57 Flush","GGLS","FFKF06",57,"SOLAR","Flush","GGLS 57","GGLS 70 3in1","ok","GGLS",70,"GGLS FFKF06 70 Flush",57,1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,0.97,1.2,0.15,0.03,0,0.15,0.06,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.88,1.18,2.21,1.444,0.98,8.7899999999999991,1.42,0.79,0.64]
["GGLS FFKF06 70 Flush + BDX","GGLS","FFKF06","70","SOLAR","Flush + BDX","GGLS 70","GGLS 70 3in1","ok","GGLS",70,"GGLS FFKF06 70 Flush + BDX","70",1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,0.98,1.2,0.93,1.2,0.24,0.04,0,0.24,0.06,0,0.04,0.08,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.9419999999999999,1.28,2.4900000000000002,1.444,0.98,8.7899999999999991,1.42,0.79,0.56999999999999995]
["GPU CK04 66 Standard","GPU","CK04","66","MANUAL","Standard","GPU 66","GPU 66","ok","GPU","66","GPU CK04 66 Standard","66",1.4,1.5,1.3,1.4,1.2,1.3,1.2,1.2,1.4,1.1000000000000001,1,1.1000000000000001,0.16,0.08,0,0.16,0.09,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1643,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GPU FK06 66 Standard","GPU","FK06","66","MANUAL","Standard","GPU 66","GPU 66","ok","GPU","66","GPU FK06 66 Standard","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.95,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1650,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GPU FK06 66 Standard","GPU","FK06","66","ELECTRIC","Standard","GPU 66","GPU 66","ok","GPU","66","GPU FK06 66 Standard","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.95,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1651,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GPU MK04 62 Standard","GPU","MK04","62","MANUAL","Standard","GPU 62","GPU 62","ok","GPU","62","GPU MK04 62 Standard","62",1.2,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.98,1.1000000000000001,1.2,1,0.88,0.98,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1658,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GPU MK06 57 Standard","GPU","MK06",57,"ELECTRIC","Standard","GPU 57","GPU 70","ok","GPU","70","GPU MK06 70 Standard",57,1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",1663,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GPU MK08 57 Standard","GPU","MK08",57,"MANUAL","Standard","GPU 57","GPU 70","ok","GPU","70","GPU MK08 70 Standard",57,1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",1669,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GPU MK08 57 Standard","GPU","MK08",57,"ELECTRIC","Standard","GPU 57","GPU 70","ok","GPU","70","GPU MK08 70 Standard",57,1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.3,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",1670,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GPU MK10 66 Standard","GPU","MK10","66","MANUAL","Standard","GPU 66","GPU 66","ok","GPU","66","GPU MK10 66 Standard","66",1.2,1.3,1.1000000000000001,1.2,1,1.2,1,1.1000000000000001,1.2,1,0.89,0.98,0.2,0.09,0,0.2,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1677,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GPU PK06 57 Standard","GPU","PK06",57,"ELECTRIC","Standard","GPU 57","GPU 70","ok","GPU","70","GPU PK06 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",1681,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GPU PK08 57 Standard","GPU","PK08",57,"ELECTRIC","Standard","GPU 57","GPU 70","ok","GPU","70","GPU PK08 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",1687,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GPU PK08 62 Standard","GPU","PK08","62","MANUAL","Standard","GPU 62","GPU 62","ok","GPU","62","GPU PK08 62 Standard","62",1,1.2,0.97,1.1000000000000001,0.92,1.1000000000000001,0.89,1,1.1000000000000001,0.98,0.81,0.93,0.26,0.08,0,0.26,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1688,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GPU PK10 62 Standard","GPU","PK10","62","MANUAL","Standard","GPU 62","GPU 62","ok","GPU","62","GPU PK10 62 Standard","62",1,1.2,0.95,1.1000000000000001,0.9,1.1000000000000001,0.88,1,1.1000000000000001,0.97,0.79,0.92,0.27,0.08,0,0.27,0.09,0,0.05,0.08,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1694,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.71]
["GPU SK06 62 Standard","GPU","SK06","62","MANUAL","Standard","GPU 62","GPU 62","ok","GPU","62","GPU SK06 62 Standard","62",1,1.2,0.95,1.1000000000000001,0.89,1.1000000000000001,0.87,1,1.1000000000000001,0.97,0.79,0.91,0.26,0.08,0,0.26,0.09,0,0.05,0.08,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1699,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GPU SK08 57 Standard","GPU","SK08",57,"ELECTRIC","Standard","GPU 57","GPU 70","ok","GPU","70","GPU SK08 70 Standard",57,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",1705,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GPU SK08 62 Standard","GPU","SK08","62","MANUAL","Standard","GPU 62","GPU 62","ok","GPU","62","GPU SK08 62 Standard","62",0.97,1.2,0.92,1.1000000000000001,0.87,1,0.85,1,1.1000000000000001,0.95,0.77,0.9,0.27,0.08,0,0.27,0.09,0,0.05,7.0000000000000007E-2,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.49,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1706,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GPU UK08 57 Standard","GPU","UK08","57","MANUAL","Standard","GPU 57","GPU 70","ok","GPU","70","GPU UK08 70 Standard","57",1.3,1.8,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1.7,1.3,0.98,1.2,0.16,0.05,0,0.16,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",1713,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GTL MK08 66 Standard","GTL","MK08","66","MANUAL","Standard","GTL 66","GPL 66","ok","GPL","66","GPL MK08 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1,1.2,0.99,1.1000000000000001,1.3,1.1000000000000001,0.88,0.99,0.2,0.09,0,0.2,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1717,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GXU CK04 66 Standard","GXU","CK04","66","MANUAL","Standard","GXU 66","GPU 66","ok","GPU","66","GPU CK04 66 Standard","66",1.4,1.5,1.3,1.4,1.2,1.3,1.2,1.2,1.4,1.1000000000000001,1,1.1000000000000001,0.16,0.08,0,0.16,0.09,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1724,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GXU CK06 66 Standard","GXU","CK06","66","MANUAL","Standard","GXU 66","GPU 66","ok","GPU","66","GPU CK06 66 Standard","66",1.4,1.5,1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,1,1.1000000000000001,0.17,0.08,0,0.17,0.09,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1725,0.55000000000000004,1.18,0.65,0.37000000000000005,0.98,2.71,0.36,0.29000000000000004,0.55000000000000004]
["VFE MK31 70 Standard","VFE","MK31","70","MANUAL","Standard","VFE 70","GPL 70","ok","GPL","70","GPL MK31 70 Standard","70",1.6,1.9,1.4,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.2,0.06,0,0.2,0.06,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1730,0.78,0.6,0.47,0.60000000000000009,0.41,2.0099999999999998,0.24,0.22999999999999998,0.51]
["VFE PK31 57 Standard","VFE","PK31","57","MANUAL","Standard","VFE 57","GPL 70","ok","GPL","70","GPL PK31 70 Standard","57",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.12,0.05,0,0.12,0.06,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1734,0.94199999999999995,0.6,0.56999999999999995,0.76200000000000001,0.41,2.34,0.31,0.25999999999999995,0.54]
["VFE PK35 62 Standard","VFE","PK35","62","MANUAL","Standard","VFE 62","VFE 62","ok","VFE","62","VFE PK35 62 Standard","62",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.97,1.1000000000000001,1.2,1,0.87,0.97,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1739,0.94199999999999995,0.95,0.9,0.76200000000000001,0.76,3.04,0.57999999999999996,0.32000000000000006,0.64]
["VFE PK35 66 Standard","VFE","PK35","66","MANUAL","Standard","VFE 66","GPL 66","ok","GPL","66","GPL PK35 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1,1.2,0.99,1.1000000000000001,1.3,1.1000000000000001,0.89,0.99,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1740,0.94199999999999995,0.95,0.9,0.76200000000000001,0.76,3.04,0.57999999999999996,0.32000000000000006,0.64]
["VFE SK31 70 Standard","VFE","SK31","70","MANUAL","Standard","VFE 70","GPL 70","ok","GPL","70","GPL SK31 70 Standard","70",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.22,0.06,0,0.22,0.06,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1745,1.1399999999999999,0.6,0.68,0.96,0.41,2.73,0.39,0.29000000000000004,0.56999999999999995]
["VFE SK35 66 Standard","VFE","SK35","66","MANUAL","Standard","VFE 66","GPL 66","ok","GPL","66","GPL SK35 66 Standard","66",1.1000000000000001,1.3,1.1000000000000001,1.2,0.99,1.1000000000000001,0.96,1.1000000000000001,1.2,1,0.86,0.97,0.2,0.08,0,0.2,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1748,1.1399999999999999,0.95,1.0900000000000001,0.96,0.76,3.44,0.73,0.3600000000000001,0.67]
["VFE UK35 57 Standard","VFE","UK35","57","MANUAL","Standard","VFE 57","GPL 70","ok","GPL","70","GPL UK35 70 Standard","57",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1754,1.34,0.95,1.28,1.1600000000000001,0.76,3.84,0.88,0.4,0.69]
["VFE UK35 62 Standard","VFE","UK35","62","MANUAL","Standard","VFE 62","VFE 62","ok","VFE","62","VFE UK35 62 Standard","62",1.1000000000000001,1.3,0.99,1.2,0.94,1.1000000000000001,0.91,1.1000000000000001,1.2,0.99,0.82,0.94,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1755,1.34,0.95,1.28,1.1600000000000001,0.76,3.84,0.88,0.4,0.69]
["VIU MK31 66 Standard","VIU","MK31","66","FIXED","Standard","VIU 66","GPU 66","ok","GPU","66","GPU MK31 66 Standard","66",1.4,1.5,1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,1,1.1000000000000001,0.16,0.08,0,0.16,0.08,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.32,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1760,0.78,0.6,0.47,0.60000000000000009,0.41,2.0099999999999998,0.24,0.22999999999999998,0.51]
["VIU PK31 57 Standard","VIU","PK31","57","FIXED","Standard","VIU 57","GPU 70","ok","GPU","70","GPU PK31 70 Standard","57",1.6,1.9,1.4,1.7,1.3,1.5,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.06,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1764,0.94199999999999995,0.6,0.56999999999999995,0.76200000000000001,0.41,2.33,0.31,0.25999999999999995,0.54]
["VIU PK35 66 Standard","VIU","PK35","66","FIXED","Standard","VIU 66","GPU 66","ok","GPU","66","GPU PK35 66 Standard","66",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.9,0.99,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1769,0.94199999999999995,0.95,0.9,0.76200000000000001,0.76,3.04,0.57999999999999996,0.32000000000000006,0.64]
["VIU SK31 57 Standard","VIU","SK31","57","FIXED","Standard","VIU 57","GPU 70","ok","GPU","70","GPU SK31 70 Standard","57",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.12,0.05,0,0.12,0.06,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1770,1.1399999999999999,0.6,0.68,0.96,0.41,2.73,0.39,0.29000000000000004,0.56999999999999995]
["VIU SK35 66 Standard","VIU","SK35","66","FIXED","Standard","VIU 66","GPU 66","ok","GPU","66","GPU SK35 66 Standard","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.98,1.1000000000000001,1.2,1,0.87,0.97,0.2,0.09,0,0.2,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1774,1.1399999999999999,0.95,1.0900000000000001,0.96,0.76,3.44,0.73,0.3600000000000001,0.67]
["GFL CK02 54F Standard + BDX","GFL","CK02","54F","MANUAL","Standard + BDX","GFL 54F","GFL 54F","ok","GFL","54F","GFL CK02 54F Standard + BDX","54F",1.7,2,1.6,1.8,1.4,1.6,1.4,1.5,1.8,1.4,1.2,1.3,0.24,0.05,0,0.24,0.05,0,0.04,0.1,0,0.15,0,0.08,0,0.08,0,0.09,0,0.09,0.35,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1800,0.6120000000000001,0.88,0.54,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.41]
["GFL MK04 54F Standard + BDX","GFL","MK04","54F","MANUAL","Standard + BDX","GFL 54F","GFL 54F","ok","GFL","54F","GFL MK04 54F Standard + BDX","54F",1.6,1.9,1.5,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.31,0.05,0,0.31,0.05,0,0.05,0.1,0,0.15,0,0.08,0,0.08,0,0.08,0,0.08,0.45,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1802,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GFL SK06 54F Standard + BDX","GFL","SK06","54F","MANUAL","Standard + BDX","GFL 54F","GFL 54F","ok","GFL","54F","GFL SK06 54F Standard + BDX","54F",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.3,1.1000000000000001,1.2,0.36,0.05,0,0.36,0.05,0,0.06,0.09,0,0.15,0,0.08,0,0.08,0,0.08,0,0.08,0.53,0,0.09,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1806,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GGL CK01 66 Standard + BDX","GGL","CK01","66","MANUAL","Standard + BDX","GGL 66","GPL 66","ok","GPL","66","GPL CK01 66 Standard + BDX","66",1.5,1.6,1.4,1.5,1.3,1.3,1.2,1.3,1.5,1.2,1.1000000000000001,1.1000000000000001,0.12,7.0000000000000007E-2,0,0.12,0.08,0,0.02,0.11,0,0.13,0,0.08,0,0.08,0,0.08,0,0.08,0.26,0,0.04,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1810,0.6120000000000001,0.8,0.49,0.37000000000000005,0.5,1.75,0.18,0.2,0.37]
["GGL CK02 62 Standard + BDX","GGL","CK02","62","MANUAL","Standard + BDX","GGL 62","GPL 62","ok","GPL","62","GPL CK02 62 Standard + BDX","62",1.4,1.5,1.3,1.4,1.2,1.3,1.2,1.2,1.4,1.2,1,1.1000000000000001,0.16,7.0000000000000007E-2,0,0.16,0.08,0,0.03,0.1,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.28999999999999998,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1815,0.6120000000000001,0.88,0.54,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.41]
["GGL CK02 66 Standard + BDX","GGL","CK02","66","SOLAR","Standard + BDX","GGL 66","GPL 66","ok","GPL","66","GPL CK02 66 Standard + BDX","66",1.5,1.6,1.3,1.5,1.2,1.3,1.2,1.3,1.5,1.2,1,1.1000000000000001,0.13,0.08,0,0.13,0.08,0,0.02,0.1,0,0.13,0,0.08,0,0.08,0,0.08,0,0.08,0.27,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1818,0.6120000000000001,0.88,0.54,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.41]
["GGL CK02 70 Standard + BDX","GGL","CK02","70","MANUAL","Standard + BDX","GGL 70","GPL 70","ok","GPL","70","GPL CK02 70 Standard + BDX","70",1.6,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.17,0.06,0,0.17,0.06,0,0.03,0.11,0,0.14000000000000001,0,0.08,0,0.08,0,0.09,0,0.09,0.3,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1821,0.6120000000000001,0.88,0.54,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.41]
["GGL CK02 76F Standard + BDX","GGL","CK02","76F","SOLAR","Standard + BDX","GGL 76F","GPL 70","ok","GPL","70","GPL CK02 70 Standard + BDX","76",1.6,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.09,0.05,0,0.09,0.05,0,0.02,0.11,0,0.13,0,0.08,0,0.08,0,0.09,0,0.09,0.27,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1828,0.6120000000000001,0.88,0.54,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.41]
["GGL CK04 62 Standard + BDX","GGL","CK04","62","ELECTRIC","Standard + BDX","GGL 62","GPL 62","ok","GPL","62","GPL CK04 62 Standard + BDX","62",1.4,1.5,1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.99,1.1000000000000001,0.18,7.0000000000000007E-2,0,0.18,0.08,0,0.03,0.1,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.32,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1834,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GGL CK04 66 Standard + BDX","GGL","CK04","66","ELECTRIC","Standard + BDX","GGL 66","GPL 66","ok","GPL","66","GPL CK04 66 Standard + BDX","66",1.4,1.6,1.3,1.4,1.2,1.3,1.2,1.3,1.4,1.2,1,1.1000000000000001,0.14000000000000001,0.08,0,0.14000000000000001,0.08,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.28999999999999998,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1836,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GGL CK04 70Q Standard + BDX","GGL","CK04","70Q","MANUAL","Standard + BDX","GGL 70Q","GPL 70","ok","GPL","70","GPL CK04 70 Standard + BDX",70,1.6,1.9,1.5,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.18,0.06,0,0.18,0.06,0,0.03,0.11,0,0.14000000000000001,0,0.08,0,0.08,0,0.09,0,0.09,0.32,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1841,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GGL CK06 62 Standard + BDX","GGL","CK06","62","ELECTRIC","Standard + BDX","GGL 62","GPL 62","ok","GPL","62","GPL CK06 62 Standard + BDX","62",1.3,1.5,1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.98,1.1000000000000001,0.18,7.0000000000000007E-2,0,0.18,0.08,0,0.03,0.09,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1847,0.6120000000000001,1.28,0.78,0.37000000000000005,0.98,2.71,0.37,0.28000000000000003,0.47]
["GGL CK06 70H Standard + BDX","GGL","CK06","70H","MANUAL","Standard + BDX","GGL 70H","GPL 70","ok","GPL","70","GPL CK06 70 Standard + BDX",70,1.6,1.9,1.5,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.19,0.06,0,0.19,0.06,0,0.03,0.1,0,0.14000000000000001,0,0.08,0,0.08,0,0.09,0,0.09,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1854,0.6120000000000001,1.28,0.78,0.37000000000000005,0.98,2.71,0.37,0.28000000000000003,0.47]
["GGL FK04 66 Standard + BDX","GGL","FK04","66","ELECTRIC","Standard + BDX","GGL 66","GPL 66","ok","GPL","66","GPL FK04 66 Standard + BDX","66",1.3,1.5,1.2,1.4,1.2,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.99,1.1000000000000001,0.15,0.08,0,0.15,0.08,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.32,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1858,0.72199999999999998,1.08,0.78,0.48000000000000004,0.78,2.5299999999999998,0.38,0.27,0.49]
["GGL FK04 70Q Standard + BDX","GGL","FK04","70Q","MANUAL","Standard + BDX","GGL 70Q","GPL 70","ok","GPL","70","GPL FK04 70 Standard + BDX",70,1.6,1.9,1.4,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.2,0.06,0,0.2,0.06,0,0.04,0.1,0,0.14000000000000001,0,0.08,0,0.08,0,0.08,0,0.08,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1860,0.72199999999999998,1.08,0.78,0.48000000000000004,0.78,2.5299999999999998,0.38,0.27,0.49]
["GGL FK06 66 Standard + BDX","GGL","FK06","66","SOLAR","Standard + BDX","GGL 66","GPL 66","ok","GPL","66","GPL FK06 66 Standard + BDX","66",1.3,1.5,1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.97,1.1000000000000001,0.16,0.08,0,0.16,0.09,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1865,0.72199999999999998,1.28,0.92,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.51]
["GGL FK08 62 Standard + BDX","GGL","FK08","62","ELECTRIC","Standard + BDX","GGL 62","GPL 62","ok","GPL","62","GPL FK08 62 Standard + BDX","62",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.92,1,0.21,0.08,0,0.21,0.08,0,0.04,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1872,0.72199999999999998,1.5,1.08,0.48000000000000004,1.2,3.37,0.57999999999999996,0.34000000000000008,0.54]
["GGL MK04 57 Standard + BDX","GGL","MK04",57,"ELECTRIC","Standard + BDX","GGL 57","GPL 70","ok","GPL","70","GPL MK04 70 Standard + BDX",57,1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.12,0.05,0,0.12,0.06,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.34,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1878,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GGL MK04 62 Standard + BDX","GGL","MK04","62","MANUAL","Standard + BDX","GGL 62","GPL 62","ok","GPL","62","GPL MK04 62 Standard + BDX","62",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.92,1,0.21,0.08,0,0.21,0.08,0,0.04,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1880,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GGL MK04 66 Standard + BDX","GGL","MK04","66","ELECTRIC","Standard + BDX","GGL 66","GPL 66","ok","GPL","66","GPL MK04 66 Standard + BDX","66",1.3,1.5,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.96,1,0.17,0.08,0,0.17,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1883,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GGL MK04 76F Standard + BDX","GGL","MK04","76F","ELECTRIC","Standard + BDX","GGL 76F","GPL 70","ok","GPL","70","GPL MK04 70 Standard + BDX","76",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.12,0.05,0,0.12,0.05,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.34,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1892,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GGL MK06 57 Standard + BDX","GGL","MK06",57,"ELECTRIC","Standard + BDX","GGL 57","GPL 70","ok","GPL","70","GPL MK06 70 Standard + BDX",57,1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.12,0.05,0,0.12,0.06,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.35,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1897,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GGL MK06 62 Standard + BDX","GGL","MK06","62","ELECTRIC","Standard + BDX","GGL 62","GPL 62","ok","GPL","62","GPL MK06 62 Standard + BDX","62",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.9,0.99,0.22,0.08,0,0.22,0.08,0,0.04,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1900,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GGL MK06 66 Standard + BDX","GGL","MK06","66","ELECTRIC","Standard + BDX","GGL 66","GPL 66","ok","GPL","66","GPL MK06 66 Standard + BDX","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.94,1,0.17,0.08,0,0.17,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1902,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GGL MK06 76F Standard + BDX","GGL","MK06","76F","MANUAL","Standard + BDX","GGL 76F","GPL 70","ok","GPL","70","GPL MK06 70 Standard + BDX","76",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.12,0.05,0,0.12,0.05,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.36,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1911,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GGL MK08 57 Standard + BDX","GGL","MK08",57,"ELECTRIC","Standard + BDX","GGL 57","GPL 70","ok","GPL","70","GPL MK08 70 Standard + BDX",57,1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.13,0.05,0,0.13,0.06,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.37,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1916,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GGL MK08 62 Standard + BDX","GGL","MK08","62","MANUAL","Standard + BDX","GGL 62","GPL 62","ok","GPL","62","GPL MK08 62 Standard + BDX","62",1.2,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.98,1.1000000000000001,1.2,1,0.88,0.98,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1918,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GGL MK08 66 Standard + BDX","GGL","MK08","66","ELECTRIC","Standard + BDX","GGL 66","GPL 66","ok","GPL","66","GPL MK08 66 Standard + BDX","66",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.92,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1921,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GGL MK08 76F Standard + BDX","GGL","MK08","76F","ELECTRIC","Standard + BDX","GGL 76F","GPL 70","ok","GPL","70","GPL MK08 70 Standard + BDX","76",1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.13,0.05,0,0.13,0.05,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.37,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1930,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GGL MK10 62 Standard + BDX","GGL","MK10","62","MANUAL","Standard + BDX","GGL 62","GPL 62","ok","GPL","62","GPL MK10 62 Standard + BDX","62",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.97,1.1000000000000001,1.2,1,0.87,0.97,0.23,0.08,0,0.23,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1935,0.84200000000000008,1.7,1.43,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.59]
["GGL MK10 66 Standard + BDX","GGL","MK10","66","ELECTRIC","Standard + BDX","GGL 66","GPL 66","ok","GPL","66","GPL MK10 66 Standard + BDX","66",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.91,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1938,0.84200000000000008,1.7,1.43,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.59]
["GGL MK10 70 Standard + BDX","GGL","MK10","70","MANUAL","Standard + BDX","GGL 70","GPL 70","ok","GPL","70","GPL MK10 70 Standard + BDX","70",1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1,1.2,0.23,0.06,0,0.23,0.06,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1942,0.84200000000000008,1.7,1.43,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.59]
["GGL MK12 70 Standard + BDX","GGL","MK12","70","MANUAL","Standard + BDX","GGL 70","GPL 70","ok","GPL","70","GPL MK12 70 Standard + BDX","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.24,7.0000000000000007E-2,0,0.24,7.0000000000000007E-2,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",4,0.84200000000000008,1.9,1.6,0.60000000000000009,1.61,4.41,0.96,0.43999999999999995,0.6]
["GGL PK04 62 Standard + BDX","GGL","PK04","62","ELECTRIC","Standard + BDX","GGL 62","GPL 62","ok","GPL","62","GPL PK04 62 Standard + BDX","62",1.2,1.3,1.1000000000000001,1.2,1,1.2,0.99,1.1000000000000001,1.2,1,0.88,0.98,0.22,0.08,0,0.22,0.08,0,0.04,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",10,1.004,1.08,1.08,0.76200000000000001,0.78,3.09,0.6,0.32000000000000006,0.56000000000000005]
["GGL PK04 66 Standard + BDX","GGL","PK04","66","MANUAL","Standard + BDX","GGL 66","GPL 66","ok","GPL","66","GPL PK04 66 Standard + BDX","66",1.2,1.4,1.2,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.93,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",11,1.004,1.08,1.08,0.76200000000000001,0.78,3.09,0.6,0.32000000000000006,0.56000000000000005]
["GGL PK06 62 Standard + BDX","GGL","PK06","62","ELECTRIC","Standard + BDX","GGL 62","GPL 62","ok","GPL","62","GPL PK06 62 Standard + BDX","62",1.1000000000000001,1.3,1,1.2,0.98,1.1000000000000001,0.96,1.1000000000000001,1.2,1,0.86,0.96,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",18,1.004,1.28,1.29,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.57999999999999996]
["GGL PK06 70Q Standard + BDX","GGL","PK06","70Q","MANUAL","Standard + BDX","GGL 70Q","GPL 70","ok","GPL","70","GPL PK06 70 Standard + BDX",70,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.23,0.06,0,0.23,0.06,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",25,1.004,1.28,1.29,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.57999999999999996]
["GGL PK08 62 Standard + BDX","GGL","PK08","62","MANUAL","Standard + BDX","GGL 62","GPL 62","ok","GPL","62","GPL PK08 62 Standard + BDX","62",1.1000000000000001,1.3,1,1.2,0.96,1.1000000000000001,0.94,1.1000000000000001,1.2,1,0.84,0.95,0.24,0.08,0,0.24,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",31,1.004,1.5,1.51,0.76200000000000001,1.2,3.93,0.92,0.4,0.61]
["GGL PK08 62 Standard + BDX","GGL","PK08","62","ELECTRIC","Standard + BDX","GGL 62","GPL 62","ok","GPL","62","GPL PK08 62 Standard + BDX","62",1.1000000000000001,1.3,1,1.2,0.96,1.1000000000000001,0.94,1.1000000000000001,1.2,1,0.84,0.95,0.24,0.08,0,0.24,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",32,1.004,1.5,1.51,0.76200000000000001,1.2,3.93,0.92,0.4,0.61]
["GGL PK08 70 Standard + BDX","GGL","PK08","70","MANUAL","Standard + BDX","GGL 70","GPL 70","ok","GPL","70","GPL PK08 70 Standard + BDX","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.24,7.0000000000000007E-2,0,0.24,7.0000000000000007E-2,0,0.04,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",39,1.004,1.5,1.51,0.76200000000000001,1.2,3.93,0.92,0.4,0.61]
["GGL PK10 57 Standard + BDX","GGL","PK10",57,"MANUAL","Standard + BDX","GGL 57","GPL 70","ok","GPL","70","GPL PK10 70 Standard + BDX",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",43,1.004,1.7,1.71,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.63]
["GGL PK10 66 Standard + BDX","GGL","PK10","66","SOLAR","Standard + BDX","GGL 66","GPL 66","ok","GPL","66","GPL PK10 66 Standard + BDX","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,0.98,1.1000000000000001,1.2,1,0.87,0.98,0.2,0.08,0,0.2,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",49,1.004,1.7,1.71,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.63]
["GGL PK10 70 Standard + BDX","GGL","PK10","70","ELECTRIC","Standard + BDX","GGL 70","GPL 70","ok","GPL","70","GPL PK10 70 Standard + BDX","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.25,7.0000000000000007E-2,0,0.25,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",51,1.004,1.7,1.71,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.63]
["GGL PK25 62 Standard + BDX","GGL","PK25","62","ELECTRIC","Standard + BDX","GGL 62","GPL 62","ok","GPL","62","GPL PK25 62 Standard + BDX","62",1.3,1.5,1.2,1.4,1.2,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.98,1.1000000000000001,0.17,7.0000000000000007E-2,0,0.17,0.08,0,0.03,0.1,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.31,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",58,1.004,0.65,0.65,0.76200000000000001,0.36,2.2400000000000002,0.27,0.25,0.42]
["GGL SK01 62 Standard + BDX","GGL","SK01","62","ELECTRIC","Standard + BDX","GGL 62","GPL 62","ok","GPL","62","GPL SK01 62 Standard + BDX","62",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.91,1,0.21,0.08,0,0.21,0.08,0,0.04,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",62,1.202,0.8,0.96,0.96,0.5,2.93,0.49,0.31000000000000005,0.51]
["GGL SK06 57 Standard + BDX","GGL","SK06",57,"ELECTRIC","Standard + BDX","GGL 57","GPL 70","ok","GPL","70","GPL SK06 70 Standard + BDX",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",66,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GGL SK06 57 Standard + BDX","GGL","SK06",57,"MANUAL","Standard + BDX","GGL 57","GPL 70","ok","GPL","70","GPL SK06 70 Standard + BDX",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",68,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GGL SK06 66 Standard + BDX","GGL","SK06","66","ELECTRIC","Standard + BDX","GGL 66","GPL 66","ok","GPL","66","GPL SK06 66 Standard + BDX","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,0.98,1.1000000000000001,1.2,1,0.88,0.98,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",73,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GGL SK06 70Q Standard + BDX","GGL","SK06","70Q","MANUAL","Standard + BDX","GGL 70Q","GPL 70","ok","GPL","70","GPL SK06 70 Standard + BDX",70,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.25,7.0000000000000007E-2,0,0.25,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",81,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GGL SK08 54F Standard + BDX","GGL","SK08","54F","MANUAL","Standard + BDX","GGL 54F","GPL 54F","ok","GPL","54F","GPL SK08 54F Standard + BDX","54F",1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.38,0.05,0,0.38,0.05,0,7.0000000000000007E-2,0.09,0,0.15,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.55000000000000004,0,0.09,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",86,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GGL SK08 57 Standard + BDX","GGL","SK08",57,"MANUAL","Standard + BDX","GGL 57","GPL 70","ok","GPL","70","GPL SK08 70 Standard + BDX",57,1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",80,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GGL SK08 70 Standard + BDX","GGL","SK08","70","MANUAL","Standard + BDX","GGL 70","GPL 70","ok","GPL","70","GPL SK08 70 Standard + BDX","70",1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.26,7.0000000000000007E-2,0,0.26,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",93,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GGL SK08 57 Standard + BDX","GGL","SK08",57,"ELECTRIC","Standard + BDX","GGL 57","GPL 70","ok","GPL","70","GPL SK08 70 Standard + BDX",57,1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",90,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GGL SK10 70Q Standard + BDX","GGL","SK10","70Q","MANUAL","Standard + BDX","GGL 70Q","GPL 70","ok","GPL","70","GPL SK10 70 Standard + BDX",70,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.26,7.0000000000000007E-2,0,0.26,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",105,1.202,1.7,2.0499999999999998,0.96,1.41,4.7300000000000004,1.35,0.47,0.66]
["GGL SK10 76F Standard + BDX","GGL","SK10","76F","MANUAL","Standard + BDX","GGL 76F","GPL 70","ok","GPL","70","GPL SK10 70 Standard + BDX","76",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",103,1.202,1.7,2.0499999999999998,0.96,1.41,4.7300000000000004,1.35,0.47,0.66]
["GGL UK04 66 Standard + BDX","GGL","UK04","66","ELECTRIC","Standard + BDX","GGL 66","GPL 66","ok","GPL","66","GPL UK04 66 Standard + BDX","66",1.2,1.3,1.1000000000000001,1.2,1,1.2,0.98,1.1000000000000001,1.2,1.1000000000000001,0.88,0.99,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",110,1.4020000000000001,1.08,1.51,1.1600000000000001,0.78,3.89,0.91,0.4,0.6]
["GGL UK04 70Q Standard + BDX","GGL","UK04","70Q","MANUAL","Standard + BDX","GGL 70Q","GPL 70","ok","GPL","70","GPL UK04 70 Standard + BDX",70,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.24,0.06,0,0.24,0.06,0,0.04,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",115,1.4020000000000001,1.08,1.51,1.1600000000000001,0.78,3.89,0.91,0.4,0.6]
["GGL UK04 70 Standard + BDX","GGL","UK04","70","ELECTRIC","Standard + BDX","GGL 70","GPL 70","ok","GPL","70","GPL UK04 70 Standard + BDX","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.24,0.06,0,0.24,0.06,0,0.04,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",121,1.4020000000000001,1.08,1.51,1.1600000000000001,0.78,3.89,0.91,0.4,0.6]
["GGL UK08 54F Standard + BDX","GGL","UK08","54F","MANUAL","Standard + BDX","GGL 54F","GPL 54F","ok","GPL","54F","GPL UK08 54F Standard + BDX","54F",1.4,1.8,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.39,0.05,0,0.39,0.05,0,7.0000000000000007E-2,0.08,0,0.15,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.56999999999999995,0,0.1,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",122,1.4020000000000001,1.5,2.1,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.66]
["GGL UK08 70 Standard + BDX","GGL","UK08","70","MANUAL","Standard + BDX","GGL 70","GPL 70","ok","GPL","70","GPL UK08 70 Standard + BDX","70",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.99,1.2,0.26,7.0000000000000007E-2,0,0.26,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",129,1.4020000000000001,1.5,2.1,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.66]
["GGL UK08 76F Standard + BDX","GGL","UK08","76F","SOLAR","Standard + BDX","GGL 76F","GPL 70","ok","GPL","70","GPL UK08 70 Standard + BDX","76",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.99,1.2,0.15,0.05,0,0.15,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",134,1.4020000000000001,1.5,2.1,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.66]
["GGL UK10 66 Standard + BDX","GGL","UK10","66","ELECTRIC","Standard + BDX","GGL 66","GPL 66","ok","GPL","66","GPL UK10 66 Standard + BDX","66",1.1000000000000001,1.3,0.99,1.2,0.93,1.1000000000000001,0.91,1.1000000000000001,1.2,1,0.82,0.94,0.21,0.09,0,0.21,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",139,1.4020000000000001,1.7,2.39,1.1600000000000001,1.41,5.13,1.63,0.51000000000000023,0.68]
["GGL UK10 70Q Standard + BDX","GGL","UK10","70Q","MANUAL","Standard + BDX","GGL 70Q","GPL 70","ok","GPL","70","GPL UK10 70 Standard + BDX",70,1.3,1.8,1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.98,1.2,0.27,7.0000000000000007E-2,0,0.27,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",142,1.4020000000000001,1.7,2.39,1.1600000000000001,1.41,5.13,1.63,0.51000000000000023,0.68]
["GGLS FFKF08 70 Standard + BDX","GGLS","FFKF08","70","SOLAR","Standard + BDX","GGLS 70","GGLS 70 3in1","ok","GGLS",70,"GGLS FFKF08 70 Standard + BDX","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.26,0.06,0,0.26,0.06,0,0.05,0.09,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",169,1.9419999999999999,1.5,2.91,1.444,1.2,10.11,1.74,0.8899999999999999,0.6]
["GGLS FFKF08 70 Flush","GGLS","FFKF08","70","MANUAL","Flush","GGLS 70","GGLS 70 3in1","ok","GGLS",70,"GGLS FFKF08 70 Flush","70",1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.96,1.2,0.27,0.06,0,0.27,0.06,0,0.05,0.08,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.49,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.88,1.4,2.63,1.444,1.2,10.11,1.74,0.8899999999999999,0.66]
["GGLS FFKF06 57 Standard","GGLS","FFKF06",57,"MANUAL","Standard","GGLS 57","GGLS 70 3in1","ok","GGLS",70,"GGLS FFKF06 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1,1.2,0.18,0.03,0,0.18,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1234,1.88,1.18,2.21,1.444,0.98,8.7899999999999991,1.42,0.79,0.64]
["GGLS FFKF06 57 Standard","GGLS","FFKF06",57,"SOLAR","Standard","GGLS 57","GGLS 70 3in1","ok","GGLS",70,"GGLS FFKF06 70 Standard",57,1.4,1.9,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1,1.2,0.18,0.03,0,0.18,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1235,1.88,1.18,2.21,1.444,0.98,8.7899999999999991,1.42,0.79,0.64]
["GGLS FFKF08 70 Standard","GGLS","FFKF08","70","MANUAL","Standard","GGLS 70","GGLS 70 3in1","ok","GGLS",70,"GGLS FFKF08 70 Standard","70",1.3,1.8,1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.99,1.2,0.27,0.06,0,0.27,0.06,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.49,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1246,1.88,1.4,2.63,1.444,1.2,10.11,1.74,0.8899999999999999,0.66]
["GPLS FFKF06 70 Standard + BDX","GPLS","FFKF06","70","MANUAL","Standard + BDX","GPLS 70","GPLS 70 3in1","ok","GPLS",70,"GPLS FFKF06 70 Standard + BDX","70",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1,1.2,0.25,0.05,0,0.25,0.06,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.9419999999999999,1.28,2.4900000000000002,1.444,0.98,8.7899999999999991,1.42,0.79,0.56999999999999995]
["GPLS FFKF06 70 Flush + BDX","GPLS","FFKF06","70","MANUAL","Flush + BDX","GPLS 70","GPLS 70 3in1","ok","GPLS",70,"GPLS FFKF06 70 Flush + BDX","70",1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1,1.3,0.98,1.2,0.93,1.2,0.24,0.04,0,0.24,0.06,0,0.04,0.08,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.9419999999999999,1.28,2.4900000000000002,1.444,0.98,8.7899999999999991,1.42,0.79,0.56999999999999995]
["GPLS FFKF08 57 Standard","GPLS","FFKF08",57,"MANUAL","Standard","GPLS 57","GGLS 70 3in1","ok","GGLS",70,"GGLS FFKF08 70 Standard",57,1.3,1.8,1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,0.99,1.2,0.19,0.04,0,0.19,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1619,1.88,1.4,2.63,1.444,1.2,10.11,1.74,0.8899999999999999,0.66]
["GPLS FFKF08 70 Flush","GPLS","FFKF08","70","MANUAL","Flush","GPLS 70","GPLS 70 3in1","ok","GPLS",70,"GPLS FFKF08 70 Flush","70",1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.97,1.2,0.27,0.06,0,0.27,0.06,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.49,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.88,1.4,2.63,1.444,1.2,10.11,1.74,0.8899999999999999,0.66]
["GGLS FFKF06 76F Flush","GGLS","FFKF06","76F","MANUAL","Flush","GGLS 76F","GPLS 70 3in1","ok","GPLS",70,"GPLS FFKF06 70 Flush","76",1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,0.98,1.2,0.15,0.03,0,0.15,0.05,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.88,1.18,2.21,1.444,0.98,8.7899999999999991,1.42,0.79,0.64]
["GGLS FFKF06 76F Flush + BDX","GGLS","FFKF06","76F","SOLAR","Flush + BDX","GGLS 76F","GPLS 70 3in1","ok","GPLS",70,"GPLS FFKF06 70 Flush + BDX","76",1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1,1.3,0.98,1.2,0.93,1.2,0.13,0.03,0,0.13,0.05,0,0.02,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.9419999999999999,1.28,2.4900000000000002,1.444,0.98,8.7899999999999991,1.42,0.79,0.56999999999999995]
["GGLS FFKF08 76F Standard + BDX","GGLS","FFKF08","76F","SOLAR","Standard + BDX","GGLS 76F","GPLS 70 3in1","ok","GPLS",70,"GPLS FFKF08 70 Standard + BDX","76",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",172,1.9419999999999999,1.5,2.91,1.444,1.2,10.11,1.74,0.8899999999999999,0.6]
["GGLS FFKF06 76F Standard","GGLS","FFKF06","76F","MANUAL","Standard","GGLS 76F","GPLS 70 3in1","ok","GPLS",70,"GPLS FFKF06 70 Standard","76",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1,1.2,0.15,0.03,0,0.15,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",1240,1.88,1.18,2.21,1.444,0.98,8.7899999999999991,1.42,0.79,0.64]
["GGU CK02 57 Standard + BDX","GGU","CK02",57,"ELECTRIC","Standard + BDX","GGU 57","GPU 70","ok","GPU","70","GPU CK02 70 Standard + BDX",57,1.7,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.09,0.05,0,0.09,0.06,0,0.02,0.11,0,0.13,0,0.08,0,0.08,0,0.09,0,0.09,0.27,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",209,0.6120000000000001,0.88,0.54,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.41]
["GGU CK02 66 Standard + BDX","GGU","CK02","66","ELECTRIC","Standard + BDX","GGU 66","GPU 66","ok","GPU","66","GPU CK02 66 Standard + BDX","66",1.5,1.6,1.4,1.5,1.3,1.3,1.2,1.3,1.5,1.2,1.1000000000000001,1.1000000000000001,0.13,0.08,0,0.13,0.08,0,0.02,0.11,0,0.13,0,0.08,0,0.08,0,0.08,0,0.08,0.27,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",213,0.6120000000000001,0.88,0.54,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.41]
["GGU CK02 66 Standard + BDX","GGU","CK02","66","SOLAR","Standard + BDX","GGU 66","GPU 66","ok","GPU","66","GPU CK02 66 Standard + BDX","66",1.5,1.6,1.4,1.5,1.3,1.3,1.2,1.3,1.5,1.2,1.1000000000000001,1.1000000000000001,0.13,0.08,0,0.13,0.08,0,0.02,0.11,0,0.13,0,0.08,0,0.08,0,0.08,0,0.08,0.27,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",214,0.6120000000000001,0.88,0.54,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.41]
["GGU CK04 57 Standard + BDX","GGU","CK04",57,"MANUAL","Standard + BDX","GGU 57","GPU 70","ok","GPU","70","GPU CK04 70 Standard + BDX",57,1.6,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.1,0.05,0,0.1,0.06,0,0.02,0.11,0,0.13,0,0.08,0,0.08,0,0.09,0,0.09,0.28999999999999998,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",223,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GGU CK04 66 Standard + BDX","GGU","CK04","66","ELECTRIC","Standard + BDX","GGU 66","GPU 66","ok","GPU","66","GPU CK04 66 Standard + BDX","66",1.5,1.6,1.3,1.4,1.2,1.3,1.2,1.3,1.4,1.2,1,1.1000000000000001,0.14000000000000001,0.08,0,0.14000000000000001,0.08,0,0.02,0.1,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.28999999999999998,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",228,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GGU CK04 70Q Standard + BDX","GGU","CK04","70Q","MANUAL","Standard + BDX","GGU 70Q","GPU 70","ok","GPU","70","GPU CK04 70 Standard + BDX",70,1.6,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.18,0.06,0,0.18,0.06,0,0.03,0.11,0,0.14000000000000001,0,0.08,0,0.08,0,0.09,0,0.09,0.32,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",234,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GGU CK04 76F Standard + BDX","GGU","CK04","76F","ELECTRIC","Standard + BDX","GGU 76F","GPU 70","ok","GPU","70","GPU CK04 70 Standard + BDX","76",1.6,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.1,0.05,0,0.1,0.05,0,0.02,0.11,0,0.13,0,0.08,0,0.08,0,0.09,0,0.09,0.28999999999999998,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",236,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GGU CK06 66 Standard + BDX","GGU","CK06","66","SOLAR","Standard + BDX","GGU 66","GPU 66","ok","GPU","66","GPU CK06 66 Standard + BDX","66",1.4,1.5,1.3,1.4,1.2,1.3,1.2,1.3,1.4,1.2,1,1.1000000000000001,0.15,0.08,0,0.15,0.08,0,0.02,0.1,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.3,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",241,0.6120000000000001,1.28,0.78,0.37000000000000005,0.98,2.71,0.36,0.29000000000000004,0.46]
["GGU FK04 70Q Standard + BDX","GGU","FK04","70Q","MANUAL","Standard + BDX","GGU 70Q","GPU 70","ok","GPU","70","GPU FK04 70 Standard + BDX",70,1.6,1.9,1.4,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.2,0.06,0,0.2,0.06,0,0.04,0.1,0,0.14000000000000001,0,0.08,0,0.08,0,0.09,0,0.09,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",251,0.72199999999999998,1.08,0.78,0.48000000000000004,0.78,2.5299999999999998,0.38,0.27,0.49]
["GGU FK06 66 Standard + BDX","GGU","FK06","66","ELECTRIC","Standard + BDX","GGU 66","GPU 66","ok","GPU","66","GPU FK06 66 Standard + BDX","66",1.3,1.5,1.2,1.4,1.2,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.99,1.1000000000000001,0.16,0.08,0,0.16,0.09,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",255,0.72199999999999998,1.28,0.92,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.51]
["GGU FK06 66 Standard + BDX","GGU","FK06","66","SOLAR","Standard + BDX","GGU 66","GPU 66","ok","GPU","66","GPU FK06 66 Standard + BDX","66",1.3,1.5,1.2,1.4,1.2,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.99,1.1000000000000001,0.16,0.08,0,0.16,0.09,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",256,0.72199999999999998,1.28,0.92,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.51]
["GGU FK08 66 Standard + BDX","GGU","FK08","66","MANUAL","Standard + BDX","GGU 66","GPU 66","ok","GPU","66","GPU FK08 66 Standard + BDX","66",1.3,1.5,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.97,1,0.17,0.08,0,0.17,0.09,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",264,0.72199999999999998,1.5,1.08,0.48000000000000004,1.2,3.37,0.57999999999999996,0.34000000000000008,0.54]
["GGU MK04 57 Standard + BDX","GGU","MK04",57,"SOLAR","Standard + BDX","GGU 57","GPU 70","ok","GPU","70","GPU MK04 70 Standard + BDX",57,1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.12,0.05,0,0.12,0.06,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.34,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",272,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GGU MK04 66 Standard + BDX","GGU","MK04","66","SOLAR","Standard + BDX","GGU 66","GPU 66","ok","GPU","66","GPU MK04 66 Standard + BDX","66",1.3,1.5,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.97,1,0.16,0.08,0,0.16,0.09,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",277,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GGU MK04 70Q Standard + BDX","GGU","MK04","70Q","MANUAL","Standard + BDX","GGU 70Q","GPU 70","ok","GPU","70","GPU MK04 70 Standard + BDX",70,1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.21,0.06,0,0.21,0.06,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",283,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GGU MK06 57 Standard + BDX","GGU","MK06",57,"MANUAL","Standard + BDX","GGU 57","GPU 70","ok","GPU","70","GPU MK06 70 Standard + BDX",57,1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.12,0.05,0,0.12,7.0000000000000007E-2,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.35,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",286,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GGU MK06 66 Standard + BDX","GGU","MK06","66","MANUAL","Standard + BDX","GGU 66","GPU 66","ok","GPU","66","GPU MK06 66 Standard + BDX","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.95,1,0.17,0.08,0,0.17,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",291,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GGU MK06 76F Standard + BDX","GGU","MK06","76F","MANUAL","Standard + BDX","GGU 76F","GPU 70","ok","GPU","70","GPU MK06 70 Standard + BDX","76",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.12,0.05,0,0.12,0.05,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.36,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",300,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GGU MK06 76F Standard + BDX","GGU","MK06","76F","ELECTRIC","Standard + BDX","GGU 76F","GPU 70","ok","GPU","70","GPU MK06 70 Standard + BDX","76",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.12,0.05,0,0.12,0.05,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.36,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",301,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GGU MK08 62 Standard + BDX","GGU","MK08","62","MANUAL","Standard + BDX","GGU 62","GPU 62","ok","GPU","62","GPU MK08 62 Standard + BDX","62",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.97,1.1000000000000001,1.2,1,0.87,0.97,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",305,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GGU MK08 70 Standard + BDX","GGU","MK08","70","MANUAL","Standard + BDX","GGU 70","GPU 70","ok","GPU","70","GPU MK08 70 Standard + BDX","70",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.23,7.0000000000000007E-2,0,0.23,7.0000000000000007E-2,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",314,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GGU MK10 62 Standard + BDX","GGU","MK10","62","ELECTRIC","Standard + BDX","GGU 62","GPU 62","ok","GPU","62","GPU MK10 62 Standard + BDX","62",1.1000000000000001,1.3,1,1.2,0.98,1.1000000000000001,0.96,1.1000000000000001,1.2,1,0.86,0.96,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",319,0.84200000000000008,1.7,1.43,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.59]
["GGU MK10 66 Standard + BDX","GGU","MK10","66","ELECTRIC","Standard + BDX","GGU 66","GPU 66","ok","GPU","66","GPU MK10 66 Standard + BDX","66",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.93,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",321,0.84200000000000008,1.7,1.43,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.59]
["GGU MK10 70 Standard + BDX","GGU","MK10","70","ELECTRIC","Standard + BDX","GGU 70","GPU 70","ok","GPU","70","GPU MK10 70 Standard + BDX","70",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.2,0.23,7.0000000000000007E-2,0,0.23,7.0000000000000007E-2,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",327,0.84200000000000008,1.7,1.43,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.59]
["GGU PK06 62 Standard + BDX","GGU","PK06","62","ELECTRIC","Standard + BDX","GGU 62","GPU 62","ok","GPU","62","GPU PK06 62 Standard + BDX","62",1.1000000000000001,1.3,1,1.2,0.97,1.1000000000000001,0.94,1.1000000000000001,1.2,1,0.85,0.95,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",332,1.004,1.28,1.29,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.57999999999999996]
["GGU PK06 70Q Standard + BDX","GGU","PK06","70Q","MANUAL","Standard + BDX","GGU 70Q","GPU 70","ok","GPU","70","GPU PK06 70 Standard + BDX",70,1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.23,7.0000000000000007E-2,0,0.23,7.0000000000000007E-2,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",341,1.004,1.28,1.29,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.57999999999999996]
["GGU PK06 76F Standard + BDX","GGU","PK06","76F","MANUAL","Standard + BDX","GGU 76F","GPU 70","ok","GPU","70","GPU PK06 70 Standard + BDX","76",1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.13,0.05,0,0.13,0.05,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",342,1.004,1.28,1.29,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.57999999999999996]
["GGU PK08 62 Standard + BDX","GGU","PK08","62","MANUAL","Standard + BDX","GGU 62","GPU 62","ok","GPU","62","GPU PK08 62 Standard + BDX","62",1.1000000000000001,1.3,1,1.2,0.95,1.1000000000000001,0.92,1.1000000000000001,1.2,1,0.83,0.94,0.24,0.08,0,0.24,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",346,1.004,1.5,1.51,0.76200000000000001,1.2,3.93,0.92,0.4,0.61]
["GGU PK08 70 Standard + BDX","GGU","PK08","70","MANUAL","Standard + BDX","GGU 70","GPU 70","ok","GPU","70","GPU PK08 70 Standard + BDX","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.24,7.0000000000000007E-2,0,0.24,7.0000000000000007E-2,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",354,1.004,1.5,1.51,0.76200000000000001,1.2,3.93,0.92,0.4,0.61]
["GGU PK10 57 Standard + BDX","GGU","PK10",57,"SOLAR","Standard + BDX","GGU 57","GPU 70","ok","GPU","70","GPU PK10 70 Standard + BDX",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",359,1.004,1.7,1.71,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.63]
["GGU PK10 62 Standard + BDX","GGU","PK10","62","MANUAL","Standard + BDX","GGU 62","GPU 62","ok","GPU","62","GPU PK10 62 Standard + BDX","62",1.1000000000000001,1.2,0.99,1.2,0.93,1.1000000000000001,0.91,1,1.2,0.99,0.82,0.93,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",360,1.004,1.7,1.71,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.63]
["GGU PK10 70Q Standard + BDX","GGU","PK10","70Q","MANUAL","Standard + BDX","GGU 70Q","GPU 70","ok","GPU","70","GPU PK10 70 Standard + BDX",70,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.25,7.0000000000000007E-2,0,0.25,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",370,1.004,1.7,1.71,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.63]
["GGU SK06 57 Standard + BDX","GGU","SK06",57,"ELECTRIC","Standard + BDX","GGU 57","GPU 70","ok","GPU","70","GPU SK06 70 Standard + BDX",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",373,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GGU SK06 66 Standard + BDX","GGU","SK06","66","ELECTRIC","Standard + BDX","GGU 66","GPU 66","ok","GPU","66","GPU SK06 66 Standard + BDX","66",1.2,1.3,1.1000000000000001,1.2,1,1.2,0.99,1.1000000000000001,1.2,1,0.89,0.98,0.19,0.09,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",379,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GGU SK06 66 Standard + BDX","GGU","SK06","66","SOLAR","Standard + BDX","GGU 66","GPU 66","ok","GPU","66","GPU SK06 66 Standard + BDX","66",1.2,1.3,1.1000000000000001,1.2,1,1.2,0.99,1.1000000000000001,1.2,1,0.89,0.98,0.19,0.09,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",378,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GGU SK06 76F Standard + BDX","GGU","SK06","76F","ELECTRIC","Standard + BDX","GGU 76F","GPU 70","ok","GPU","70","GPU SK06 70 Standard + BDX","76",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",387,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GGU SK08 62 Standard + BDX","GGU","SK08","62","ELECTRIC","Standard + BDX","GGU 62","GPU 62","ok","GPU","62","GPU SK08 62 Standard + BDX","62",1,1.2,0.96,1.1000000000000001,0.91,1.1000000000000001,0.88,1,1.1000000000000001,0.97,0.8,0.92,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",392,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GGU SK08 76F Standard + BDX","GGU","SK08","76F","MANUAL","Standard + BDX","GGU 76F","GPU 70","ok","GPU","70","GPU SK08 70 Standard + BDX","76",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",400,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GGU SK08 76F Standard + BDX","GGU","SK08","76F","ELECTRIC","Standard + BDX","GGU 76F","GPU 70","ok","GPU","70","GPU SK08 70 Standard + BDX","76",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",401,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GGU UK04 57 Standard + BDX","GGU","UK04",57,"SOLAR","Standard + BDX","GGU 57","GPU 70","ok","GPU","70","GPU UK04 70 Standard + BDX",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.13,0.05,0,0.13,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",409,1.4020000000000001,1.08,1.51,1.1600000000000001,0.78,3.89,0.91,0.4,0.6]
["GGU UK04 66 Standard + BDX","GGU","UK04","66","SOLAR","Standard + BDX","GGU 66","GPU 66","ok","GPU","66","GPU UK04 66 Standard + BDX","66",1.2,1.3,1.1000000000000001,1.2,1,1.2,0.99,1.1000000000000001,1.2,1.1000000000000001,0.89,0.99,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",413,1.4020000000000001,1.08,1.51,1.1600000000000001,0.78,3.89,0.91,0.4,0.6]
["GGU UK08 57 Standard + BDX","GGU","UK08",57,"MANUAL","Standard + BDX","GGU 57","GPU 70","ok","GPU","70","GPU UK08 70 Standard + BDX",57,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",420,1.4020000000000001,1.5,2.1,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.66]
["GGU UK08 57 Standard + BDX","GGU","UK08",57,"ELECTRIC","Standard + BDX","GGU 57","GPU 70","ok","GPU","70","GPU UK08 70 Standard + BDX",57,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",427,1.4020000000000001,1.5,2.1,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.66]
["GGU UK08 66 Standard + BDX","GGU","UK08","66","SOLAR","Standard + BDX","GGU 66","GPU 66","ok","GPU","66","GPU UK08 66 Standard + BDX","66",1.1000000000000001,1.3,1,1.2,0.96,1.1000000000000001,0.94,1.1000000000000001,1.2,1,0.84,0.95,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.5,2.1,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.66]
["GGU UK10 66 Standard + BDX","GGU","UK10","66","MANUAL","Standard + BDX","GGU 66","GPU 66","ok","GPU","66","GPU UK10 66 Standard + BDX","66",1.1000000000000001,1.3,1,1.2,0.95,1.1000000000000001,0.92,1.1000000000000001,1.2,1,0.83,0.94,0.21,0.09,0,0.21,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.7,2.39,1.1600000000000001,1.41,5.13,1.63,0.51000000000000023,0.68]
["GIL MK34 66 Standard + BDX","GIL","MK34","66","FIXED","Standard + BDX","GIL 66","GPL 66","ok","GPL","66","GPL MK34 66 Standard + BDX","66",1.3,1.5,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.96,1.1000000000000001,0.16,0.08,0,0.16,0.09,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.02,0.86,0.60000000000000009,0.73,2.65,0.44,0.27999999999999997,0.51]
["GIL MK34 70 Standard + BDX","GIL","MK34","70","FIXED","Standard + BDX","GIL 70","GPL 70","ok","GPL","70","GPL MK34 70 Standard + BDX","70",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.21,0.06,0,0.21,0.06,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.02,0.86,0.60000000000000009,0.73,2.65,0.44,0.27999999999999997,0.51]
["GIL SK34 57 Standard + BDX","GIL","SK34","57","FIXED","Standard + BDX","GIL 57","GPL 70","ok","GPL","70","GPL SK34 70 Standard + BDX","57",1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.12,0.05,0,0.12,0.06,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.02,1.23,0.96,0.73,3.37,0.7,0.35000000000000009,0.56999999999999995]
["GIL UK34 66 Standard + BDX","GIL","UK34","66","FIXED","Standard + BDX","GIL 66","GPL 66","ok","GPL","66","GPL UK34 66 Standard + BDX","66",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.9,1,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.02,1.43,1.1600000000000001,0.73,3.77,0.84,0.39,0.59]
["GIU MK34 57 Standard + BDX","GIU","MK34","57","FIXED","Standard + BDX","GIU 57","GPU 70","ok","GPU","70","GPU MK34 70 Standard + BDX","57",1.5,1.9,1.4,1.7,1.3,1.5,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.06,0,0.02,0.1,0,0.12,0,0.08,0,0.08,0,0.08,0,0.08,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.02,0.86,0.60000000000000009,0.73,2.65,0.44,0.27999999999999997,0.51]
["GIU MK34 62 Standard + BDX","GIU","MK34","62","FIXED","Standard + BDX","GIU 62","GIU 62","ok","GIU","62","GIU MK34 62 Standard + BDX","62",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.94,1,0.2,0.08,0,0.2,0.08,0,0.04,0.09,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.02,0.86,0.60000000000000009,0.73,2.65,0.44,0.27999999999999997,0.51]
["GIU SK34 57 Standard + BDX","GIU","SK34","57","FIXED","Standard + BDX","GIU 57","GPU 70","ok","GPU","70","GPU SK34 70 Standard + BDX","57",1.5,1.9,1.4,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1.1000000000000001,1.2,0.12,0.05,0,0.12,0.06,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.02,1.23,0.96,0.73,3.37,0.7,0.35000000000000009,0.56999999999999995]
["GIU UK34 57 Standard + BDX","GIU","UK34","57","FIXED","Standard + BDX","GIU 57","GPU 70","ok","GPU","70","GPU UK34 70 Standard + BDX","57",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.13,0.05,0,0.13,0.06,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.02,1.43,1.1600000000000001,0.73,3.77,0.84,0.39,0.59]
["GPL CK04 70 Standard + BDX","GPL","CK04","70","MANUAL","Standard + BDX","GPL 70","GPL 70","ok","GPL","70","GPL CK04 70 Standard + BDX","70",1.6,1.9,1.5,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.18,0.06,0,0.18,0.06,0,0.03,0.11,0,0.14000000000000001,0,0.08,0,0.08,0,0.09,0,0.09,0.32,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GPL CK06 66 Standard + BDX","GPL","CK06","66","MANUAL","Standard + BDX","GPL 66","GPL 66","ok","GPL","66","GPL CK06 66 Standard + BDX","66",1.4,1.5,1.3,1.4,1.2,1.3,1.2,1.3,1.4,1.2,1,1.1000000000000001,0.15,0.08,0,0.15,0.08,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.3,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,1.28,0.78,0.37000000000000005,0.98,2.71,0.37,0.28000000000000003,0.47]
["GPL MK04 66 Standard + BDX","GPL","MK04","66","MANUAL","Standard + BDX","GPL 66","GPL 66","ok","GPL","66","GPL MK04 66 Standard + BDX","66",1.3,1.5,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.96,1,0.17,0.08,0,0.17,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GPL MK06 76F Standard + BDX","GPL","MK06","76F","MANUAL","Standard + BDX","GPL 76F","GPL 70","ok","GPL","70","GPL MK06 70 Standard + BDX","76",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.12,0.05,0,0.12,0.05,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.36,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",422,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GPL MK08 76F Standard + BDX","GPL","MK08","76F","MANUAL","Standard + BDX","GPL 76F","GPL 70","ok","GPL","70","GPL MK08 70 Standard + BDX","76",1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.13,0.05,0,0.13,0.05,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.37,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",422,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GPL MK08 70 Standard + BDX","GPL","MK08","70","MANUAL","Standard + BDX","GPL 70","GPL 70","ok","GPL","70","GPL MK08 70 Standard + BDX","70",1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.23,0.06,0,0.23,0.06,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GPL PK06 66 Standard + BDX","GPL","PK06","66","MANUAL","Standard + BDX","GPL 66","GPL 66","ok","GPL","66","GPL PK06 66 Standard + BDX","66",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.9,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.28,1.29,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.57999999999999996]
["GPL PK10 57 Standard + BDX","GPL","PK10",57,"MANUAL","Standard + BDX","GPL 57","GPL 70","ok","GPL","70","GPL PK10 70 Standard + BDX",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",422,1.004,1.7,1.71,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.63]
["GPL SK06 76F Standard + BDX","GPL","SK06","76F","MANUAL","Standard + BDX","GPL 76F","GPL 70","ok","GPL","70","GPL SK06 70 Standard + BDX","76",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",422,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GPL SK06 70 Standard + BDX","GPL","SK06","70","MANUAL","Standard + BDX","GPL 70","GPL 70","ok","GPL","70","GPL SK06 70 Standard + BDX","70",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.25,7.0000000000000007E-2,0,0.25,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GPL UK04 57 Standard + BDX","GPL","UK04",57,"MANUAL","Standard + BDX","GPL 57","GPL 70","ok","GPL","70","GPL UK04 70 Standard + BDX",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.13,0.05,0,0.13,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",422,1.4020000000000001,1.08,1.51,1.1600000000000001,0.78,3.89,0.91,0.4,0.6]
["GPL UK08 66 Standard + BDX","GPL","UK08","66","MANUAL","Standard + BDX","GPL 66","GPL 66","ok","GPL","66","GPL UK08 66 Standard + BDX","66",1.1000000000000001,1.3,1,1.2,0.95,1.1000000000000001,0.93,1.1000000000000001,1.2,1,0.83,0.95,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.5,2.1,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.66]
["GPLS FFKF06 76F Standard","GPLS","FFKF06","76F","MANUAL","Standard","GPLS 76F","GPLS 70 3in1","ok","GPLS",70,"GPLS FFKF06 70 Standard","76",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1,1.2,0.15,0.03,0,0.15,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",1618,1.88,1.18,2.21,1.444,0.98,8.7899999999999991,1.42,0.79,0.64]
["GPLS FFKF06 76F Standard + BDX","GPLS","FFKF06","76F","MANUAL","Standard + BDX","GPLS 76F","GPLS 70 3in1","ok","GPLS",70,"GPLS FFKF06 70 Standard + BDX","76",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1,1.2,0.14000000000000001,0.03,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.9419999999999999,1.28,2.4900000000000002,1.444,0.98,8.7899999999999991,1.42,0.79,0.56999999999999995]
["GPLS FFKF08 76F Flush","GPLS","FFKF08","76F","MANUAL","Flush","GPLS 76F","GPLS 70 3in1","ok","GPLS",70,"GPLS FFKF08 70 Flush","76",1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.97,1.2,0.15,0.05,0,0.15,0.05,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.88,1.4,2.63,1.444,1.2,10.11,1.74,0.8899999999999999,0.66]
["GPU CK04 76F Standard + BDX","GPU","CK04","76F","MANUAL","Standard + BDX","GPU 76F","GPU 70","ok","GPU","70","GPU CK04 70 Standard + BDX","76",1.6,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.1,0.05,0,0.1,0.05,0,0.02,0.11,0,0.13,0,0.08,0,0.08,0,0.09,0,0.09,0.28999999999999998,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GPU FK06 62 Standard + BDX","GPU","FK06","62","MANUAL","Standard + BDX","GPU 62","GPU 62","ok","GPU","62","GPU FK06 62 Standard + BDX","62",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.92,1,0.2,0.08,0,0.2,0.08,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.72199999999999998,1.28,0.92,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.51]
["GPU FK06 66 Standard + BDX","GPU","FK06","66","ELECTRIC","Standard + BDX","GPU 66","GPU 66","ok","GPU","66","GPU FK06 66 Standard + BDX","66",1.3,1.5,1.2,1.4,1.2,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.99,1.1000000000000001,0.16,0.08,0,0.16,0.09,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.72199999999999998,1.28,0.92,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.51]
["GPU MK04 62 Standard + BDX","GPU","MK04","62","MANUAL","Standard + BDX","GPU 62","GPU 62","ok","GPU","62","GPU MK04 62 Standard + BDX","62",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.9,0.99,0.21,0.08,0,0.21,0.08,0,0.04,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GPU MK06 62 Standard + BDX","GPU","MK06","62","MANUAL","Standard + BDX","GPU 62","GPU 62","ok","GPU","62","GPU MK06 62 Standard + BDX","62",1.2,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.99,1.1000000000000001,1.2,1,0.88,0.98,0.22,0.08,0,0.22,0.08,0,0.04,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GPU MK06 66 Standard + BDX","GPU","MK06","66","ELECTRIC","Standard + BDX","GPU 66","GPU 66","ok","GPU","66","GPU MK06 66 Standard + BDX","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.95,1,0.17,0.08,0,0.17,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GPU MK08 57 Standard + BDX","GPU","MK08",57,"ELECTRIC","Standard + BDX","GPU 57","GPU 70","ok","GPU","70","GPU MK08 70 Standard + BDX",57,1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.13,0.05,0,0.13,7.0000000000000007E-2,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.37,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GPU MK10 62 Standard + BDX","GPU","MK10","62","MANUAL","Standard + BDX","GPU 62","GPU 62","ok","GPU","62","GPU MK10 62 Standard + BDX","62",1.1000000000000001,1.3,1,1.2,0.98,1.1000000000000001,0.96,1.1000000000000001,1.2,1,0.86,0.96,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.7,1.43,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.59]
["GPU PK06 62 Standard + BDX","GPU","PK06","62","MANUAL","Standard + BDX","GPU 62","GPU 62","ok","GPU","62","GPU PK06 62 Standard + BDX","62",1.1000000000000001,1.3,1,1.2,0.97,1.1000000000000001,0.94,1.1000000000000001,1.2,1,0.85,0.95,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.28,1.29,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.57999999999999996]
["GPU PK08 57 Standard + BDX","GPU","PK08",57,"MANUAL","Standard + BDX","GPU 57","GPU 70","ok","GPU","70","GPU PK08 70 Standard + BDX",57,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.13,0.05,0,0.13,7.0000000000000007E-2,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,1.004,1.5,1.51,0.76200000000000001,1.2,3.93,0.92,0.4,0.61]
["GPU PK08 62 Standard + BDX","GPU","PK08","62","MANUAL","Standard + BDX","GPU 62","GPU 62","ok","GPU","62","GPU PK08 62 Standard + BDX","62",1.1000000000000001,1.3,1,1.2,0.95,1.1000000000000001,0.92,1.1000000000000001,1.2,1,0.83,0.94,0.24,0.08,0,0.24,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.5,1.51,0.76200000000000001,1.2,3.93,0.92,0.4,0.61]
["GPU PK10 62 Standard + BDX","GPU","PK10","62","MANUAL","Standard + BDX","GPU 62","GPU 62","ok","GPU","62","GPU PK10 62 Standard + BDX","62",1.1000000000000001,1.2,0.99,1.2,0.93,1.1000000000000001,0.91,1,1.2,0.99,0.82,0.93,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.7,1.71,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.63]
["GPU SK06 66 Standard + BDX","GPU","SK06","66","MANUAL","Standard + BDX","GPU 66","GPU 66","ok","GPU","66","GPU SK06 66 Standard + BDX","66",1.2,1.3,1.1000000000000001,1.2,1,1.2,0.99,1.1000000000000001,1.2,1,0.89,0.98,0.19,0.09,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GPU SK06 76F Standard + BDX","GPU","SK06","76F","MANUAL","Standard + BDX","GPU 76F","GPU 70","ok","GPU","70","GPU SK06 70 Standard + BDX","76",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GPU SK08 62 Standard + BDX","GPU","SK08","62","MANUAL","Standard + BDX","GPU 62","GPU 62","ok","GPU","62","GPU SK08 62 Standard + BDX","62",1,1.2,0.96,1.1000000000000001,0.91,1.1000000000000001,0.88,1,1.1000000000000001,0.97,0.8,0.92,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GPU UK08 57 Standard + BDX","GPU","UK08","57","MANUAL","Standard + BDX","GPU 57","GPU 70","ok","GPU","70","GPU UK08 70 Standard + BDX","57",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,1.4020000000000001,1.5,2.1,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.66]
["GTL SK08 66 Standard + BDX","GTL","SK08","66","MANUAL","Standard + BDX","GTL 66","GPL 66","ok","GPL","66","GPL SK08 66 Standard + BDX","66",1.1000000000000001,1.3,1,1.2,0.98,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.86,0.97,0.2,0.09,0,0.2,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GXU CK06 66 Standard + BDX","GXU","CK06","66","MANUAL","Standard + BDX","GXU 66","GPU 66","ok","GPU","66","GPU CK06 66 Standard + BDX","66",1.4,1.5,1.3,1.4,1.2,1.3,1.2,1.3,1.4,1.2,1,1.1000000000000001,0.15,0.08,0,0.15,0.08,0,0.02,0.1,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.3,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,1.28,0.78,0.37000000000000005,0.98,2.71,0.36,0.29000000000000004,0.46]
["VFE MK31 62 Standard + BDX","VFE","MK31","62","MANUAL","Standard + BDX","VFE 62","VFE 62","ok","VFE","62","VFE MK31 62 Standard + BDX","62",1.4,1.5,1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,1,1.1000000000000001,0.17,7.0000000000000007E-2,0,0.17,0.08,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.3,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,0.7,0.59,0.60000000000000009,0.41,2.0099999999999998,0.24,0.22999999999999998,0.41]
["VFE MK31 70 Standard + BDX","VFE","MK31","70","MANUAL","Standard + BDX","VFE 70","GPL 70","ok","GPL","70","GPL MK31 70 Standard + BDX","70",1.6,1.9,1.5,1.7,1.3,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.17,0.06,0,0.17,0.06,0,0.03,0.11,0,0.14000000000000001,0,0.08,0,0.08,0,0.09,0,0.09,0.31,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,0.7,0.59,0.60000000000000009,0.41,2.0099999999999998,0.24,0.22999999999999998,0.41]
["VFE PK31 62 Standard + BDX","VFE","PK31","62","MANUAL","Standard + BDX","VFE 62","VFE 62","ok","VFE","62","VFE PK31 62 Standard + BDX","62",1.3,1.5,1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.98,1.1000000000000001,0.18,7.0000000000000007E-2,0,0.18,0.08,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.32,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,0.7,0.7,0.76200000000000001,0.41,2.34,0.31,0.25999999999999995,0.44]
["VFE PK35 66 Standard + BDX","VFE","PK35","66","MANUAL","Standard + BDX","VFE 66","GPL 66","ok","GPL","66","GPL PK35 66 Standard + BDX","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.94,1,0.17,0.08,0,0.17,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.06,1.06,0.76200000000000001,0.76,3.04,0.57999999999999996,0.32000000000000006,0.55000000000000004]
["VFE PK35 70 Standard + BDX","VFE","PK35","70","MANUAL","Standard + BDX","VFE 70","GPL 70","ok","GPL","70","GPL PK35 70 Standard + BDX","70",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.2,0.21,0.06,0,0.21,0.06,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.06,1.06,0.76200000000000001,0.76,3.04,0.57999999999999996,0.32000000000000006,0.55000000000000004]
["VFE SK31 70 Standard + BDX","VFE","SK31","70","MANUAL","Standard + BDX","VFE 70","GPL 70","ok","GPL","70","GPL SK31 70 Standard + BDX","70",1.5,1.9,1.4,1.7,1.3,1.5,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.19,0.06,0,0.19,0.06,0,0.04,0.1,0,0.14000000000000001,0,0.08,0,0.08,0,0.08,0,0.08,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,0.7,0.84,0.96,0.41,2.73,0.39,0.29000000000000004,0.46]
["VFE UK31 57 Standard + BDX","VFE","UK31","57","MANUAL","Standard + BDX","VFE 57","GPL 70","ok","GPL","70","GPL UK31 70 Standard + BDX","57",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.06,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.32,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,0.7,0.98,1.1600000000000001,0.41,3.13,0.47,0.33000000000000007,0.48]
["VFE UK35 62 Standard + BDX","VFE","UK35","62","MANUAL","Standard + BDX","VFE 62","VFE 62","ok","VFE","62","VFE UK35 62 Standard + BDX","62",1.1000000000000001,1.3,1,1.2,0.98,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.86,0.96,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.06,1.48,1.1600000000000001,0.76,3.84,0.88,0.4,0.59]
["VIU MK31 57 Standard + BDX","VIU","MK31","57","FIXED","Standard + BDX","VIU 57","GPU 70","ok","GPU","70","GPU MK31 70 Standard + BDX","57",1.6,1.9,1.5,1.7,1.4,1.6,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.1,0.05,0,0.1,0.06,0,0.02,0.11,0,0.13,0,0.08,0,0.08,0,0.09,0,0.09,0.28000000000000003,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,0.7,0.59,0.60000000000000009,0.41,2.0099999999999998,0.24,0.22999999999999998,0.41]
["VIU MK31 66 Standard + BDX","VIU","MK31","66","FIXED","Standard + BDX","VIU 66","GPU 66","ok","GPU","66","GPU MK31 66 Standard + BDX","66",1.4,1.6,1.3,1.4,1.2,1.3,1.2,1.3,1.4,1.2,1,1.1000000000000001,0.14000000000000001,0.08,0,0.14000000000000001,0.08,0,0.02,0.1,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.28000000000000003,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,0.7,0.59,0.60000000000000009,0.41,2.0099999999999998,0.24,0.22999999999999998,0.41]
["VIU PK31 62 Standard + BDX","VIU","PK31","62","FIXED","Standard + BDX","VIU 62","GIU 62","ok","GIU","62","GIU PK31 62 Standard + BDX","62",1.4,1.5,1.2,1.4,1.2,1.3,1.1000000000000001,1.2,1.4,1.1000000000000001,0.99,1.1000000000000001,0.18,0.08,0,0.18,0.08,0,0.03,0.1,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,0.7,0.7,0.76200000000000001,0.41,2.33,0.31,0.25999999999999995,0.44]
["VIU SK31 57 Standard + BDX","VIU","SK31","57","FIXED","Standard + BDX","VIU 57","GPU 70","ok","GPU","70","GPU SK31 70 Standard + BDX","57",1.6,1.9,1.4,1.7,1.3,1.5,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.11,0.05,0,0.11,0.06,0,0.02,0.1,0,0.12,0,0.08,0,0.08,0,0.08,0,0.08,0.31,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,0.7,0.84,0.96,0.41,2.73,0.39,0.29000000000000004,0.46]
["VIU SK31 62 Standard + BDX","VIU","SK31","62","FIXED","Standard + BDX","VIU 62","GIU 62","ok","GIU","62","GIU SK31 62 Standard + BDX","62",1.3,1.5,1.2,1.4,1.1000000000000001,1.2,1.1000000000000001,1.2,1.4,1.1000000000000001,0.97,1.1000000000000001,0.19,0.08,0,0.19,0.08,0,0.03,0.09,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,0.7,0.84,0.96,0.41,2.73,0.39,0.29000000000000004,0.46]
["VIU SK35 66 Standard + BDX","VIU","SK35","66","FIXED","Standard + BDX","VIU 66","GPU 66","ok","GPU","66","GPU SK35 66 Standard + BDX","66",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.92,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.06,1.27,0.96,0.76,3.44,0.73,0.3600000000000001,0.56999999999999995]
["GFL CK02 54F Flush","GFL","CK02","54F","MANUAL","Flush","GFL 54F","GFL 54F","ok","GFL","54F","GFL CK02 54F Flush","54F",1.6,1.9,1.5,1.7,1.3,1.5,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.27,0.05,0,0.27,0.05,0,0.05,0.1,0,0.15,0,0.08,0,0.08,0,0.09,0,0.09,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GFL SK06 54F Flush","GFL","SK06","54F","MANUAL","Flush","GFL 54F","GFL 54F","ok","GFL","54F","GFL SK06 54F Flush","54F",1.4,1.8,1.3,1.6,1.2,1.5,1.2,1.4,1.6,1.3,1,1.2,0.39,0.05,0,0.39,0.05,0,7.0000000000000007E-2,0.08,0,0.15,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.56999999999999995,0,0.1,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GFL SK08 54F Flush","GFL","SK08","54F","MANUAL","Flush","GFL 54F","GFL 54F","ok","GFL","54F","GFL SK08 54F Flush","54F",1.4,1.8,1.3,1.6,1.2,1.5,1.1000000000000001,1.4,1.6,1.3,1,1.2,0.4,0.05,0,0.4,0.05,0,7.0000000000000007E-2,0.08,0,0.15,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.59,0,0.1,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGL CK02 54F Flush","GGL","CK02","54F","MANUAL","Flush","GGL 54F","GPL 54F","ok","GPL","54F","GPL CK02 54F Flush","54F",1.6,1.9,1.5,1.7,1.3,1.5,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.28000000000000003,0.05,0,0.28000000000000003,0.05,0,0.05,0.09,0,0.14000000000000001,0,0.08,0,0.08,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGL CK02 62 Flush","GGL","CK02","62","MANUAL","Flush","GGL 62","GPL 62","ok","GPL","62","GPL CK02 62 Flush","62",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.95,1,0.19,7.0000000000000007E-2,0,0.19,0.08,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGL CK02 70 Flush","GGL","CK02","70","MANUAL","Flush","GGL 70","GPL 70","ok","GPL","70","GPL CK02 70 Flush","70",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.3,1.1000000000000001,1.2,0.19,0.06,0,0.19,0.06,0,0.04,0.1,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGL CK02 70 Flush","GGL","CK02","70","MANUALBOTTOM","Flush","GGL 70","GPL 70","ok","GPL","70","GPL CK02 70 Flush","70",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.3,1.1000000000000001,1.2,0.19,0.06,0,0.19,0.06,0,0.04,0.1,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGL CK04 54F Flush","GGL","CK04","54F","MANUAL","Flush","GGL 54F","GPL 54F","ok","GPL","54F","GPL CK04 54F Flush","54F",1.6,1.9,1.4,1.7,1.3,1.5,1.3,1.5,1.7,1.4,1.1000000000000001,1.3,0.3,0.05,0,0.3,0.05,0,0.05,0.09,0,0.15,0,0.08,0,0.08,0,0.08,0,0.08,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGL CK04 62 Flush","GGL","CK04","62","ELECTRIC","Flush","GGL 62","GPL 62","ok","GPL","62","GPL CK04 62 Flush","62",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.94,1,0.2,7.0000000000000007E-2,0,0.2,0.08,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGL CK04 70Q Flush","GGL","CK04","70Q","MANUAL","Flush","GGL 70Q","GPL 70","ok","GPL","70","GPL CK04 70 Flush",70,1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.3,1.1000000000000001,1.2,0.21,0.06,0,0.21,0.06,0,0.04,0.1,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGL CK04 76F Flush","GGL","CK04","76F","MANUAL","Flush","GGL 76F","GPL 70","ok","GPL","70","GPL CK04 70 Flush","76",1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.3,1.1000000000000001,1.2,0.11,0.05,0,0.11,0.05,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.33,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGL CK06 66 Flush","GGL","CK06","66","ELECTRIC","Flush","GGL 66","GPL 66","ok","GPL","66","GPL CK06 66 Flush","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.94,1,0.17,0.08,0,0.17,0.08,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.55000000000000004,1.18,0.65,0.37000000000000005,0.98,2.71,0.37,0.28000000000000003,0.56999999999999995]
["GGL CK06 70H Flush","GGL","CK06","70H","MANUAL","Flush","GGL 70H","GPL 70","ok","GPL","70","GPL CK06 70 Flush",70,1.5,1.9,1.4,1.7,1.3,1.5,1.2,1.5,1.7,1.4,1.1000000000000001,1.2,0.21,0.06,0,0.21,0.06,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.55000000000000004,1.18,0.65,0.37000000000000005,0.98,2.71,0.37,0.28000000000000003,0.56999999999999995]
["GGL FK04 70Q Flush","GGL","FK04","70Q","MANUAL","Flush","GGL 70Q","GPL 70","ok","GPL","70","GPL FK04 70 Flush",70,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.22,0.06,0,0.22,0.06,0,0.04,0.09,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.66,0.98,0.65,0.48000000000000004,0.78,2.5299999999999998,0.38,0.27,0.57999999999999996]
["GGL FK06 62 Flush","GGL","FK06","62","MANUAL","Flush","GGL 62","GPL 62","ok","GPL","62","GPL FK06 62 Flush","62",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.98,1.1000000000000001,1.2,1,0.88,0.98,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GGL FK06 70Q Flush","GGL","FK06","70Q","MANUAL","Flush","GGL 70Q","GPL 70","ok","GPL","70","GPL FK06 70 Flush",70,1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.23,0.06,0,0.23,0.06,0,0.04,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GGL FK08 62 Flush","GGL","FK08","62","ELECTRIC","Flush","GGL 62","GPL 62","ok","GPL","62","GPL FK08 62 Flush","62",1.1000000000000001,1.3,1.1000000000000001,1.2,0.99,1.1000000000000001,0.96,1.1000000000000001,1.2,1,0.86,0.97,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.66,1.4,0.92,0.48000000000000004,1.2,3.37,0.57999999999999996,0.34000000000000008,0.63]
["GGL MK04 57 Flush","GGL","MK04",57,"ELECTRIC","Flush","GGL 57","GPL 70","ok","GPL","70","GPL MK04 70 Flush",57,1.4,1.8,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.13,0.05,0,0.13,0.06,0,0.02,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGL MK04 57 Flush","GGL","MK04",57,"MANUAL","Flush","GGL 57","GPL 70","ok","GPL","70","GPL MK04 70 Flush",57,1.4,1.8,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.13,0.05,0,0.13,0.06,0,0.02,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGL MK04 66 Flush","GGL","MK04","66","SOLAR","Flush","GGL 66","GPL 66","ok","GPL","66","GPL MK04 66 Flush","66",1.2,1.3,1.1000000000000001,1.2,1,1.2,0.99,1.1000000000000001,1.2,1,0.88,0.99,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGL MK04 76F Flush","GGL","MK04","76F","MANUAL","Flush","GGL 76F","GPL 70","ok","GPL","70","GPL MK04 70 Flush","76",1.4,1.8,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.13,0.05,0,0.13,0.05,0,0.02,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGL MK06 57 Flush","GGL","MK06",57,"ELECTRIC","Flush","GGL 57","GPL 70","ok","GPL","70","GPL MK06 70 Flush",57,1.4,1.8,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.13,0.05,0,0.13,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGL MK06 57 Flush","GGL","MK06",57,"MANUAL","Flush","GGL 57","GPL 70","ok","GPL","70","GPL MK06 70 Flush",57,1.4,1.8,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.13,0.05,0,0.13,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGL MK06 66 Flush","GGL","MK06","66","SOLAR","Flush","GGL 66","GPL 66","ok","GPL","66","GPL MK06 66 Flush","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.97,1.1000000000000001,1.2,1,0.87,0.98,0.19,0.08,0,0.19,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGL MK06 76F Flush","GGL","MK06","76F","MANUAL","Flush","GGL 76F","GPL 70","ok","GPL","70","GPL MK06 70 Flush","76",1.4,1.8,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.13,0.05,0,0.13,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGL MK08 57 Flush","GGL","MK08",57,"ELECTRIC","Flush","GGL 57","GPL 70","ok","GPL","70","GPL MK08 70 Flush",57,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGL MK08 57 Flush","GGL","MK08",57,"MANUAL","Flush","GGL 57","GPL 70","ok","GPL","70","GPL MK08 70 Flush",57,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGL MK08 66 Flush","GGL","MK08","66","SOLAR","Flush","GGL 66","GPL 66","ok","GPL","66","GPL MK08 66 Flush","66",1.1000000000000001,1.3,1,1.2,0.98,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.86,0.97,0.2,0.08,0,0.2,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGL MK08 70Q Flush","GGL","MK08","70Q","MANUAL","Flush","GGL 70Q","GPL 70","ok","GPL","70","GPL MK08 70 Flush",70,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.25,0.06,0,0.25,0.06,0,0.05,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGL MK10 62 Flush","GGL","MK10","62","MANUAL","Flush","GGL 62","GPL 62","ok","GPL","62","GPL MK10 62 Flush","62",1,1.2,0.98,1.2,0.93,1.1000000000000001,0.9,1,1.2,0.99,0.81,0.93,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GGL MK10 62 Flush","GGL","MK10","62","ELECTRIC","Flush","GGL 62","GPL 62","ok","GPL","62","GPL MK10 62 Flush","62",1,1.2,0.98,1.2,0.93,1.1000000000000001,0.9,1,1.2,0.99,0.81,0.93,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GGL MK10 70Q Flush","GGL","MK10","70Q","MANUAL","Flush","GGL 70Q","GPL 70","ok","GPL","70","GPL MK10 70 Flush",70,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.26,0.06,0,0.26,0.06,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GGL MK12 70 Flush","GGL","MK12","70","MANUAL","Flush","GGL 70","GPL 70","ok","GPL","70","GPL MK12 70 Flush","70",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.26,0.06,0,0.26,0.06,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,1.8,1.4,0.60000000000000009,1.61,4.41,0.96,0.43999999999999995,0.69]
["GGL PK04 62 Flush","GGL","PK04","62","ELECTRIC","Flush","GGL 62","GPL 62","ok","GPL","62","GPL PK04 62 Flush","62",1.1000000000000001,1.2,0.99,1.2,0.94,1.1000000000000001,0.91,1.1000000000000001,1.2,0.99,0.82,0.93,0.24,0.08,0,0.24,0.08,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,0.98,0.92,0.76200000000000001,0.78,3.09,0.6,0.32000000000000006,0.65]
["GGL PK04 66 Flush","GGL","PK04","66","MANUAL","Flush","GGL 66","GPL 66","ok","GPL","66","GPL PK04 66 Flush","66",1.1000000000000001,1.3,1,1.2,0.98,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.85,0.97,0.19,0.08,0,0.19,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,0.98,0.92,0.76200000000000001,0.78,3.09,0.6,0.32000000000000006,0.65]
["GGL PK06 62 Flush","GGL","PK06","62","ELECTRIC","Flush","GGL 62","GPL 62","ok","GPL","62","GPL PK06 62 Flush","62",1,1.2,0.96,1.1000000000000001,0.91,1.1000000000000001,0.88,1,1.1000000000000001,0.97,0.8,0.92,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGL PK06 76F Flush","GGL","PK06","76F","ELECTRIC","Flush","GGL 76F","GPL 70","ok","GPL","70","GPL PK06 70 Flush","76",1.3,1.8,1.2,1.6,1.2,1.5,1.1000000000000001,1.4,1.6,1.3,0.99,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGL PK08 57 Flush","GGL","PK08",57,"ELECTRIC","Flush","GGL 57","GPL 70","ok","GPL","70","GPL PK08 70 Flush",57,1.3,1.8,1.2,1.6,1.2,1.5,1.1000000000000001,1.4,1.6,1.3,0.98,1.2,0.15,0.05,0,0.15,0.06,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGL PK08 62 Flush","GGL","PK08","62","ELECTRIC","Flush","GGL 62","GPL 62","ok","GPL","62","GPL PK08 62 Flush","62",1,1.2,0.94,1.1000000000000001,0.89,1.1000000000000001,0.87,1,1.1000000000000001,0.96,0.79,0.91,0.26,0.08,0,0.26,0.09,0,0.04,7.0000000000000007E-2,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGL PK08 70 Flush","GGL","PK08","70","MANUALBOTTOM","Flush","GGL 70","GPL 70","ok","GPL","70","GPL PK08 70 Flush","70",1.3,1.8,1.2,1.6,1.2,1.5,1.1000000000000001,1.4,1.6,1.3,0.98,1.2,0.26,0.06,0,0.26,0.06,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGL PK10 62 Flush","GGL","PK10","62","MANUAL","Flush","GGL 62","GPL 62","ok","GPL","62","GPL PK10 62 Flush","62",0.98,1.2,0.93,1.1000000000000001,0.88,1,0.85,1,1.1000000000000001,0.95,0.78,0.9,0.27,0.08,0,0.27,0.09,0,0.05,7.0000000000000007E-2,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.71]
["GGL PK10 66 Flush","GGL","PK10","66","SOLAR","Flush","GGL 66","GPL 66","ok","GPL","66","GPL PK10 66 Flush","66",1,1.3,0.98,1.2,0.92,1.1000000000000001,0.9,1.1000000000000001,1.2,0.99,0.81,0.94,0.21,0.09,0,0.21,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.71]
["GGL PK10 70 Flush","GGL","PK10","70","ELECTRIC","Flush","GGL 70","GPL 70","ok","GPL","70","GPL PK10 70 Flush","70",1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.98,1.2,0.27,0.06,0,0.27,0.06,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.71]
["GGL PK25 62 Flush","GGL","PK25","62","ELECTRIC","Flush","GGL 62","GPL 62","ok","GPL","62","GPL PK25 62 Flush","62",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.91,1,0.19,7.0000000000000007E-2,0,0.19,0.08,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,0.55000000000000004,0.52,0.76200000000000001,0.36,2.2400000000000002,0.27,0.25,0.52]
["GGL SK01 66 Flush","GGL","SK01","66","MANUAL","Flush","GGL 66","GPL 66","ok","GPL","66","GPL SK01 66 Flush","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.98,1.1000000000000001,1.2,1,0.88,0.98,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.1399999999999999,0.7,0.8,0.96,0.5,2.93,0.49,0.31000000000000005,0.61]
["GGL SK01 76F Flush","GGL","SK01","76F","MANUAL","Flush","GGL 76F","GPL 70","ok","GPL","70","GPL SK01 70 Flush","76",1.4,1.8,1.3,1.6,1.2,1.5,1.1000000000000001,1.4,1.6,1.3,1,1.2,0.13,0.05,0,0.13,0.05,0,0.02,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.1399999999999999,0.7,0.8,0.96,0.5,2.93,0.49,0.31000000000000005,0.61]
["GGL SK06 57 Flush","GGL","SK06",57,"MANUAL","Flush","GGL 57","GPL 70","ok","GPL","70","GPL SK06 70 Flush",57,1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.97,1.2,0.15,0.05,0,0.15,0.06,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGL SK06 66 Flush","GGL","SK06","66","SOLAR","Flush","GGL 66","GPL 66","ok","GPL","66","GPL SK06 66 Flush","66",1,1.2,0.97,1.2,0.92,1.1000000000000001,0.9,1,1.2,0.99,0.81,0.93,0.21,0.08,0,0.21,0.09,0,0.04,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGL SK06 76F Flush","GGL","SK06","76F","ELECTRIC","Flush","GGL 76F","GPL 70","ok","GPL","70","GPL SK06 70 Flush","76",1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.97,1.2,0.15,0.05,0,0.15,0.05,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGL SK08 54F Flush","GGL","SK08","54F","MANUAL","Flush","GGL 54F","GPL 54F","ok","GPL","54F","GPL SK08 54F Flush","54F",1.4,1.8,1.3,1.6,1.2,1.5,1.1000000000000001,1.4,1.6,1.3,1,1.2,0.4,0.05,0,0.4,0.05,0,7.0000000000000007E-2,0.08,0,0.15,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.59,0,0.1,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGL SK08 57 Flush","GGL","SK08",57,"MANUAL","Flush","GGL 57","GPL 70","ok","GPL","70","GPL SK08 70 Flush",57,1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.96,1.2,0.15,0.05,0,0.15,0.06,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGL SK08 70 Flush","GGL","SK08","70","MANUAL","Flush","GGL 70","GPL 70","ok","GPL","70","GPL SK08 70 Flush","70",1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.96,1.2,0.28000000000000003,0.06,0,0.28000000000000003,0.06,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.49,0,0.09,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGL SK08 57 Flush","GGL","SK08",57,"SOLAR","Flush","GGL 57","GPL 70","ok","GPL","70","GPL SK08 70 Flush",57,1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.96,1.2,0.15,0.05,0,0.15,0.06,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGL SK10 66 Flush","GGL","SK10","66","ELECTRIC","Flush","GGL 66","GPL 66","ok","GPL","66","GPL SK10 66 Flush","66",0.99,1.2,0.94,1.1000000000000001,0.89,1.1000000000000001,0.86,1,1.1000000000000001,0.97,0.78,0.91,0.22,0.09,0,0.22,0.09,0,0.04,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.1399999999999999,1.6,1.82,0.96,1.41,4.7300000000000004,1.35,0.47,0.74]
["GGL SK10 76F Flush","GGL","SK10","76F","MANUAL","Flush","GGL 76F","GPL 70","ok","GPL","70","GPL SK10 70 Flush","76",1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.96,1.2,0.16,0.05,0,0.16,0.05,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.1399999999999999,1.6,1.82,0.96,1.41,4.7300000000000004,1.35,0.47,0.74]
["GGL UK04 66 Flush","GGL","UK04","66","ELECTRIC","Flush","GGL 66","GPL 66","ok","GPL","66","GPL UK04 66 Flush","66",1,1.2,0.98,1.2,0.92,1.1000000000000001,0.9,1,1.2,0.99,0.81,0.93,0.21,0.08,0,0.21,0.09,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGL UK04 76F Flush","GGL","UK04","76F","MANUAL","Flush","GGL 76F","GPL 70","ok","GPL","70","GPL UK04 70 Flush","76",1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.97,1.2,0.15,0.05,0,0.15,0.05,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGL UK08 54F Flush","GGL","UK08","54F","MANUAL","Flush","GGL 54F","GPL 54F","ok","GPL","54F","GPL UK08 54F Flush","54F",1.4,1.8,1.3,1.6,1.2,1.5,1.1000000000000001,1.4,1.6,1.3,0.99,1.2,0.42,0.05,0,0.42,0.05,0,7.0000000000000007E-2,0.08,0,0.15,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.61,0,0.1,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGL UK08 66 Flush","GGL","UK08","66","ELECTRIC","Flush","GGL 66","GPL 66","ok","GPL","66","GPL UK08 66 Flush","66",0.97,1.2,0.92,1.1000000000000001,0.87,1,0.85,1,1.1000000000000001,0.96,0.77,0.91,0.22,0.09,0,0.22,0.09,0,0.04,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGL UK08 70 Flush","GGL","UK08","70","MANUAL","Flush","GGL 70","GPL 70","ok","GPL","70","GPL UK08 70 Flush","70",1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.95,1.2,0.28000000000000003,0.06,0,0.28000000000000003,0.06,0,0.05,0.08,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.51,0,0.09,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGL UK08 76F Flush","GGL","UK08","76F","SOLAR","Flush","GGL 76F","GPL 70","ok","GPL","70","GPL UK08 70 Flush","76",1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.95,1.2,0.16,0.05,0,0.16,0.05,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGL UK10 70Q Flush","GGL","UK10","70Q","MANUAL","Flush","GGL 70Q","GPL 70","ok","GPL","70","GPL UK10 70 Flush",70,1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.94,1.2,0.28999999999999998,7.0000000000000007E-2,0,0.28999999999999998,7.0000000000000007E-2,0,0.05,0.08,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.52,0,0.09,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.34,1.6,2.14,1.1600000000000001,1.41,5.13,1.63,0.51000000000000023,0.76]
["GGU CK02 57 Flush","GGU","CK02",57,"MANUAL","Flush","GGU 57","GPU 70","ok","GPU","70","GPU CK02 70 Flush",57,1.6,1.9,1.4,1.7,1.3,1.5,1.3,1.5,1.7,1.3,1.1000000000000001,1.2,0.11,0.05,0,0.11,0.06,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.31,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGU CK02 62 Flush","GGU","CK02","62","ELECTRIC","Flush","GGU 62","GPU 62","ok","GPU","62","GPU CK02 62 Flush","62",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.94,1,0.19,7.0000000000000007E-2,0,0.19,0.08,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGU CK02 70Q Flush","GGU","CK02","70Q","MANUAL","Flush","GGU 70Q","GPU 70","ok","GPU","70","GPU CK02 70 Flush",70,1.6,1.9,1.4,1.7,1.3,1.5,1.3,1.5,1.7,1.3,1.1000000000000001,1.2,0.19,0.06,0,0.19,0.06,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.55000000000000004,0.78,0.43,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.51]
["GGU CK04 62 Flush","GGU","CK04","62","MANUAL","Flush","GGU 62","GPU 62","ok","GPU","62","GPU CK04 62 Flush","62",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.2,1.3,1.1000000000000001,0.93,1,0.2,7.0000000000000007E-2,0,0.2,0.08,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGU CK04 66 Flush","GGU","CK04","66","ELECTRIC","Flush","GGU 66","GPU 66","ok","GPU","66","GPU CK04 66 Flush","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.98,1,0.16,0.08,0,0.16,0.08,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGU CK04 70 Flush","GGU","CK04","70","MANUAL","Flush","GGU 70","GPU 70","ok","GPU","70","GPU CK04 70 Flush","70",1.5,1.9,1.4,1.7,1.3,1.5,1.3,1.5,1.7,1.3,1.1000000000000001,1.2,0.2,0.06,0,0.2,0.06,0,0.04,0.1,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GGU CK06 62 Flush","GGU","CK06","62","ELECTRIC","Flush","GGU 62","GPU 62","ok","GPU","62","GPU CK06 62 Flush","62",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.92,1,0.21,0.08,0,0.21,0.08,0,0.04,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.55000000000000004,1.18,0.65,0.37000000000000005,0.98,2.71,0.36,0.29000000000000004,0.55000000000000004]
["GGU FK04 62 Flush","GGU","FK04","62","ELECTRIC","Flush","GGU 62","GPU 62","ok","GPU","62","GPU FK04 62 Flush","62",1.2,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.98,1.1000000000000001,1.2,1,0.88,0.98,0.22,0.08,0,0.22,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.66,0.98,0.65,0.48000000000000004,0.78,2.5299999999999998,0.38,0.27,0.57999999999999996]
["GGU FK04 66 Flush","GGU","FK04","66","ELECTRIC","Flush","GGU 66","GPU 66","ok","GPU","66","GPU FK04 66 Flush","66",1.2,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.93,1,0.17,0.08,0,0.17,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.66,0.98,0.65,0.48000000000000004,0.78,2.5299999999999998,0.38,0.27,0.57999999999999996]
["GGU FK06 62 Flush","GGU","FK06","62","ELECTRIC","Flush","GGU 62","GPU 62","ok","GPU","62","GPU FK06 62 Flush","62",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.97,1.1000000000000001,1.2,1,0.87,0.97,0.22,0.08,0,0.22,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GGU FK06 76F Flush","GGU","FK06","76F","MANUAL","Flush","GGU 76F","GPU 70","ok","GPU","70","GPU FK06 70 Flush","76",1.5,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1.1000000000000001,1.2,0.13,0.05,0,0.13,0.05,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GGU FK08 66 Flush","GGU","FK08","66","SOLAR","Flush","GGU 66","GPU 66","ok","GPU","66","GPU FK08 66 Flush","66",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.91,0.99,0.19,0.08,0,0.19,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.66,1.4,0.92,0.48000000000000004,1.2,3.37,0.57999999999999996,0.34000000000000008,0.63]
["GGU MK04 57 Flush","GGU","MK04",57,"MANUAL","Flush","GGU 57","GPU 70","ok","GPU","70","GPU MK04 70 Flush",57,1.4,1.8,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.13,0.05,0,0.13,0.06,0,0.02,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGU MK04 62 Flush","GGU","MK04","62","ELECTRIC","Flush","GGU 62","GPU 62","ok","GPU","62","GPU MK04 62 Flush","62",1.1000000000000001,1.3,1,1.2,0.97,1.1000000000000001,0.94,1.1000000000000001,1.2,1,0.84,0.95,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGU MK04 70Q Flush","GGU","MK04","70Q","MANUAL","Flush","GGU 70Q","GPU 70","ok","GPU","70","GPU MK04 70 Flush",70,1.4,1.8,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.23,0.06,0,0.23,0.06,0,0.04,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GGU MK06 57 Flush","GGU","MK06",57,"SOLAR","Flush","GGU 57","GPU 70","ok","GPU","70","GPU MK06 70 Flush",57,1.4,1.8,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.13,0.05,0,0.13,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGU MK06 62 Flush","GGU","MK06","62","MANUAL","Flush","GGU 62","GPU 62","ok","GPU","62","GPU MK06 62 Flush","62",1.1000000000000001,1.3,1,1.2,0.95,1.1000000000000001,0.92,1.1000000000000001,1.2,0.99,0.83,0.94,0.24,0.08,0,0.24,0.08,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGU MK06 70 Flush","GGU","MK06","70","MANUAL","Flush","GGU 70","GPU 70","ok","GPU","70","GPU MK06 70 Flush","70",1.4,1.8,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.24,0.06,0,0.24,0.06,0,0.04,0.09,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GGU MK08 57 Flush","GGU","MK08",57,"MANUAL","Flush","GGU 57","GPU 70","ok","GPU","70","GPU MK08 70 Flush",57,1.4,1.8,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGU MK08 66 Flush","GGU","MK08","66","MANUAL","Flush","GGU 66","GPU 66","ok","GPU","66","GPU MK08 66 Flush","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.97,1.1000000000000001,1.2,1,0.87,0.97,0.2,0.08,0,0.2,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGU MK08 66 Flush","GGU","MK08","66","ELECTRIC","Flush","GGU 66","GPU 66","ok","GPU","66","GPU MK08 66 Flush","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.97,1.1000000000000001,1.2,1,0.87,0.97,0.2,0.08,0,0.2,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGU MK08 76F Flush","GGU","MK08","76F","MANUAL","Flush","GGU 76F","GPU 70","ok","GPU","70","GPU MK08 70 Flush","76",1.4,1.8,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GGU MK10 66 Flush","GGU","MK10","66","ELECTRIC","Flush","GGU 66","GPU 66","ok","GPU","66","GPU MK10 66 Flush","66",1.1000000000000001,1.3,1.1000000000000001,1.2,0.99,1.1000000000000001,0.96,1.1000000000000001,1.2,1,0.86,0.96,0.2,0.09,0,0.2,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GGU PK06 57 Flush","GGU","PK06",57,"ELECTRIC","Flush","GGU 57","GPU 70","ok","GPU","70","GPU PK06 70 Flush",57,1.4,1.8,1.3,1.6,1.2,1.5,1.1000000000000001,1.4,1.6,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGU PK06 57 Flush","GGU","PK06",57,"SOLAR","Flush","GGU 57","GPU 70","ok","GPU","70","GPU PK06 70 Flush",57,1.4,1.8,1.3,1.6,1.2,1.5,1.1000000000000001,1.4,1.6,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGU PK06 66 Flush","GGU","PK06","66","SOLAR","Flush","GGU 66","GPU 66","ok","GPU","66","GPU PK06 66 Flush","66",1.1000000000000001,1.3,1,1.2,0.97,1.1000000000000001,0.94,1.1000000000000001,1.2,1,0.84,0.95,0.2,0.08,0,0.2,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GGU PK08 57 Flush","GGU","PK08",57,"MANUAL","Flush","GGU 57","GPU 70","ok","GPU","70","GPU PK08 70 Flush",57,1.4,1.8,1.3,1.6,1.2,1.5,1.1000000000000001,1.4,1.6,1.3,0.99,1.2,0.15,0.05,0,0.15,0.06,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGU PK08 66 Flush","GGU","PK08","66","MANUAL","Flush","GGU 66","GPU 66","ok","GPU","66","GPU PK08 66 Flush","66",1.1000000000000001,1.3,1,1.2,0.96,1.1000000000000001,0.93,1.1000000000000001,1.2,1,0.84,0.94,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGU PK08 66 Flush","GGU","PK08","66","ELECTRIC","Flush","GGU 66","GPU 66","ok","GPU","66","GPU PK08 66 Flush","66",1.1000000000000001,1.3,1,1.2,0.96,1.1000000000000001,0.93,1.1000000000000001,1.2,1,0.84,0.94,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GGU PK10 57 Flush","GGU","PK10",57,"MANUAL","Flush","GGU 57","GPU 70","ok","GPU","70","GPU PK10 70 Flush",57,1.3,1.8,1.2,1.6,1.2,1.5,1.1000000000000001,1.4,1.6,1.3,0.99,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.71]
["GGU PK10 62 Flush","GGU","PK10","62","MANUAL","Flush","GGU 62","GPU 62","ok","GPU","62","GPU PK10 62 Flush","62",0.97,1.2,0.92,1.1000000000000001,0.87,1,0.85,1,1.1000000000000001,0.95,0.77,0.89,0.27,0.08,0,0.27,0.09,0,0.05,7.0000000000000007E-2,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.71]
["GGU PK10 70Q Flush","GGU","PK10","70Q","MANUAL","Flush","GGU 70Q","GPU 70","ok","GPU","70","GPU PK10 70 Flush",70,1.3,1.8,1.2,1.6,1.2,1.5,1.1000000000000001,1.4,1.6,1.3,0.99,1.2,0.27,7.0000000000000007E-2,0,0.27,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.71]
["GGU PK10 76F Flush","GGU","PK10","76F","MANUAL","Flush","GGU 76F","GPU 70","ok","GPU","70","GPU PK10 70 Flush","76",1.3,1.8,1.2,1.6,1.2,1.5,1.1000000000000001,1.4,1.6,1.3,0.99,1.2,0.15,0.05,0,0.15,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.71]
["GGU SK06 62 Flush","GGU","SK06","62","ELECTRIC","Flush","GGU 62","GPU 62","ok","GPU","62","GPU SK06 62 Flush","62",0.96,1.2,0.9,1.1000000000000001,0.86,1,0.84,0.99,1.1000000000000001,0.94,0.76,0.89,0.26,0.08,0,0.26,0.09,0,0.05,7.0000000000000007E-2,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGU SK06 70Q Flush","GGU","SK06","70Q","MANUAL","Flush","GGU 70Q","GPU 70","ok","GPU","70","GPU SK06 70 Flush",70,1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.98,1.2,0.27,0.06,0,0.27,0.06,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GGU SK08 57 Flush","GGU","SK08",57,"ELECTRIC","Flush","GGU 57","GPU 70","ok","GPU","70","GPU SK08 70 Flush",57,1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.97,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGU SK08 57 Flush","GGU","SK08",57,"SOLAR","Flush","GGU 57","GPU 70","ok","GPU","70","GPU SK08 70 Flush",57,1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.97,1.2,0.15,0.05,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGU SK08 70 Flush","GGU","SK08","70","MANUAL","Flush","GGU 70","GPU 70","ok","GPU","70","GPU SK08 70 Flush","70",1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.97,1.2,0.28000000000000003,7.0000000000000007E-2,0,0.28000000000000003,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.49,0,0.09,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGU SK08 76F Flush","GGU","SK08","76F","ELECTRIC","Flush","GGU 76F","GPU 70","ok","GPU","70","GPU SK08 70 Flush","76",1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.97,1.2,0.15,0.05,0,0.15,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.45,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GGU UK04 57 Flush","GGU","UK04",57,"SOLAR","Flush","GGU 57","GPU 70","ok","GPU","70","GPU UK04 70 Flush",57,1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.98,1.2,0.15,0.05,0,0.15,0.06,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGU UK04 66 Flush","GGU","UK04","66","MANUAL","Flush","GGU 66","GPU 66","ok","GPU","66","GPU UK04 66 Flush","66",1.1000000000000001,1.2,0.99,1.2,0.93,1.1000000000000001,0.91,1,1.2,0.99,0.82,0.93,0.21,0.08,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGU UK04 76F Flush","GGU","UK04","76F","MANUAL","Flush","GGU 76F","GPU 70","ok","GPU","70","GPU UK04 70 Flush","76",1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.98,1.2,0.15,0.05,0,0.15,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GGU UK08 66 Flush","GGU","UK08","66","MANUAL","Flush","GGU 66","GPU 66","ok","GPU","66","GPU UK08 66 Flush","66",0.99,1.2,0.94,1.1000000000000001,0.89,1,0.86,1,1.1000000000000001,0.96,0.78,0.91,0.22,0.09,0,0.22,0.1,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGU UK08 70Q Flush","GGU","UK08","70Q","MANUAL","Flush","GGU 70Q","GPU 70","ok","GPU","70","GPU UK08 70 Flush",70,1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.96,1.2,0.28000000000000003,7.0000000000000007E-2,0,0.28000000000000003,7.0000000000000007E-2,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.51,0,0.09,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GGU UK08 76F Flush","GGU","UK08","76F","MANUAL","Flush","GGU 76F","GPU 70","ok","GPU","70","GPU UK08 70 Flush","76",1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.96,1.2,0.16,0.05,0,0.16,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GIL MK34 57 Flush","GIL","MK34","57","FIXED","Flush","GIL 57","GPL 70","ok","GPL","70","GPL MK34 70 Flush","57",1.4,1.8,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.13,0.05,0,0.13,0.06,0,0.02,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,0.92,0.72,0.60000000000000009,0.73,2.65,0.44,0.27999999999999997,0.61]
["GIL PK34 62 Flush","GIL","PK34","62","FIXED","Flush","GIL 62","VFE 62","ok","VFE","62","VFE PK34 62 Flush","62",1.1000000000000001,1.2,0.99,1.2,0.93,1.1000000000000001,0.91,1,1.2,0.99,0.82,0.93,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,0.92,0.87,0.76200000000000001,0.73,2.98,0.56000000000000005,0.30999999999999994,0.64]
["GIL PK34 70 Flush","GIL","PK34","70","FIXED","Flush","GIL 70","GPL 70","ok","GPL","70","GPL PK34 70 Flush","70",1.4,1.8,1.3,1.6,1.2,1.5,1.1000000000000001,1.4,1.6,1.3,1,1.2,0.24,0.06,0,0.24,0.06,0,0.04,0.09,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,0.92,0.87,0.76200000000000001,0.73,2.98,0.56000000000000005,0.30999999999999994,0.64]
["GIL SK34 66 Flush","GIL","SK34","66","FIXED","Flush","GIL 66","GPL 66","ok","GPL","66","GPL SK34 66 Flush","66",1.1000000000000001,1.3,1,1.2,0.95,1.1000000000000001,0.92,1.1000000000000001,1.2,1,0.83,0.95,0.2,0.08,0,0.2,0.09,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.1399999999999999,0.92,1.05,0.96,0.73,3.37,0.7,0.35000000000000009,0.67]
["GIU FK34 62 Flush","GIU","FK34","62","FIXED","Flush","GIU 62","GIU 62","ok","GIU","62","GIU FK34 62 Flush","62",1.2,1.4,1.1000000000000001,1.3,1,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.9,1,0.22,0.08,0,0.22,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.66,0.92,0.61,0.48000000000000004,0.73,2.41,0.35,0.26,0.56999999999999995]
["GIU PK34 57 Flush","GIU","PK34","57","FIXED","Flush","GIU 57","GPU 70","ok","GPU","70","GPU PK34 70 Flush","57",1.4,1.8,1.3,1.6,1.2,1.5,1.1000000000000001,1.4,1.6,1.3,1,1.2,0.13,0.05,0,0.13,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,0.92,0.87,0.76200000000000001,0.73,2.97,0.55000000000000004,0.31999999999999995,0.63]
["GIU SK34 62 Flush","GIU","SK34","62","FIXED","Flush","GIU 62","GIU 62","ok","GIU","62","GIU SK34 62 Flush","62",1,1.2,0.97,1.1000000000000001,0.92,1.1000000000000001,0.89,1,1.1000000000000001,0.98,0.81,0.92,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.1399999999999999,0.92,1.05,0.96,0.73,3.37,0.7,0.35000000000000009,0.67]
["GIU SK34 66 Flush","GIU","SK34","66","FIXED","Flush","GIU 66","GPU 66","ok","GPU","66","GPU SK34 66 Flush","66",1.1000000000000001,1.3,1,1.2,0.96,1.1000000000000001,0.93,1.1000000000000001,1.2,1,0.84,0.95,0.2,0.08,0,0.2,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.1399999999999999,0.92,1.05,0.96,0.73,3.37,0.7,0.35000000000000009,0.67]
["GPL CK04 66 Flush","GPL","CK04","66","MANUAL","Flush","GPL 66","GPL 66","ok","GPL","66","GPL CK04 66 Flush","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.96,1,0.16,0.08,0,0.16,0.08,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GPL FK06 76F Flush","GPL","FK06","76F","MANUAL","Flush","GPL 76F","GPL 70","ok","GPL","70","GPL FK06 70 Flush","76",1.4,1.9,1.3,1.7,1.2,1.5,1.2,1.5,1.7,1.3,1,1.2,0.13,0.05,0,0.13,0.05,0,0.02,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.38,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GPL MK04 66 Flush","GPL","MK04","66","MANUAL","Flush","GPL 66","GPL 66","ok","GPL","66","GPL MK04 66 Flush","66",1.2,1.3,1.1000000000000001,1.2,1,1.2,0.99,1.1000000000000001,1.2,1,0.88,0.99,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GPL MK04 70 Flush","GPL","MK04","70","MANUAL","Flush","GPL 70","GPL 70","ok","GPL","70","GPL MK04 70 Flush","70",1.4,1.8,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.23,0.06,0,0.23,0.06,0,0.04,0.09,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GPL MK08 57 Flush","GPL","MK08",57,"MANUAL","Flush","GPL 57","GPL 70","ok","GPL","70","GPL MK08 70 Flush",57,1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",422,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GPL MK10 70 Flush","GPL","MK10","70","MANUAL","Flush","GPL 70","GPL 70","ok","GPL","70","GPL MK10 70 Flush","70",1.4,1.8,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.7,1.3,1,1.2,0.26,0.06,0,0.26,0.06,0,0.05,0.09,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GPL PK06 76F Flush","GPL","PK06","76F","MANUAL","Flush","GPL 76F","GPL 70","ok","GPL","70","GPL PK06 70 Flush","76",1.3,1.8,1.2,1.6,1.2,1.5,1.1000000000000001,1.4,1.6,1.3,0.99,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",422,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GPL PK08 57 Flush","GPL","PK08",57,"MANUAL","Flush","GPL 57","GPL 70","ok","GPL","70","GPL PK08 70 Flush",57,1.3,1.8,1.2,1.6,1.2,1.5,1.1000000000000001,1.4,1.6,1.3,0.98,1.2,0.15,0.05,0,0.15,0.06,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",422,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GPL SK06 57 Flush","GPL","SK06",57,"MANUAL","Flush","GPL 57","GPL 70","ok","GPL","70","GPL SK06 70 Flush",57,1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.97,1.2,0.15,0.05,0,0.15,0.06,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",422,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GPL SK08 66 Flush","GPL","SK08","66","MANUAL","Flush","GPL 66","GPL 66","ok","GPL","66","GPL SK08 66 Flush","66",1,1.2,0.95,1.1000000000000001,0.9,1.1000000000000001,0.88,1,1.1000000000000001,0.97,0.79,0.92,0.22,0.09,0,0.22,0.09,0,0.04,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GPL UK04 57 Flush","GPL","UK04",57,"MANUAL","Flush","GPL 57","GPL 70","ok","GPL","70","GPL UK04 70 Flush",57,1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.97,1.2,0.15,0.05,0,0.15,0.06,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",422,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GPL UK04 76F Flush","GPL","UK04","76F","MANUAL","Flush","GPL 76F","GPL 70","ok","GPL","70","GPL UK04 70 Flush","76",1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.97,1.2,0.15,0.05,0,0.15,0.05,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",422,1.34,0.98,1.31,1.1600000000000001,0.78,3.89,0.91,0.4,0.69]
["GPL UK08 70 Flush","GPL","UK08","70","MANUAL","Flush","GPL 70","GPL 70","ok","GPL","70","GPL UK08 70 Flush","70",1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.95,1.2,0.28000000000000003,0.06,0,0.28000000000000003,0.06,0,0.05,0.08,0,0.14000000000000001,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.51,0,0.09,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GPU CK04 76F Flush","GPU","CK04","76F","MANUAL","Flush","GPU 76F","GPU 70","ok","GPU","70","GPU CK04 70 Flush","76",1.5,1.9,1.4,1.7,1.3,1.5,1.3,1.5,1.7,1.3,1.1000000000000001,1.2,0.11,0.05,0,0.11,0.05,0,0.02,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.33,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,0.55000000000000004,0.98,0.54,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.54]
["GPU FK06 66 Flush","GPU","FK06","66","ELECTRIC","Flush","GPU 66","GPU 66","ok","GPU","66","GPU FK06 66 Flush","66",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.92,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["GPU FK08 62 Flush","GPU","FK08","62","MANUAL","Flush","GPU 62","GPU 62","ok","GPU","62","GPU FK08 62 Flush","62",1.1000000000000001,1.3,1,1.2,0.98,1.1000000000000001,0.96,1.1000000000000001,1.2,1,0.86,0.96,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.66,1.4,0.92,0.48000000000000004,1.2,3.37,0.57999999999999996,0.34000000000000008,0.63]
["GPU MK04 62 Flush","GPU","MK04","62","MANUAL","Flush","GPU 62","GPU 62","ok","GPU","62","GPU MK04 62 Flush","62",1.1000000000000001,1.3,1,1.2,0.97,1.1000000000000001,0.94,1.1000000000000001,1.2,1,0.84,0.95,0.23,0.08,0,0.23,0.08,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,0.98,0.76,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.62]
["GPU MK06 62 Flush","GPU","MK06","62","MANUAL","Flush","GPU 62","GPU 62","ok","GPU","62","GPU MK06 62 Flush","62",1.1000000000000001,1.3,1,1.2,0.95,1.1000000000000001,0.92,1.1000000000000001,1.2,0.99,0.83,0.94,0.24,0.08,0,0.24,0.08,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,1.18,0.92,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.64]
["GPU MK08 57 Flush","GPU","MK08",57,"ELECTRIC","Flush","GPU 57","GPU 70","ok","GPU","70","GPU MK08 70 Flush",57,1.4,1.8,1.3,1.7,1.2,1.5,1.2,1.4,1.7,1.3,1,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GPU MK08 66 Flush","GPU","MK08","66","MANUAL","Flush","GPU 66","GPU 66","ok","GPU","66","GPU MK08 66 Flush","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.97,1.1000000000000001,1.2,1,0.87,0.97,0.2,0.08,0,0.2,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,1.4,1.0900000000000001,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.66]
["GPU MK10 62 Flush","GPU","MK10","62","MANUAL","Flush","GPU 62","GPU 62","ok","GPU","62","GPU MK10 62 Flush","62",1,1.2,0.97,1.1000000000000001,0.92,1.1000000000000001,0.9,1,1.1000000000000001,0.98,0.81,0.93,0.25,0.08,0,0.25,0.09,0,0.04,0.08,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,1.6,1.25,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.67]
["GPU PK06 62 Flush","GPU","PK06","62","MANUAL","Flush","GPU 62","GPU 62","ok","GPU","62","GPU PK06 62 Flush","62",1,1.2,0.94,1.1000000000000001,0.89,1,0.87,1,1.1000000000000001,0.96,0.79,0.91,0.25,0.08,0,0.25,0.09,0,0.04,7.0000000000000007E-2,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,1.18,1.1100000000000001,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.68]
["GPU PK08 62 Flush","GPU","PK08","62","MANUAL","Flush","GPU 62","GPU 62","ok","GPU","62","GPU PK08 62 Flush","62",0.98,1.2,0.93,1.1000000000000001,0.88,1,0.86,1,1.1000000000000001,0.95,0.78,0.9,0.26,0.08,0,0.26,0.09,0,0.04,7.0000000000000007E-2,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GPU PK08 66 Flush","GPU","PK08","66","MANUAL","Flush","GPU 66","GPU 66","ok","GPU","66","GPU PK08 66 Flush","66",1.1000000000000001,1.3,1,1.2,0.96,1.1000000000000001,0.93,1.1000000000000001,1.2,1,0.84,0.94,0.21,0.09,0,0.21,0.09,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,1.4,1.32,0.76200000000000001,1.2,3.93,0.92,0.4,0.7]
["GPU PK10 62 Flush","GPU","PK10","62","MANUAL","Flush","GPU 62","GPU 62","ok","GPU","62","GPU PK10 62 Flush","62",0.97,1.2,0.92,1.1000000000000001,0.87,1,0.85,1,1.1000000000000001,0.95,0.77,0.89,0.27,0.08,0,0.27,0.09,0,0.05,7.0000000000000007E-2,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.48,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,1.6,1.51,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.71]
["GPU SK06 66 Flush","GPU","SK06","66","MANUAL","Flush","GPU 66","GPU 66","ok","GPU","66","GPU SK06 66 Flush","66",1.1000000000000001,1.2,0.99,1.2,0.93,1.1000000000000001,0.91,1,1.2,0.99,0.82,0.93,0.21,0.09,0,0.21,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.1399999999999999,1.18,1.34,0.96,0.98,3.89,0.94,0.40000000000000013,0.7]
["GPU SK08 62 Flush","GPU","SK08","62","MANUAL","Flush","GPU 62","GPU 62","ok","GPU","62","GPU SK08 62 Flush","62",0.93,1.1000000000000001,0.88,1.1000000000000001,0.84,1,0.82,0.98,1.1000000000000001,0.92,0.74,0.88,0.27,0.08,0,0.27,0.09,0,0.05,7.0000000000000007E-2,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.49,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GPU SK08 66 Flush","GPU","SK08","66","ELECTRIC","Flush","GPU 66","GPU 66","ok","GPU","66","GPU SK08 66 Flush","66",1,1.2,0.97,1.1000000000000001,0.91,1.1000000000000001,0.89,1,1.1000000000000001,0.97,0.8,0.92,0.22,0.09,0,0.22,0.09,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GPU UK08 57 Flush","GPU","UK08","57","MANUAL","Flush","GPU 57","GPU 70","ok","GPU","70","GPU UK08 70 Flush","57",1.3,1.8,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1.6,1.3,0.96,1.2,0.16,0.05,0,0.16,7.0000000000000007E-2,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.46,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,1.34,1.4,1.87,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.74]
["GTL SK08 66 Flush","GTL","SK08","66","MANUAL","Flush","GTL 66","GPL 66","ok","GPL","66","GPL SK08 66 Flush","66",1,1.2,0.95,1.1000000000000001,0.9,1.1000000000000001,0.88,1,1.1000000000000001,0.97,0.79,0.92,0.22,0.09,0,0.22,0.09,0,0.04,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.1399999999999999,1.4,1.59,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.72]
["GXU CK06 66 Flush","GXU","CK06","66","MANUAL","Flush","GXU 66","GPU 66","ok","GPU","66","GPU CK06 66 Flush","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.97,1,0.17,0.08,0,0.17,0.09,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.55000000000000004,1.18,0.65,0.37000000000000005,0.98,2.71,0.36,0.29000000000000004,0.55000000000000004]
["GXU FK06 66 Flush","GXU","FK06","66","MANUAL","Flush","GXU 66","GPU 66","ok","GPU","66","GPU FK06 66 Flush","66",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.92,1,0.18,0.08,0,0.18,0.09,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.66,1.18,0.78,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.6]
["VFE MK31 70 Flush","VFE","MK31","70","MANUAL","Flush","VFE 70","GPL 70","ok","GPL","70","GPL MK31 70 Flush","70",1.5,1.8,1.4,1.7,1.3,1.5,1.2,1.4,1.7,1.3,1.1000000000000001,1.2,0.2,0.06,0,0.2,0.06,0,0.04,0.1,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,0.6,0.47,0.60000000000000009,0.41,2.0099999999999998,0.24,0.22999999999999998,0.51]
["VFE PK31 62 Flush","VFE","PK31","62","MANUAL","Flush","VFE 62","VFE 62","ok","VFE","62","VFE PK31 62 Flush","62",1.2,1.3,1.1000000000000001,1.2,1,1.2,1,1.1000000000000001,1.2,1,0.9,0.98,0.19,7.0000000000000007E-2,0,0.19,7.0000000000000007E-2,0,0.03,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,0.6,0.56999999999999995,0.76200000000000001,0.41,2.34,0.31,0.25999999999999995,0.54]
["VFE PK35 66 Flush","VFE","PK35","66","MANUAL","Flush","VFE 66","GPL 66","ok","GPL","66","GPL PK35 66 Flush","66",1.1000000000000001,1.3,1,1.2,0.98,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.85,0.96,0.19,0.08,0,0.19,0.09,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,0.95,0.9,0.76200000000000001,0.76,3.04,0.57999999999999996,0.32000000000000006,0.64]
["VFE PK35 70 Flush","VFE","PK35","70","MANUAL","Flush","VFE 70","GPL 70","ok","GPL","70","GPL PK35 70 Flush","70",1.4,1.8,1.3,1.6,1.2,1.5,1.1000000000000001,1.4,1.6,1.3,1,1.2,0.24,0.06,0,0.24,0.06,0,0.04,0.09,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,0.95,0.9,0.76200000000000001,0.76,3.04,0.57999999999999996,0.32000000000000006,0.64]
["VFE SK35 62 Flush","VFE","SK35","62","MANUAL","Flush","VFE 62","VFE 62","ok","VFE","62","VFE SK35 62 Flush","62",1,1.2,0.95,1.1000000000000001,0.9,1.1000000000000001,0.87,1,1.1000000000000001,0.96,0.79,0.91,0.24,0.08,0,0.24,0.08,0,0.04,7.0000000000000007E-2,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.44,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.1399999999999999,0.95,1.0900000000000001,0.96,0.76,3.44,0.73,0.3600000000000001,0.67]
["VFE UK31 57 Flush","VFE","UK31","57","MANUAL","Flush","VFE 57","GPL 70","ok","GPL","70","GPL UK31 70 Flush","57",1.4,1.8,1.3,1.6,1.2,1.5,1.2,1.4,1.6,1.3,1,1.2,0.12,0.05,0,0.12,0.06,0,0.02,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.34,0.6,0.8,1.1600000000000001,0.41,3.13,0.47,0.33000000000000007,0.59]
["VFE UK35 62 Flush","VFE","UK35","62","MANUAL","Flush","VFE 62","VFE 62","ok","VFE","62","VFE UK35 62 Flush","62",0.98,1.2,0.92,1.1000000000000001,0.87,1,0.85,1,1.1000000000000001,0.94,0.77,0.89,0.25,0.08,0,0.25,0.08,0,0.04,7.0000000000000007E-2,0,0.12,0,0.05,0,0.05,0,0.05,0,0.05,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.34,0.95,1.28,1.1600000000000001,0.76,3.84,0.88,0.4,0.69]
["VFE UK35 66 Flush","VFE","UK35","66","MANUAL","Flush","VFE 66","GPL 66","ok","GPL","66","GPL UK35 66 Flush","66",1,1.2,0.98,1.2,0.92,1.1000000000000001,0.9,1,1.2,0.99,0.81,0.93,0.21,0.08,0,0.21,0.09,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.34,0.95,1.28,1.1600000000000001,0.76,3.84,0.88,0.4,0.69]
["VIU MK31 66 Flush","VIU","MK31","66","FIXED","Flush","VIU 66","GPU 66","ok","GPU","66","GPU MK31 66 Flush","66",1.3,1.4,1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.2,1.3,1.1000000000000001,0.96,1,0.16,0.08,0,0.16,0.08,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.32,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.78,0.6,0.47,0.60000000000000009,0.41,2.0099999999999998,0.24,0.22999999999999998,0.51]
["VIU PK31 62 Flush","VIU","PK31","62","FIXED","Flush","VIU 62","GIU 62","ok","GIU","62","GIU PK31 62 Flush","62",1.2,1.4,1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,1.3,1.1000000000000001,0.91,1,0.21,0.08,0,0.21,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.38,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.94199999999999995,0.6,0.56999999999999995,0.76200000000000001,0.41,2.33,0.31,0.25999999999999995,0.54]
["VIU SK31 57 Flush","VIU","SK31","57","FIXED","Flush","VIU 57","GPU 70","ok","GPU","70","GPU SK31 70 Flush","57",1.4,1.8,1.3,1.6,1.2,1.5,1.2,1.4,1.6,1.3,1,1.2,0.12,0.05,0,0.12,0.06,0,0.02,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.1399999999999999,0.6,0.68,0.96,0.41,2.73,0.39,0.29000000000000004,0.56999999999999995]
["VIU SK31 62 Flush","VIU","SK31","62","FIXED","Flush","VIU 62","GIU 62","ok","GIU","62","GIU SK31 62 Flush","62",1.2,1.3,1.1000000000000001,1.2,1,1.2,0.99,1.1000000000000001,1.2,1,0.89,0.98,0.22,0.08,0,0.22,0.08,0,0.04,0.08,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.1399999999999999,0.6,0.68,0.96,0.41,2.73,0.39,0.29000000000000004,0.56999999999999995]
["VIU UK31 66 Flush","VIU","UK31","66","FIXED","Flush","VIU 66","GPU 66","ok","GPU","66","GPU UK31 66 Flush","66",1.2,1.3,1.1000000000000001,1.2,1,1.2,1,1.1000000000000001,1.2,1,0.9,0.99,0.18,0.08,0,0.18,0.08,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,0.06,0,0.06,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.34,0.6,0.8,1.1600000000000001,0.41,3.13,0.47,0.33000000000000007,0.59]
["GFL CK02 54F Flush + BDX","GFL","CK02","54F","MANUAL","Flush + BDX","GFL 54F","GFL 54F","ok","GFL","54F","GFL CK02 54F Flush + BDX","54F",1.3,1.6,1.2,1.4,1.2,1.3,1.1000000000000001,1.3,1.4,1.2,0.98,1.1000000000000001,0.23,0.04,0,0.23,0.04,0,0.04,0.09,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.33,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.6120000000000001,0.88,0.54,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.41]
["GFL SK06 54F Flush + BDX","GFL","SK06","54F","MANUAL","Flush + BDX","GFL 54F","GFL 54F","ok","GFL","54F","GFL SK06 54F Flush + BDX","54F",1.2,1.6,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.93,1.1000000000000001,0.35,0.05,0,0.35,0.05,0,0.06,0.08,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.5,0,0.09,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GFL SK08 54F Flush + BDX","GFL","SK08","54F","MANUAL","Flush + BDX","GFL 54F","GFL 54F","ok","GFL","54F","GFL SK08 54F Flush + BDX","54F",1.2,1.6,1.2,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.93,1.1000000000000001,0.36,0.05,0,0.36,0.05,0,0.06,0.08,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.53,0,0.09,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GGL CK01 76F Flush + BDX","GGL","CK01","76F","MANUAL","Flush + BDX","GGL 76F","GPL 70","ok","GPL","70","GPL CK01 70 Flush + BDX","76",1.4,1.6,1.3,1.5,1.2,1.4,1.1000000000000001,1.3,1.5,1.2,1,1.1000000000000001,0.08,0.04,0,0.08,0.04,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.24,0,0.04,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.6120000000000001,0.8,0.49,0.37000000000000005,0.5,1.75,0.18,0.2,0.37]
["GGL CK02 62 Flush + BDX","GGL","CK02","62","MANUAL","Flush + BDX","GGL 62","GPL 62","ok","GPL","62","GPL CK02 62 Flush + BDX","62",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.98,1.1000000000000001,1.2,1,0.88,0.94,0.15,0.06,0,0.15,7.0000000000000007E-2,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.27,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,0.88,0.54,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.41]
["GGL CK02 70 Flush + BDX","GGL","CK02","70","MANUAL","Flush + BDX","GGL 70","GPL 70","ok","GPL","70","GPL CK02 70 Flush + BDX","70",1.4,1.6,1.3,1.5,1.2,1.4,1.1000000000000001,1.3,1.5,1.2,1,1.1000000000000001,0.15,0.05,0,0.15,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.28000000000000003,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,0.88,0.54,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.41]
["GGL CK02 70 Flush + BDX","GGL","CK02","70","MANUALBOTTOM","Flush + BDX","GGL 70","GPL 70","ok","GPL","70","GPL CK02 70 Flush + BDX","70",1.4,1.6,1.3,1.5,1.2,1.4,1.1000000000000001,1.3,1.5,1.2,1,1.1000000000000001,0.15,0.05,0,0.15,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.28000000000000003,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,0.88,0.54,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.41]
["GGL CK04 54F Flush + BDX","GGL","CK04","54F","MANUAL","Flush + BDX","GGL 54F","GPL 54F","ok","GPL","54F","GPL CK04 54F Flush + BDX","54F",1.4,1.7,1.3,1.5,1.2,1.4,1.2,1.4,1.5,1.2,1,1.2,0.25,0.05,0,0.25,0.05,0,0.04,0.09,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.36,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GGL CK04 66 Flush + BDX","GGL","CK04","66","MANUAL","Flush + BDX","GGL 66","GPL 66","ok","GPL","66","GPL CK04 66 Flush + BDX","66",1.2,1.3,1.1000000000000001,1.2,1,1.1000000000000001,1,1.1000000000000001,1.2,1,0.9,0.97,0.13,7.0000000000000007E-2,0,0.13,7.0000000000000007E-2,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.27,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GGL CK04 70Q Flush + BDX","GGL","CK04","70Q","MANUAL","Flush + BDX","GGL 70Q","GPL 70","ok","GPL","70","GPL CK04 70 Flush + BDX",70,1.4,1.7,1.3,1.5,1.2,1.4,1.1000000000000001,1.3,1.5,1.2,1,1.2,0.17,0.05,0,0.17,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.3,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GGL CK04 76F Flush + BDX","GGL","CK04","76F","MANUAL","Flush + BDX","GGL 76F","GPL 70","ok","GPL","70","GPL CK04 70 Flush + BDX","76",1.4,1.7,1.3,1.5,1.2,1.4,1.1000000000000001,1.3,1.5,1.2,1,1.2,0.09,0.05,0,0.09,0.05,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.27,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GGL CK06 66 Flush + BDX","GGL","CK06","66","MANUAL","Flush + BDX","GGL 66","GPL 66","ok","GPL","66","GPL CK06 66 Flush + BDX","66",1.2,1.3,1.1000000000000001,1.2,1,1.1000000000000001,1,1.1000000000000001,1.2,1,0.89,0.97,0.14000000000000001,7.0000000000000007E-2,0,0.14000000000000001,7.0000000000000007E-2,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.28999999999999998,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,1.28,0.78,0.37000000000000005,0.98,2.71,0.37,0.28000000000000003,0.47]
["GGL CK06 70H Flush + BDX","GGL","CK06","70H","MANUAL","Flush + BDX","GGL 70H","GPL 70","ok","GPL","70","GPL CK06 70 Flush + BDX",70,1.4,1.7,1.3,1.5,1.2,1.4,1.1000000000000001,1.3,1.5,1.2,1,1.2,0.18,0.06,0,0.18,0.06,0,0.03,0.09,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.32,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,1.28,0.78,0.37000000000000005,0.98,2.71,0.37,0.28000000000000003,0.47]
["GGL FK04 70Q Flush + BDX","GGL","FK04","70Q","MANUAL","Flush + BDX","GGL 70Q","GPL 70","ok","GPL","70","GPL FK04 70 Flush + BDX",70,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.98,1.1000000000000001,0.19,0.06,0,0.19,0.06,0,0.03,0.09,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.72199999999999998,1.08,0.78,0.48000000000000004,0.78,2.5299999999999998,0.38,0.27,0.49]
["GGL FK06 62 Flush + BDX","GGL","FK06","62","MANUAL","Flush + BDX","GGL 62","GPL 62","ok","GPL","62","GPL FK06 62 Flush + BDX","62",1.1000000000000001,1.2,0.99,1.1000000000000001,0.94,1.1000000000000001,0.91,1,1.1000000000000001,0.96,0.82,0.91,0.19,7.0000000000000007E-2,0,0.19,7.0000000000000007E-2,0,0.03,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.72199999999999998,1.28,0.92,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.51]
["GGL FK06 70Q Flush + BDX","GGL","FK06","70Q","MANUAL","Flush + BDX","GGL 70Q","GPL 70","ok","GPL","70","GPL FK06 70 Flush + BDX",70,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.97,1.2,0.2,0.06,0,0.2,0.06,0,0.04,0.09,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.72199999999999998,1.28,0.92,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.51]
["GGL FK08 66 Flush + BDX","GGL","FK08","66","MANUAL","Flush + BDX","GGL 66","GPL 66","ok","GPL","66","GPL FK08 66 Flush + BDX","66",1.1000000000000001,1.3,1,1.2,0.98,1.1000000000000001,0.95,1.1000000000000001,1.2,1,0.85,0.94,0.16,7.0000000000000007E-2,0,0.16,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.72199999999999998,1.5,1.08,0.48000000000000004,1.2,3.37,0.57999999999999996,0.34000000000000008,0.54]
["GGL MK04 57 Flush + BDX","GGL","MK04",57,"ELECTRIC","Flush + BDX","GGL 57","GPL 70","ok","GPL","70","GPL MK04 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.96,1.1000000000000001,0.11,0.05,0,0.11,0.06,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.32,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GGL MK04 57 Flush + BDX","GGL","MK04",57,"MANUAL","Flush + BDX","GGL 57","GPL 70","ok","GPL","70","GPL MK04 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.96,1.1000000000000001,0.11,0.05,0,0.11,0.06,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.32,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GGL MK04 66 Flush + BDX","GGL","MK04","66","SOLAR","Flush + BDX","GGL 66","GPL 66","ok","GPL","66","GPL MK04 66 Flush + BDX","66",1.1000000000000001,1.2,1,1.2,0.96,1.1000000000000001,0.94,1,1.2,0.99,0.84,0.93,0.16,7.0000000000000007E-2,0,0.16,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.32,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GGL MK04 76F Flush + BDX","GGL","MK04","76F","MANUAL","Flush + BDX","GGL 76F","GPL 70","ok","GPL","70","GPL MK04 70 Flush + BDX","76",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.96,1.1000000000000001,0.11,0.05,0,0.11,0.05,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.32,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GGL MK06 54F Flush + BDX","GGL","MK06","54F","MANUAL","Flush + BDX","GGL 54F","GPL 54F","ok","GPL","54F","GPL MK06 54F Flush + BDX","54F",1.4,1.7,1.3,1.5,1.2,1.4,1.1000000000000001,1.4,1.5,1.2,1,1.2,0.31,0.05,0,0.31,0.05,0,0.06,0.08,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.45,0,0.08,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GGL MK06 57 Flush + BDX","GGL","MK06",57,"MANUAL","Flush + BDX","GGL 57","GPL 70","ok","GPL","70","GPL MK06 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.96,1.2,0.12,0.05,0,0.12,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.34,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GGL MK06 66 Flush + BDX","GGL","MK06","66","SOLAR","Flush + BDX","GGL 66","GPL 66","ok","GPL","66","GPL MK06 66 Flush + BDX","66",1.1000000000000001,1.2,1,1.2,0.95,1.1000000000000001,0.92,1,1.2,0.98,0.83,0.93,0.17,7.0000000000000007E-2,0,0.17,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GGL MK06 76F Flush + BDX","GGL","MK06","76F","SOLAR","Flush + BDX","GGL 76F","GPL 70","ok","GPL","70","GPL MK06 70 Flush + BDX","76",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.96,1.2,0.12,0.05,0,0.12,0.05,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.34,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GGL MK06 57 Flush + BDX","GGL","MK06",57,"SOLAR","Flush + BDX","GGL 57","GPL 70","ok","GPL","70","GPL MK06 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.96,1.2,0.12,0.05,0,0.12,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.34,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GGL MK08 57 Flush + BDX","GGL","MK08",57,"MANUAL","Flush + BDX","GGL 57","GPL 70","ok","GPL","70","GPL MK08 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.95,1.2,0.12,0.05,0,0.12,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GGL MK08 66 Flush + BDX","GGL","MK08","66","SOLAR","Flush + BDX","GGL 66","GPL 66","ok","GPL","66","GPL MK08 66 Flush + BDX","66",1.1000000000000001,1.2,0.99,1.1000000000000001,0.94,1.1000000000000001,0.91,1,1.1000000000000001,0.98,0.82,0.92,0.17,0.08,0,0.17,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GGL MK08 76F Flush + BDX","GGL","MK08","76F","MANUAL","Flush + BDX","GGL 76F","GPL 70","ok","GPL","70","GPL MK08 70 Flush + BDX","76",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.95,1.2,0.12,0.05,0,0.12,0.05,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GGL MK08 57 Flush + BDX","GGL","MK08",57,"SOLAR","Flush + BDX","GGL 57","GPL 70","ok","GPL","70","GPL MK08 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.95,1.2,0.12,0.05,0,0.12,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GGL MK10 62 Flush + BDX","GGL","MK10","62","ELECTRIC","Flush + BDX","GGL 62","GPL 62","ok","GPL","62","GPL MK10 62 Flush + BDX","62",0.98,1.2,0.92,1.1000000000000001,0.87,1,0.85,0.98,1.1000000000000001,0.93,0.77,0.88,0.22,7.0000000000000007E-2,0,0.22,0.08,0,0.04,0.08,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.7,1.43,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.59]
["GGL MK10 70Q Flush + BDX","GGL","MK10","70Q","MANUAL","Flush + BDX","GGL 70Q","GPL 70","ok","GPL","70","GPL MK10 70 Flush + BDX",70,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.4,1.5,1.3,0.95,1.2,0.23,0.06,0,0.23,0.06,0,0.04,0.09,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.7,1.43,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.59]
["GGL MK27 66 Flush + BDX","GGL","MK27","66","MANUAL","Flush + BDX","GGL 66","GPL 66","ok","GPL","66","GPL MK27 66 Flush + BDX","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.98,1.1000000000000001,1.2,1,0.87,0.95,0.13,7.0000000000000007E-2,0,0.13,7.0000000000000007E-2,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.26,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,0.73,0.61,0.60000000000000009,0.43,2.06,0.26,0.22999999999999998,0.43]
["GGL PK04 57 Flush + BDX","GGL","PK04",57,"ELECTRIC","Flush + BDX","GGL 57","GPL 70","ok","GPL","70","GPL PK04 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.94,1.1000000000000001,0.12,0.05,0,0.12,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.08,1.08,0.76200000000000001,0.78,3.09,0.6,0.32000000000000006,0.56000000000000005]
["GGL PK04 66 Flush + BDX","GGL","PK04","66","MANUAL","Flush + BDX","GGL 66","GPL 66","ok","GPL","66","GPL PK04 66 Flush + BDX","66",1,1.2,0.98,1.1000000000000001,0.93,1.1000000000000001,0.9,1,1.1000000000000001,0.97,0.82,0.91,0.17,7.0000000000000007E-2,0,0.17,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.08,1.08,0.76200000000000001,0.78,3.09,0.6,0.32000000000000006,0.56000000000000005]
["GGL PK06 62 Flush + BDX","GGL","PK06","62","ELECTRIC","Flush + BDX","GGL 62","GPL 62","ok","GPL","62","GPL PK06 62 Flush + BDX","62",0.95,1.1000000000000001,0.9,1.1000000000000001,0.85,0.99,0.83,0.96,1.1000000000000001,0.91,0.76,0.86,0.22,7.0000000000000007E-2,0,0.22,0.08,0,0.04,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.28,1.29,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.57999999999999996]
["GGL PK06 76F Flush + BDX","GGL","PK06","76F","ELECTRIC","Flush + BDX","GGL 76F","GPL 70","ok","GPL","70","GPL PK06 70 Flush + BDX","76",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.94,1.1000000000000001,0.12,0.05,0,0.12,0.05,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.004,1.28,1.29,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.57999999999999996]
["GGL PK08 62 Flush + BDX","GGL","PK08","62","ELECTRIC","Flush + BDX","GGL 62","GPL 62","ok","GPL","62","GPL PK08 62 Flush + BDX","62",0.94,1.1000000000000001,0.89,1.1000000000000001,0.84,0.99,0.82,0.96,1.1000000000000001,0.91,0.75,0.86,0.23,7.0000000000000007E-2,0,0.23,0.08,0,0.04,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.5,1.51,0.76200000000000001,1.2,3.93,0.92,0.4,0.61]
["GGL PK08 66 Flush + BDX","GGL","PK08","66","ELECTRIC","Flush + BDX","GGL 66","GPL 66","ok","GPL","66","GPL PK08 66 Flush + BDX","66",1,1.2,0.95,1.1000000000000001,0.9,1,0.88,1,1.1000000000000001,0.95,0.79,0.9,0.18,0.08,0,0.18,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.5,1.51,0.76200000000000001,1.2,3.93,0.92,0.4,0.61]
["GGL PK08 70 Flush + BDX","GGL","PK08","70","MANUALBOTTOM","Flush + BDX","GGL 70","GPL 70","ok","GPL","70","GPL PK08 70 Flush + BDX","70",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.94,1.2,0.23,0.06,0,0.23,0.06,0,0.04,0.09,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.5,1.51,0.76200000000000001,1.2,3.93,0.92,0.4,0.61]
["GGL PK10 62 Flush + BDX","GGL","PK10","62","MANUAL","Flush + BDX","GGL 62","GPL 62","ok","GPL","62","GPL PK10 62 Flush + BDX","62",0.93,1.1000000000000001,0.88,1,0.83,0.98,0.81,0.95,1,0.9,0.74,0.86,0.24,0.08,0,0.24,0.08,0,0.04,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.7,1.71,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.63]
["GGL PK10 70 Flush + BDX","GGL","PK10","70","ELECTRIC","Flush + BDX","GGL 70","GPL 70","ok","GPL","70","GPL PK10 70 Flush + BDX","70",1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.93,1.2,0.24,0.06,0,0.24,0.06,0,0.04,0.09,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.7,1.71,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.63]
["GGL PK10 70 Flush + BDX","GGL","PK10","70","MANUALBOTTOM","Flush + BDX","GGL 70","GPL 70","ok","GPL","70","GPL PK10 70 Flush + BDX","70",1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.93,1.2,0.24,0.06,0,0.24,0.06,0,0.04,0.09,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.7,1.71,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.63]
["GGL PK25 62 Flush + BDX","GGL","PK25","62","ELECTRIC","Flush + BDX","GGL 62","GPL 62","ok","GPL","62","GPL PK25 62 Flush + BDX","62",1.1000000000000001,1.2,1,1.1000000000000001,0.96,1.1000000000000001,0.93,1,1.1000000000000001,0.96,0.84,0.91,0.16,0.06,0,0.16,7.0000000000000007E-2,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.28000000000000003,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,0.65,0.65,0.76200000000000001,0.36,2.2400000000000002,0.27,0.25,0.42]
["GGL SK01 66 Flush + BDX","GGL","SK01","66","MANUAL","Flush + BDX","GGL 66","GPL 66","ok","GPL","66","GPL SK01 66 Flush + BDX","66",1.1000000000000001,1.2,1,1.1000000000000001,0.94,1.1000000000000001,0.92,1,1.1000000000000001,0.97,0.83,0.91,0.15,7.0000000000000007E-2,0,0.15,7.0000000000000007E-2,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.31,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,0.8,0.96,0.96,0.5,2.93,0.49,0.31000000000000005,0.51]
["GGL SK06 57 Flush + BDX","GGL","SK06",57,"MANUAL","Flush + BDX","GGL 57","GPL 70","ok","GPL","70","GPL SK06 70 Flush + BDX",57,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.93,1.1000000000000001,0.13,0.05,0,0.13,0.06,0,0.02,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GGL SK06 66 Flush + BDX","GGL","SK06","66","MANUAL","Flush + BDX","GGL 66","GPL 66","ok","GPL","66","GPL SK06 66 Flush + BDX","66",0.99,1.2,0.93,1.1000000000000001,0.88,1,0.86,1,1.1000000000000001,0.94,0.78,0.89,0.19,0.08,0,0.19,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GGL SK06 66 Flush + BDX","GGL","SK06","66","SOLAR","Flush + BDX","GGL 66","GPL 66","ok","GPL","66","GPL SK06 66 Flush + BDX","66",0.99,1.2,0.93,1.1000000000000001,0.88,1,0.86,1,1.1000000000000001,0.94,0.78,0.89,0.19,0.08,0,0.19,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GGL SK06 76F Flush + BDX","GGL","SK06","76F","ELECTRIC","Flush + BDX","GGL 76F","GPL 70","ok","GPL","70","GPL SK06 70 Flush + BDX","76",1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.93,1.1000000000000001,0.13,0.05,0,0.13,0.05,0,0.02,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GGL SK08 57 Flush + BDX","GGL","SK08",57,"MANUAL","Flush + BDX","GGL 57","GPL 70","ok","GPL","70","GPL SK08 70 Flush + BDX",57,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.92,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GGL SK08 62 Flush + BDX","GGL","SK08","62","MANUAL","Flush + BDX","GGL 62","GPL 62","ok","GPL","62","GPL SK08 62 Flush + BDX","62",0.9,1.1000000000000001,0.85,1,0.81,0.96,0.79,0.94,1,0.89,0.72,0.84,0.24,0.08,0,0.24,0.08,0,0.04,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GGL SK08 70 Flush + BDX","GGL","SK08","70","MANUAL","Flush + BDX","GGL 70","GPL 70","ok","GPL","70","GPL SK08 70 Flush + BDX","70",1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.92,1.2,0.24,0.06,0,0.24,0.06,0,0.05,0.08,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GGL SK08 57 Flush + BDX","GGL","SK08",57,"SOLAR","Flush + BDX","GGL 57","GPL 70","ok","GPL","70","GPL SK08 70 Flush + BDX",57,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.92,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GGL SK10 76F Flush + BDX","GGL","SK10","76F","MANUAL","Flush + BDX","GGL 76F","GPL 70","ok","GPL","70","GPL SK10 70 Flush + BDX","76",1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.92,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.7,2.0499999999999998,0.96,1.41,4.7300000000000004,1.35,0.47,0.66]
["GGL UK04 57 Flush + BDX","GGL","UK04",57,"MANUAL","Flush + BDX","GGL 57","GPL 70","ok","GPL","70","GPL UK04 70 Flush + BDX",57,1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.92,1.1000000000000001,0.13,0.05,0,0.13,0.06,0,0.02,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.37,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.4020000000000001,1.08,1.51,1.1600000000000001,0.78,3.89,0.91,0.4,0.6]
["GGL UK04 66 Flush + BDX","GGL","UK04","66","ELECTRIC","Flush + BDX","GGL 66","GPL 66","ok","GPL","66","GPL UK04 66 Flush + BDX","66",0.98,1.2,0.93,1.1000000000000001,0.88,1,0.86,0.99,1.1000000000000001,0.94,0.78,0.89,0.18,0.08,0,0.18,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.08,1.51,1.1600000000000001,0.78,3.89,0.91,0.4,0.6]
["GGL UK04 76F Flush + BDX","GGL","UK04","76F","MANUAL","Flush + BDX","GGL 76F","GPL 70","ok","GPL","70","GPL UK04 70 Flush + BDX","76",1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.92,1.1000000000000001,0.13,0.05,0,0.13,0.05,0,0.02,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.37,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.4020000000000001,1.08,1.51,1.1600000000000001,0.78,3.89,0.91,0.4,0.6]
["GGL UK08 54F Flush + BDX","GGL","UK08","54F","MANUAL","Flush + BDX","GGL 54F","GPL 54F","ok","GPL","54F","GPL UK08 54F Flush + BDX","54F",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.95,1.2,0.37,0.05,0,0.37,0.05,0,7.0000000000000007E-2,0.08,0,0.14000000000000001,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.55000000000000004,0,0.09,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.4020000000000001,1.5,2.1,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.66]
["GGL UK08 57 Flush + BDX","GGL","UK08",57,"MANUAL","Flush + BDX","GGL 57","GPL 70","ok","GPL","70","GPL UK08 70 Flush + BDX",57,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.91,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.4020000000000001,1.5,2.1,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.66]
["GGL UK08 70 Flush + BDX","GGL","UK08","70","ELECTRIC","Flush + BDX","GGL 70","GPL 70","ok","GPL","70","GPL UK08 70 Flush + BDX","70",1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.91,1.2,0.25,0.06,0,0.25,0.06,0,0.05,0.08,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.5,2.1,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.66]
["GGL UK08 76F Flush + BDX","GGL","UK08","76F","SOLAR","Flush + BDX","GGL 76F","GPL 70","ok","GPL","70","GPL UK08 70 Flush + BDX","76",1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.91,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42364",422,1.4020000000000001,1.5,2.1,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.66]
["GGL UK10 70Q Flush + BDX","GGL","UK10","70Q","MANUAL","Flush + BDX","GGL 70Q","GPL 70","ok","GPL","70","GPL UK10 70 Flush + BDX",70,1.2,1.7,1.1000000000000001,1.5,1,1.4,1,1.3,1.5,1.2,0.91,1.2,0.26,0.06,0,0.26,0.06,0,0.05,0.08,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.47,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.7,2.39,1.1600000000000001,1.41,5.13,1.63,0.51000000000000023,0.68]
["GGL UK10 76F Flush + BDX","GGL","UK10","76F","MANUAL","Flush + BDX","GGL 76F","GPL 70","ok","GPL","70","GPL UK10 70 Flush + BDX","76",1.2,1.7,1.1000000000000001,1.5,1,1.4,1,1.3,1.5,1.2,0.91,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.7,2.39,1.1600000000000001,1.41,5.13,1.63,0.51000000000000023,0.68]
["GGU CK02 66 Flush + BDX","GGU","CK02","66","ELECTRIC","Flush + BDX","GGU 66","GPU 66","ok","GPU","66","GPU CK02 66 Flush + BDX","66",1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.1000000000000001,1,1.1000000000000001,1.2,1,0.92,0.98,0.12,7.0000000000000007E-2,0,0.12,7.0000000000000007E-2,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.25,0,0.04,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,0.88,0.54,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.41]
["GGU CK02 70Q Flush + BDX","GGU","CK02","70Q","MANUAL","Flush + BDX","GGU 70Q","GPU 70","ok","GPU","70","GPU CK02 70 Flush + BDX",70,1.4,1.6,1.3,1.5,1.2,1.4,1.2,1.3,1.5,1.2,1,1.1000000000000001,0.15,0.05,0,0.15,0.05,0,0.03,0.1,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.28000000000000003,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,0.88,0.54,0.37000000000000005,0.57999999999999996,1.91,0.22,0.21,0.41]
["GGU CK04 62 Flush + BDX","GGU","CK04","62","MANUAL","Flush + BDX","GGU 62","GPU 62","ok","GPU","62","GPU CK04 62 Flush + BDX","62",1.1000000000000001,1.2,1,1.2,0.98,1.1000000000000001,0.95,1,1.2,0.98,0.85,0.93,0.17,0.06,0,0.17,7.0000000000000007E-2,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.3,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GGU CK04 62 Flush + BDX","GGU","CK04","62","ELECTRIC","Flush + BDX","GGU 62","GPU 62","ok","GPU","62","GPU CK04 62 Flush + BDX","62",1.1000000000000001,1.2,1,1.2,0.98,1.1000000000000001,0.95,1,1.2,0.98,0.85,0.93,0.17,0.06,0,0.17,7.0000000000000007E-2,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.3,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GGU CK04 70Q Flush + BDX","GGU","CK04","70Q","MANUAL","Flush + BDX","GGU 70Q","GPU 70","ok","GPU","70","GPU CK04 70 Flush + BDX",70,1.4,1.7,1.3,1.5,1.2,1.4,1.2,1.3,1.5,1.2,1,1.2,0.17,0.06,0,0.17,0.06,0,0.03,0.1,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.3,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GGU CK06 62 Flush + BDX","GGU","CK06","62","ELECTRIC","Flush + BDX","GGU 62","GPU 62","ok","GPU","62","GPU CK06 62 Flush + BDX","62",1.1000000000000001,1.2,1,1.2,0.97,1.1000000000000001,0.94,1,1.2,0.98,0.85,0.93,0.18,7.0000000000000007E-2,0,0.18,7.0000000000000007E-2,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.32,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,1.28,0.78,0.37000000000000005,0.98,2.71,0.36,0.29000000000000004,0.46]
["GGU FK04 62 Flush + BDX","GGU","FK04","62","ELECTRIC","Flush + BDX","GGU 62","GPU 62","ok","GPU","62","GPU FK04 62 Flush + BDX","62",1,1.2,0.99,1.1000000000000001,0.93,1,0.91,1,1.1000000000000001,0.95,0.82,0.9,0.18,7.0000000000000007E-2,0,0.18,7.0000000000000007E-2,0,0.03,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.72199999999999998,1.08,0.78,0.48000000000000004,0.78,2.5299999999999998,0.38,0.27,0.49]
["GGU FK04 66 Flush + BDX","GGU","FK04","66","MANUAL","Flush + BDX","GGU 66","GPU 66","ok","GPU","66","GPU FK04 66 Flush + BDX","66",1.2,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.99,1.1000000000000001,1.2,1,0.88,0.95,0.15,7.0000000000000007E-2,0,0.15,0.08,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.3,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.72199999999999998,1.08,0.78,0.48000000000000004,0.78,2.5299999999999998,0.38,0.27,0.49]
["GGU FK06 66 Flush + BDX","GGU","FK06","66","ELECTRIC","Flush + BDX","GGU 66","GPU 66","ok","GPU","66","GPU FK06 66 Flush + BDX","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.98,1.1000000000000001,1.2,1,0.87,0.95,0.15,7.0000000000000007E-2,0,0.15,0.08,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.32,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.72199999999999998,1.28,0.92,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.51]
["GGU FK06 76F Flush + BDX","GGU","FK06","76F","MANUAL","Flush + BDX","GGU 76F","GPU 70","ok","GPU","70","GPU FK06 70 Flush + BDX","76",1.3,1.7,1.2,1.5,1.2,1.4,1.1000000000000001,1.3,1.5,1.2,0.99,1.2,0.11,0.05,0,0.11,0.05,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.32,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.72199999999999998,1.28,0.92,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.51]
["GGU FK08 66 Flush + BDX","GGU","FK08","66","SOLAR","Flush + BDX","GGU 66","GPU 66","ok","GPU","66","GPU FK08 66 Flush + BDX","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.97,1.1000000000000001,1.2,1,0.87,0.94,0.16,7.0000000000000007E-2,0,0.16,0.08,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.72199999999999998,1.5,1.08,0.48000000000000004,1.2,3.37,0.57999999999999996,0.34000000000000008,0.54]
["GGU MK04 57 Flush + BDX","GGU","MK04",57,"MANUAL","Flush + BDX","GGU 57","GPU 70","ok","GPU","70","GPU MK04 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.97,1.1000000000000001,0.11,0.05,0,0.11,0.06,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.32,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GGU MK04 66 Flush + BDX","GGU","MK04","66","MANUAL","Flush + BDX","GGU 66","GPU 66","ok","GPU","66","GPU MK04 66 Flush + BDX","66",1.1000000000000001,1.2,1,1.2,0.98,1.1000000000000001,0.95,1,1.2,0.99,0.85,0.93,0.16,7.0000000000000007E-2,0,0.16,0.08,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.32,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GGU MK04 70Q Flush + BDX","GGU","MK04","70Q","MANUAL","Flush + BDX","GGU 70Q","GPU 70","ok","GPU","70","GPU MK04 70 Flush + BDX",70,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.97,1.1000000000000001,0.2,0.06,0,0.2,0.06,0,0.04,0.09,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GGU MK06 57 Flush + BDX","GGU","MK06",57,"SOLAR","Flush + BDX","GGU 57","GPU 70","ok","GPU","70","GPU MK06 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.97,1.2,0.12,0.05,0,0.12,0.06,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.34,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GGU MK06 62 Flush + BDX","GGU","MK06","62","MANUAL","Flush + BDX","GGU 62","GPU 62","ok","GPU","62","GPU MK06 62 Flush + BDX","62",0.98,1.1000000000000001,0.93,1.1000000000000001,0.88,1,0.86,0.98,1.1000000000000001,0.93,0.78,0.88,0.21,7.0000000000000007E-2,0,0.21,7.0000000000000007E-2,0,0.04,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GGU MK06 70 Flush + BDX","GGU","MK06","70","MANUAL","Flush + BDX","GGU 70","GPU 70","ok","GPU","70","GPU MK06 70 Flush + BDX","70",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.97,1.2,0.21,0.06,0,0.21,0.06,0,0.04,0.09,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GGU MK06 76F Flush + BDX","GGU","MK06","76F","ELECTRIC","Flush + BDX","GGU 76F","GPU 70","ok","GPU","70","GPU MK06 70 Flush + BDX","76",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.97,1.2,0.12,0.05,0,0.12,0.05,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.34,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GGU MK08 66 Flush + BDX","GGU","MK08","66","MANUAL","Flush + BDX","GGU 66","GPU 66","ok","GPU","66","GPU MK08 66 Flush + BDX","66",1.1000000000000001,1.2,1,1.1000000000000001,0.96,1.1000000000000001,0.93,1,1.1000000000000001,0.98,0.84,0.92,0.17,0.08,0,0.17,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GGU MK08 66 Flush + BDX","GGU","MK08","66","ELECTRIC","Flush + BDX","GGU 66","GPU 66","ok","GPU","66","GPU MK08 66 Flush + BDX","66",1.1000000000000001,1.2,1,1.1000000000000001,0.96,1.1000000000000001,0.93,1,1.1000000000000001,0.98,0.84,0.92,0.17,0.08,0,0.17,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GGU MK08 76F Flush + BDX","GGU","MK08","76F","ELECTRIC","Flush + BDX","GGU 76F","GPU 70","ok","GPU","70","GPU MK08 70 Flush + BDX","76",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.97,1.2,0.12,0.05,0,0.12,0.05,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GGU MK10 66 Flush + BDX","GGU","MK10","66","ELECTRIC","Flush + BDX","GGU 66","GPU 66","ok","GPU","66","GPU MK10 66 Flush + BDX","66",1.1000000000000001,1.2,1,1.1000000000000001,0.95,1.1000000000000001,0.92,1,1.1000000000000001,0.97,0.83,0.92,0.18,0.08,0,0.18,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.7,1.43,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.59]
["GGU PK06 57 Flush + BDX","GGU","PK06",57,"ELECTRIC","Flush + BDX","GGU 57","GPU 70","ok","GPU","70","GPU PK06 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.94,1.1000000000000001,0.12,0.05,0,0.12,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,1.004,1.28,1.29,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.57999999999999996]
["GGU PK06 57 Flush + BDX","GGU","PK06",57,"SOLAR","Flush + BDX","GGU 57","GPU 70","ok","GPU","70","GPU PK06 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.94,1.1000000000000001,0.12,0.05,0,0.12,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,1.004,1.28,1.29,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.57999999999999996]
["GGU PK06 66 Flush + BDX","GGU","PK06","66","SOLAR","Flush + BDX","GGU 66","GPU 66","ok","GPU","66","GPU PK06 66 Flush + BDX","66",1,1.2,0.97,1.1000000000000001,0.92,1,0.89,1,1.1000000000000001,0.95,0.81,0.9,0.18,0.08,0,0.18,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.28,1.29,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.57999999999999996]
["GGU PK06 76F Flush + BDX","GGU","PK06","76F","MANUAL","Flush + BDX","GGU 76F","GPU 70","ok","GPU","70","GPU PK06 70 Flush + BDX","76",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.94,1.1000000000000001,0.12,0.05,0,0.12,0.05,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,1.004,1.28,1.29,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.57999999999999996]
["GGU PK08 66 Flush + BDX","GGU","PK08","66","MANUAL","Flush + BDX","GGU 66","GPU 66","ok","GPU","66","GPU PK08 66 Flush + BDX","66",1,1.2,0.97,1.1000000000000001,0.91,1,0.89,1,1.1000000000000001,0.95,0.8,0.9,0.18,0.08,0,0.18,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.5,1.51,0.76200000000000001,1.2,3.93,0.92,0.4,0.61]
["GGU PK08 66 Flush + BDX","GGU","PK08","66","ELECTRIC","Flush + BDX","GGU 66","GPU 66","ok","GPU","66","GPU PK08 66 Flush + BDX","66",1,1.2,0.97,1.1000000000000001,0.91,1,0.89,1,1.1000000000000001,0.95,0.8,0.9,0.18,0.08,0,0.18,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.5,1.51,0.76200000000000001,1.2,3.93,0.92,0.4,0.61]
["GGU PK10 57 Flush + BDX","GGU","PK10",57,"MANUAL","Flush + BDX","GGU 57","GPU 70","ok","GPU","70","GPU PK10 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.95,1.2,0.13,0.05,0,0.13,0.06,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,1.004,1.7,1.71,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.63]
["GGU PK10 66 Flush + BDX","GGU","PK10","66","MANUAL","Flush + BDX","GGU 66","GPU 66","ok","GPU","66","GPU PK10 66 Flush + BDX","66",1,1.2,0.96,1.1000000000000001,0.91,1,0.88,1,1.1000000000000001,0.95,0.8,0.9,0.19,0.08,0,0.19,0.09,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.7,1.71,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.63]
["GGU PK10 70 Flush + BDX","GGU","PK10","70","MANUAL","Flush + BDX","GGU 70","GPU 70","ok","GPU","70","GPU PK10 70 Flush + BDX","70",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.95,1.2,0.24,0.06,0,0.24,0.06,0,0.04,0.09,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.7,1.71,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.63]
["GGU PK10 76F Flush + BDX","GGU","PK10","76F","MANUAL","Flush + BDX","GGU 76F","GPU 70","ok","GPU","70","GPU PK10 70 Flush + BDX","76",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.95,1.2,0.13,0.05,0,0.13,0.05,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,1.004,1.7,1.71,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.63]
["GGU SK06 62 Flush + BDX","GGU","SK06","62","ELECTRIC","Flush + BDX","GGU 62","GPU 62","ok","GPU","62","GPU SK06 62 Flush + BDX","62",0.89,1.1000000000000001,0.85,1,0.81,0.95,0.79,0.93,1,0.88,0.72,0.84,0.23,7.0000000000000007E-2,0,0.23,0.08,0,0.04,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GGU SK06 70Q Flush + BDX","GGU","SK06","70Q","MANUAL","Flush + BDX","GGU 70Q","GPU 70","ok","GPU","70","GPU SK06 70 Flush + BDX",70,1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.93,1.1000000000000001,0.23,0.06,0,0.23,0.06,0,0.04,0.09,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GGU SK06 76F Flush + BDX","GGU","SK06","76F","ELECTRIC","Flush + BDX","GGU 76F","GPU 70","ok","GPU","70","GPU SK06 70 Flush + BDX","76",1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.93,1.1000000000000001,0.13,0.05,0,0.13,0.05,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GGU SK08 57 Flush + BDX","GGU","SK08",57,"SOLAR","Flush + BDX","GGU 57","GPU 70","ok","GPU","70","GPU SK08 70 Flush + BDX",57,1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.93,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GGU SK08 70 Flush + BDX","GGU","SK08","70","MANUAL","Flush + BDX","GGU 70","GPU 70","ok","GPU","70","GPU SK08 70 Flush + BDX","70",1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.93,1.2,0.24,0.06,0,0.24,0.06,0,0.05,0.09,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GGU SK10 66 Flush + BDX","GGU","SK10","66","ELECTRIC","Flush + BDX","GGU 66","GPU 66","ok","GPU","66","GPU SK10 66 Flush + BDX","66",0.97,1.2,0.92,1.1000000000000001,0.87,1,0.85,0.98,1.1000000000000001,0.93,0.77,0.88,0.2,0.08,0,0.2,0.09,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.7,2.0499999999999998,0.96,1.41,4.7300000000000004,1.35,0.47,0.66]
["GGU UK04 57 Flush + BDX","GGU","UK04",57,"SOLAR","Flush + BDX","GGU 57","GPU 70","ok","GPU","70","GPU UK04 70 Flush + BDX",57,1.2,1.6,1.2,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.93,1.1000000000000001,0.13,0.05,0,0.13,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.37,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,1.4020000000000001,1.08,1.51,1.1600000000000001,0.78,3.89,0.91,0.4,0.6]
["GGU UK04 66 Flush + BDX","GGU","UK04","66","MANUAL","Flush + BDX","GGU 66","GPU 66","ok","GPU","66","GPU UK04 66 Flush + BDX","66",1,1.2,0.94,1.1000000000000001,0.89,1,0.87,0.99,1.1000000000000001,0.94,0.79,0.89,0.18,0.08,0,0.18,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.08,1.51,1.1600000000000001,0.78,3.89,0.91,0.4,0.6]
["GGU UK04 76F Flush + BDX","GGU","UK04","76F","MANUAL","Flush + BDX","GGU 76F","GPU 70","ok","GPU","70","GPU UK04 70 Flush + BDX","76",1.2,1.6,1.2,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.93,1.1000000000000001,0.13,0.05,0,0.13,0.05,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.37,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,1.4020000000000001,1.08,1.51,1.1600000000000001,0.78,3.89,0.91,0.4,0.6]
["GGU UK08 66 Flush + BDX","GGU","UK08","66","MANUAL","Flush + BDX","GGU 66","GPU 66","ok","GPU","66","GPU UK08 66 Flush + BDX","66",0.95,1.1000000000000001,0.9,1.1000000000000001,0.85,1,0.83,0.97,1.1000000000000001,0.92,0.76,0.87,0.2,0.08,0,0.2,0.09,0,0.03,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.5,2.1,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.66]
["GGU UK08 66 Flush + BDX","GGU","UK08","66","SOLAR","Flush + BDX","GGU 66","GPU 66","ok","GPU","66","GPU UK08 66 Flush + BDX","66",0.95,1.1000000000000001,0.9,1.1000000000000001,0.85,1,0.83,0.97,1.1000000000000001,0.92,0.76,0.87,0.2,0.08,0,0.2,0.09,0,0.03,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.5,2.1,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.66]
["GGU UK08 76F Flush + BDX","GGU","UK08","76F","MANUAL","Flush + BDX","GGU 76F","GPU 70","ok","GPU","70","GPU UK08 70 Flush + BDX","76",1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.92,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42366 ",422,1.4020000000000001,1.5,2.1,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.66]
["GIL MK34 57 Flush + BDX","GIL","MK34","57","FIXED","Flush + BDX","GIL 57","GPL 70","ok","GPL","70","GPL MK34 70 Flush + BDX","57",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.96,1.1000000000000001,0.11,0.05,0,0.11,0.06,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.31,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.02,0.86,0.60000000000000009,0.73,2.65,0.44,0.27999999999999997,0.51]
["GIL PK34 62 Flush + BDX","GIL","PK34","62","FIXED","Flush + BDX","GIL 62","VFE 62","ok","VFE","62","VFE PK34 62 Flush + BDX","62",0.97,1.1000000000000001,0.92,1.1000000000000001,0.87,1,0.85,0.97,1.1000000000000001,0.92,0.77,0.87,0.21,7.0000000000000007E-2,0,0.21,0.08,0,0.04,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.02,1.03,0.76200000000000001,0.73,2.98,0.56000000000000005,0.30999999999999994,0.54]
["GIL SK34 66 Flush + BDX","GIL","SK34","66","FIXED","Flush + BDX","GIL 66","GPL 66","ok","GPL","66","GPL SK34 66 Flush + BDX","66",1,1.2,0.96,1.1000000000000001,0.91,1,0.88,1,1.1000000000000001,0.95,0.8,0.9,0.17,7.0000000000000007E-2,0,0.17,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.02,1.23,0.96,0.73,3.37,0.7,0.35000000000000009,0.56999999999999995]
["GIL UK34 66 Flush + BDX","GIL","UK34","66","FIXED","Flush + BDX","GIL 66","GPL 66","ok","GPL","66","GPL UK34 66 Flush + BDX","66",0.99,1.2,0.94,1.1000000000000001,0.89,1,0.86,0.99,1.1000000000000001,0.94,0.78,0.89,0.17,7.0000000000000007E-2,0,0.17,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.02,1.43,1.1600000000000001,0.73,3.77,0.84,0.39,0.59]
["GIU FK34 62 Flush + BDX","GIU","FK34","62","FIXED","Flush + BDX","GIU 62","GIU 62","ok","GIU","62","GIU FK34 62 Flush + BDX","62",1.1000000000000001,1.2,1,1.2,0.97,1.1000000000000001,0.94,1,1.2,0.98,0.85,0.93,0.18,7.0000000000000007E-2,0,0.18,7.0000000000000007E-2,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.72199999999999998,1.02,0.74,0.48000000000000004,0.73,2.41,0.35,0.26,0.47]
["GIU PK34 57 Flush + BDX","GIU","PK34","57","FIXED","Flush + BDX","GIU 57","GPU 70","ok","GPU","70","GPU PK34 70 Flush + BDX","57",1.3,1.6,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.95,1.1000000000000001,0.11,0.05,0,0.11,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.32,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.02,1.03,0.76200000000000001,0.73,2.97,0.55000000000000004,0.31999999999999995,0.53]
["GIU SK34 66 Flush + BDX","GIU","SK34","66","FIXED","Flush + BDX","GIU 66","GPU 66","ok","GPU","66","GPU SK34 66 Flush + BDX","66",1,1.2,0.97,1.1000000000000001,0.92,1,0.89,1,1.1000000000000001,0.95,0.81,0.9,0.17,7.0000000000000007E-2,0,0.17,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.02,1.23,0.96,0.73,3.37,0.7,0.35000000000000009,0.56999999999999995]
["GIU UK34 57 Flush + BDX","GIU","UK34","57","FIXED","Flush + BDX","GIU 57","GPU 70","ok","GPU","70","GPU UK34 70 Flush + BDX","57",1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.93,1.1000000000000001,0.12,0.05,0,0.12,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.02,1.43,1.1600000000000001,0.73,3.77,0.84,0.39,0.59]
["GPL CK04 66 Flush + BDX","GPL","CK04","66","MANUAL","Flush + BDX","GPL 66","GPL 66","ok","GPL","66","GPL CK04 66 Flush + BDX","66",1.2,1.3,1.1000000000000001,1.2,1,1.1000000000000001,1,1.1000000000000001,1.2,1,0.9,0.97,0.13,7.0000000000000007E-2,0,0.13,7.0000000000000007E-2,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.27,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GPL FK06 76F Flush + BDX","GPL","FK06","76F","MANUAL","Flush + BDX","GPL 76F","GPL 70","ok","GPL","70","GPL FK06 70 Flush + BDX","76",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.97,1.2,0.11,0.05,0,0.11,0.05,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.32,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.72199999999999998,1.28,0.92,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.51]
["GPL MK04 70 Flush + BDX","GPL","MK04","70","MANUAL","Flush + BDX","GPL 70","GPL 70","ok","GPL","70","GPL MK04 70 Flush + BDX","70",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.96,1.1000000000000001,0.2,0.06,0,0.2,0.06,0,0.04,0.09,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GPL MK06 76F Flush + BDX","GPL","MK06","76F","MANUAL","Flush + BDX","GPL 76F","GPL 70","ok","GPL","70","GPL MK06 70 Flush + BDX","76",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.96,1.2,0.12,0.05,0,0.12,0.05,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.34,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",422,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GPL MK08 57 Flush + BDX","GPL","MK08",57,"MANUAL","Flush + BDX","GPL 57","GPL 70","ok","GPL","70","GPL MK08 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.95,1.2,0.12,0.05,0,0.12,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",422,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GPL MK10 70 Flush + BDX","GPL","MK10","70","MANUAL","Flush + BDX","GPL 70","GPL 70","ok","GPL","70","GPL MK10 70 Flush + BDX","70",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.4,1.5,1.3,0.95,1.2,0.23,0.06,0,0.23,0.06,0,0.04,0.09,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.7,1.43,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.59]
["GPL PK08 57 Flush + BDX","GPL","PK08",57,"MANUAL","Flush + BDX","GPL 57","GPL 70","ok","GPL","70","GPL PK08 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.94,1.2,0.13,0.05,0,0.13,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",422,1.004,1.5,1.51,0.76200000000000001,1.2,3.93,0.92,0.4,0.61]
["GPL PK10 57 Flush + BDX","GPL","PK10",57,"MANUAL","Flush + BDX","GPL 57","GPL 70","ok","GPL","70","GPL PK10 70 Flush + BDX",57,1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.93,1.2,0.13,0.05,0,0.13,0.06,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",422,1.004,1.7,1.71,0.76200000000000001,1.41,4.34,1.07,0.43999999999999995,0.63]
["GPL SK06 57 Flush + BDX","GPL","SK06",57,"MANUAL","Flush + BDX","GPL 57","GPL 70","ok","GPL","70","GPL SK06 70 Flush + BDX",57,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.93,1.1000000000000001,0.13,0.05,0,0.13,0.06,0,0.02,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",422,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GPL SK08 66 Flush + BDX","GPL","SK08","66","MANUAL","Flush + BDX","GPL 66","GPL 66","ok","GPL","66","GPL SK08 66 Flush + BDX","66",0.97,1.2,0.92,1.1000000000000001,0.87,1,0.85,0.99,1.1000000000000001,0.93,0.77,0.88,0.19,0.08,0,0.19,0.09,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GPL UK04 76F Flush + BDX","GPL","UK04","76F","MANUAL","Flush + BDX","GPL 76F","GPL 70","ok","GPL","70","GPL UK04 70 Flush + BDX","76",1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.92,1.1000000000000001,0.13,0.05,0,0.13,0.05,0,0.02,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.37,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",422,1.4020000000000001,1.08,1.51,1.1600000000000001,0.78,3.89,0.91,0.4,0.6]
["GPL UK04 70 Flush + BDX","GPL","UK04","70","MANUAL","Flush + BDX","GPL 70","GPL 70","ok","GPL","70","GPL UK04 70 Flush + BDX","70",1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.92,1.1000000000000001,0.23,0.06,0,0.23,0.06,0,0.04,0.08,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.08,1.51,1.1600000000000001,0.78,3.89,0.91,0.4,0.6]
["GPL UK08 70 Flush + BDX","GPL","UK08","70","MANUAL","Flush + BDX","GPL 70","GPL 70","ok","GPL","70","GPL UK08 70 Flush + BDX","70",1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.91,1.2,0.25,0.06,0,0.25,0.06,0,0.05,0.08,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.45,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.5,2.1,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.66]
["GPL UK08 57 Flush + BDX","GPL","UK08",57,"MANUAL","Flush + BDX","GPL 57","GPL 70","ok","GPL","70","GPL UK08 70 Flush + BDX",57,1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.91,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42365  ",422,1.4020000000000001,1.5,2.1,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.66]
["GPU CK04 57 Flush + BDX","GPU","CK04",57,"MANUAL","Flush + BDX","GPU 57","GPU 70","ok","GPU","70","GPU CK04 70 Flush + BDX",57,1.4,1.7,1.3,1.5,1.2,1.4,1.2,1.3,1.5,1.2,1,1.2,0.09,0.05,0,0.09,0.06,0,0.02,0.1,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.27,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GPU CK04 62 Flush + BDX","GPU","CK04","62","MANUAL","Flush + BDX","GPU 62","GPU 62","ok","GPU","62","GPU CK04 62 Flush + BDX","62",1.1000000000000001,1.2,1,1.2,0.98,1.1000000000000001,0.95,1,1.2,0.98,0.85,0.93,0.17,0.06,0,0.17,7.0000000000000007E-2,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.3,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GPU CK04 66 Flush + BDX","GPU","CK04","66","MANUAL","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU CK04 66 Flush + BDX","66",1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.1000000000000001,1,1.1000000000000001,1.2,1,0.92,0.97,0.13,7.0000000000000007E-2,0,0.13,7.0000000000000007E-2,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.27,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GPU CK04 76F Flush + BDX","GPU","CK04","76F","MANUAL","Flush + BDX","GPU 76F","GPU 70","ok","GPU","70","GPU CK04 70 Flush + BDX","76",1.4,1.7,1.3,1.5,1.2,1.4,1.2,1.3,1.5,1.2,1,1.2,0.09,0.05,0,0.09,0.05,0,0.02,0.1,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.27,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GPU CK06 62 Flush + BDX","GPU","CK06","62","MANUAL","Flush + BDX","GPU 62","GPU 62","ok","GPU","62","GPU CK06 62 Flush + BDX","62",1.1000000000000001,1.2,1,1.2,0.97,1.1000000000000001,0.94,1,1.2,0.98,0.85,0.93,0.18,7.0000000000000007E-2,0,0.18,7.0000000000000007E-2,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.32,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,1.28,0.78,0.37000000000000005,0.98,2.71,0.36,0.29000000000000004,0.46]
["GPU CK06 66 Flush + BDX","GPU","CK06","66","MANUAL","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU CK06 66 Flush + BDX","66",1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.1000000000000001,1,1.1000000000000001,1.2,1,0.91,0.97,0.14000000000000001,7.0000000000000007E-2,0,0.14000000000000001,0.08,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.28999999999999998,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,1.28,0.78,0.37000000000000005,0.98,2.71,0.36,0.29000000000000004,0.46]
["GPU FK06 62 Flush + BDX","GPU","FK06","62","MANUAL","Flush + BDX","GPU 62","GPU 62","ok","GPU","62","GPU FK06 62 Flush + BDX","62",1,1.2,0.97,1.1000000000000001,0.92,1,0.9,1,1.1000000000000001,0.95,0.81,0.9,0.19,7.0000000000000007E-2,0,0.19,7.0000000000000007E-2,0,0.03,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.72199999999999998,1.28,0.92,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.51]
["GPU FK06 66 Flush + BDX","GPU","FK06","66","MANUAL","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU FK06 66 Flush + BDX","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.98,1.1000000000000001,1.2,1,0.87,0.95,0.15,7.0000000000000007E-2,0,0.15,0.08,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.32,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.72199999999999998,1.28,0.92,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.51]
["GPU FK06 66 Flush + BDX","GPU","FK06","66","ELECTRIC","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU FK06 66 Flush + BDX","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.98,1.1000000000000001,1.2,1,0.87,0.95,0.15,7.0000000000000007E-2,0,0.15,0.08,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.32,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.72199999999999998,1.28,0.92,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.51]
["GPU FK08 62 Flush + BDX","GPU","FK08","62","MANUAL","Flush + BDX","GPU 62","GPU 62","ok","GPU","62","GPU FK08 62 Flush + BDX","62",1,1.2,0.97,1.1000000000000001,0.91,1,0.89,1,1.1000000000000001,0.95,0.8,0.9,0.2,7.0000000000000007E-2,0,0.2,7.0000000000000007E-2,0,0.03,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.72199999999999998,1.5,1.08,0.48000000000000004,1.2,3.37,0.57999999999999996,0.34000000000000008,0.54]
["GPU FK08 66 Flush + BDX","GPU","FK08","66","MANUAL","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU FK08 66 Flush + BDX","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.97,1.1000000000000001,1.2,1,0.87,0.94,0.16,7.0000000000000007E-2,0,0.16,0.08,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.72199999999999998,1.5,1.08,0.48000000000000004,1.2,3.37,0.57999999999999996,0.34000000000000008,0.54]
["GPU FK08 66 Flush + BDX","GPU","FK08","66","ELECTRIC","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU FK08 66 Flush + BDX","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.97,1.1000000000000001,1.2,1,0.87,0.94,0.16,7.0000000000000007E-2,0,0.16,0.08,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.72199999999999998,1.5,1.08,0.48000000000000004,1.2,3.37,0.57999999999999996,0.34000000000000008,0.54]
["GPU MK04 57 Flush + BDX","GPU","MK04",57,"MANUAL","Flush + BDX","GPU 57","GPU 70","ok","GPU","70","GPU MK04 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.97,1.1000000000000001,0.11,0.05,0,0.11,0.06,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.32,0,0.05,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GPU MK04 62 Flush + BDX","GPU","MK04","62","MANUAL","Flush + BDX","GPU 62","GPU 62","ok","GPU","62","GPU MK04 62 Flush + BDX","62",1,1.2,0.94,1.1000000000000001,0.89,1,0.87,0.98,1.1000000000000001,0.93,0.79,0.88,0.2,7.0000000000000007E-2,0,0.2,7.0000000000000007E-2,0,0.03,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GPU MK04 66 Flush + BDX","GPU","MK04","66","MANUAL","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU MK04 66 Flush + BDX","66",1.1000000000000001,1.2,1,1.2,0.98,1.1000000000000001,0.95,1,1.2,0.99,0.85,0.93,0.16,7.0000000000000007E-2,0,0.16,0.08,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.32,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GPU MK04 76F Flush + BDX","GPU","MK04","76F","MANUAL","Flush + BDX","GPU 76F","GPU 70","ok","GPU","70","GPU MK04 70 Flush + BDX","76",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.97,1.1000000000000001,0.11,0.05,0,0.11,0.05,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.32,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,0.84200000000000008,1.08,0.91,0.60000000000000009,0.78,2.77,0.47,0.29000000000000004,0.52]
["GPU MK06 57 Flush + BDX","GPU","MK06",57,"MANUAL","Flush + BDX","GPU 57","GPU 70","ok","GPU","70","GPU MK06 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.97,1.2,0.12,0.05,0,0.12,0.06,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.34,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GPU MK06 57 Flush + BDX","GPU","MK06",57,"ELECTRIC","Flush + BDX","GPU 57","GPU 70","ok","GPU","70","GPU MK06 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.97,1.2,0.12,0.05,0,0.12,0.06,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.34,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GPU MK06 62 Flush + BDX","GPU","MK06","62","MANUAL","Flush + BDX","GPU 62","GPU 62","ok","GPU","62","GPU MK06 62 Flush + BDX","62",0.98,1.1000000000000001,0.93,1.1000000000000001,0.88,1,0.86,0.98,1.1000000000000001,0.93,0.78,0.88,0.21,7.0000000000000007E-2,0,0.21,7.0000000000000007E-2,0,0.04,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GPU MK06 66 Flush + BDX","GPU","MK06","66","MANUAL","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU MK06 66 Flush + BDX","66",1.1000000000000001,1.2,1,1.2,0.97,1.1000000000000001,0.94,1,1.2,0.98,0.84,0.93,0.17,7.0000000000000007E-2,0,0.17,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GPU MK06 66 Flush + BDX","GPU","MK06","66","ELECTRIC","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU MK06 66 Flush + BDX","66",1.1000000000000001,1.2,1,1.2,0.97,1.1000000000000001,0.94,1,1.2,0.98,0.84,0.93,0.17,7.0000000000000007E-2,0,0.17,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GPU MK06 76F Flush + BDX","GPU","MK06","76F","MANUAL","Flush + BDX","GPU 76F","GPU 70","ok","GPU","70","GPU MK06 70 Flush + BDX","76",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.97,1.2,0.12,0.05,0,0.12,0.05,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.34,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,0.84200000000000008,1.28,1.08,0.60000000000000009,0.98,3.17,0.59,0.33000000000000007,0.55000000000000004]
["GPU MK08 57 Flush + BDX","GPU","MK08",57,"MANUAL","Flush + BDX","GPU 57","GPU 70","ok","GPU","70","GPU MK08 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.97,1.2,0.12,0.05,0,0.12,0.06,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GPU MK08 57 Flush + BDX","GPU","MK08",57,"ELECTRIC","Flush + BDX","GPU 57","GPU 70","ok","GPU","70","GPU MK08 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.97,1.2,0.12,0.05,0,0.12,0.06,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GPU MK08 62 Flush + BDX","GPU","MK08","62","MANUAL","Flush + BDX","GPU 62","GPU 62","ok","GPU","62","GPU MK08 62 Flush + BDX","62",0.97,1.1000000000000001,0.92,1.1000000000000001,0.87,1,0.85,0.98,1.1000000000000001,0.92,0.77,0.87,0.22,7.0000000000000007E-2,0,0.22,0.08,0,0.04,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GPU MK08 66 Flush + BDX","GPU","MK08","66","MANUAL","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU MK08 66 Flush + BDX","66",1.1000000000000001,1.2,1,1.1000000000000001,0.96,1.1000000000000001,0.93,1,1.1000000000000001,0.98,0.84,0.92,0.17,0.08,0,0.17,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GPU MK08 66 Flush + BDX","GPU","MK08","66","ELECTRIC","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU MK08 66 Flush + BDX","66",1.1000000000000001,1.2,1,1.1000000000000001,0.96,1.1000000000000001,0.93,1,1.1000000000000001,0.98,0.84,0.92,0.17,0.08,0,0.17,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GPU MK08 76F Flush + BDX","GPU","MK08","76F","MANUAL","Flush + BDX","GPU 76F","GPU 70","ok","GPU","70","GPU MK08 70 Flush + BDX","76",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.97,1.2,0.12,0.05,0,0.12,0.05,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GPU MK10 62 Flush + BDX","GPU","MK10","62","MANUAL","Flush + BDX","GPU 62","GPU 62","ok","GPU","62","GPU MK10 62 Flush + BDX","62",0.96,1.1000000000000001,0.91,1.1000000000000001,0.86,1,0.84,0.97,1.1000000000000001,0.92,0.76,0.87,0.22,7.0000000000000007E-2,0,0.22,0.08,0,0.04,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.7,1.43,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.59]
["GPU MK10 66 Flush + BDX","GPU","MK10","66","MANUAL","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU MK10 66 Flush + BDX","66",1.1000000000000001,1.2,1,1.1000000000000001,0.95,1.1000000000000001,0.92,1,1.1000000000000001,0.97,0.83,0.92,0.18,0.08,0,0.18,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.7,1.43,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.59]
["GPU MK10 70 Flush + BDX","GPU","MK10","70","MANUAL","Flush + BDX","GPU 70","GPU 70","ok","GPU","70","GPU MK10 70 Flush + BDX","70",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.4,1.5,1.3,0.97,1.2,0.23,0.06,0,0.23,0.06,0,0.04,0.09,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.7,1.43,0.60000000000000009,1.41,4.01,0.84,0.41000000000000003,0.59]
["GPU PK06 57 Flush + BDX","GPU","PK06",57,"MANUAL","Flush + BDX","GPU 57","GPU 70","ok","GPU","70","GPU PK06 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.94,1.1000000000000001,0.12,0.05,0,0.12,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,1.004,1.28,1.29,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.57999999999999996]
["GPU PK06 57 Flush + BDX","GPU","PK06",57,"ELECTRIC","Flush + BDX","GPU 57","GPU 70","ok","GPU","70","GPU PK06 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.94,1.1000000000000001,0.12,0.05,0,0.12,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,1.004,1.28,1.29,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.57999999999999996]
["GPU PK06 62 Flush + BDX","GPU","PK06","62","MANUAL","Flush + BDX","GPU 62","GPU 62","ok","GPU","62","GPU PK06 62 Flush + BDX","62",0.93,1.1000000000000001,0.88,1,0.83,0.97,0.81,0.94,1,0.89,0.74,0.85,0.22,7.0000000000000007E-2,0,0.22,0.08,0,0.04,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.28,1.29,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.57999999999999996]
["GPU PK06 66 Flush + BDX","GPU","PK06","66","MANUAL","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU PK06 66 Flush + BDX","66",1,1.2,0.97,1.1000000000000001,0.92,1,0.89,1,1.1000000000000001,0.95,0.81,0.9,0.18,0.08,0,0.18,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.28,1.29,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.57999999999999996]
["GPU PK06 66 Flush + BDX","GPU","PK06","66","ELECTRIC","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU PK06 66 Flush + BDX","66",1,1.2,0.97,1.1000000000000001,0.92,1,0.89,1,1.1000000000000001,0.95,0.81,0.9,0.18,0.08,0,0.18,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.28,1.29,0.76200000000000001,0.98,3.49,0.75,0.3600000000000001,0.57999999999999996]
["GPU PK08 57 Flush + BDX","GPU","PK08",57,"MANUAL","Flush + BDX","GPU 57","GPU 70","ok","GPU","70","GPU PK08 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.95,1.2,0.13,0.05,0,0.13,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,1.004,1.5,1.51,0.76200000000000001,1.2,3.93,0.92,0.4,0.61]
["GPU PK08 57 Flush + BDX","GPU","PK08",57,"ELECTRIC","Flush + BDX","GPU 57","GPU 70","ok","GPU","70","GPU PK08 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.95,1.2,0.13,0.05,0,0.13,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,0.06,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,1.004,1.5,1.51,0.76200000000000001,1.2,3.93,0.92,0.4,0.61]
["GPU PK08 62 Flush + BDX","GPU","PK08","62","MANUAL","Flush + BDX","GPU 62","GPU 62","ok","GPU","62","GPU PK08 62 Flush + BDX","62",0.92,1.1000000000000001,0.87,1,0.83,0.97,0.81,0.95,1,0.9,0.74,0.85,0.23,7.0000000000000007E-2,0,0.23,0.08,0,0.04,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.5,1.51,0.76200000000000001,1.2,3.93,0.92,0.4,0.61]
["GPU PK08 66 Flush + BDX","GPU","PK08","66","MANUAL","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU PK08 66 Flush + BDX","66",1,1.2,0.97,1.1000000000000001,0.91,1,0.89,1,1.1000000000000001,0.95,0.8,0.9,0.18,0.08,0,0.18,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.5,1.51,0.76200000000000001,1.2,3.93,0.92,0.4,0.61]
["GPU PK08 66 Flush + BDX","GPU","PK08","66","ELECTRIC","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU PK08 66 Flush + BDX","66",1,1.2,0.97,1.1000000000000001,0.91,1,0.89,1,1.1000000000000001,0.95,0.8,0.9,0.18,0.08,0,0.18,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.5,1.51,0.76200000000000001,1.2,3.93,0.92,0.4,0.61]
["GPU PK08 76F Flush + BDX","GPU","PK08","76F","MANUAL","Flush + BDX","GPU 76F","GPU 70","ok","GPU","70","GPU PK08 70 Flush + BDX","76",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.95,1.2,0.13,0.05,0,0.13,0.05,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,1.004,1.5,1.51,0.76200000000000001,1.2,3.93,0.92,0.4,0.61]
["GPU PK10 57 Flush + BDX","GPU","PK10",57,"MANUAL","Flush + BDX","GPU 57","GPU 70","ok","GPU","70","GPU PK10 70 Flush + BDX",57,1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.95,1.2,0.13,0.05,0,0.13,0.06,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,1.004,1.7,1.71,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.63]
["GPU PK10 62 Flush + BDX","GPU","PK10","62","MANUAL","Flush + BDX","GPU 62","GPU 62","ok","GPU","62","GPU PK10 62 Flush + BDX","62",0.91,1.1000000000000001,0.86,1,0.82,0.97,0.8,0.94,1,0.89,0.73,0.85,0.24,7.0000000000000007E-2,0,0.24,0.08,0,0.04,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.43,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.7,1.71,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.63]
["GPU PK10 66 Flush + BDX","GPU","PK10","66","MANUAL","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU PK10 66 Flush + BDX","66",1,1.2,0.96,1.1000000000000001,0.91,1,0.88,1,1.1000000000000001,0.95,0.8,0.9,0.19,0.08,0,0.19,0.09,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.7,1.71,0.76200000000000001,1.41,4.33,1.07,0.43999999999999995,0.63]
["GPU SK06 57 Flush + BDX","GPU","SK06",57,"MANUAL","Flush + BDX","GPU 57","GPU 70","ok","GPU","70","GPU SK06 70 Flush + BDX",57,1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.93,1.1000000000000001,0.13,0.05,0,0.13,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GPU SK06 57 Flush + BDX","GPU","SK06",57,"ELECTRIC","Flush + BDX","GPU 57","GPU 70","ok","GPU","70","GPU SK06 70 Flush + BDX",57,1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.93,1.1000000000000001,0.13,0.05,0,0.13,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GPU SK06 62 Flush + BDX","GPU","SK06","62","MANUAL","Flush + BDX","GPU 62","GPU 62","ok","GPU","62","GPU SK06 62 Flush + BDX","62",0.89,1.1000000000000001,0.85,1,0.81,0.95,0.79,0.93,1,0.88,0.72,0.84,0.23,7.0000000000000007E-2,0,0.23,0.08,0,0.04,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GPU SK06 66 Flush + BDX","GPU","SK06","66","MANUAL","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU SK06 66 Flush + BDX","66",1,1.2,0.95,1.1000000000000001,0.89,1,0.87,1,1.1000000000000001,0.94,0.79,0.89,0.19,0.08,0,0.19,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GPU SK06 66 Flush + BDX","GPU","SK06","66","ELECTRIC","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU SK06 66 Flush + BDX","66",1,1.2,0.95,1.1000000000000001,0.89,1,0.87,1,1.1000000000000001,0.94,0.79,0.89,0.19,0.08,0,0.19,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GPU SK06 76F Flush + BDX","GPU","SK06","76F","MANUAL","Flush + BDX","GPU 76F","GPU 70","ok","GPU","70","GPU SK06 70 Flush + BDX","76",1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.93,1.1000000000000001,0.13,0.05,0,0.13,0.05,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,1.202,1.28,1.54,0.96,0.98,3.89,0.94,0.40000000000000013,0.61]
["GPU SK08 57 Flush + BDX","GPU","SK08",57,"MANUAL","Flush + BDX","GPU 57","GPU 70","ok","GPU","70","GPU SK08 70 Flush + BDX",57,1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.93,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GPU SK08 57 Flush + BDX","GPU","SK08",57,"ELECTRIC","Flush + BDX","GPU 57","GPU 70","ok","GPU","70","GPU SK08 70 Flush + BDX",57,1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.93,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GPU SK08 62 Flush + BDX","GPU","SK08","62","MANUAL","Flush + BDX","GPU 62","GPU 62","ok","GPU","62","GPU SK08 62 Flush + BDX","62",0.88,1.1000000000000001,0.83,1,0.79,0.95,0.77,0.92,1,0.87,0.71,0.83,0.24,0.08,0,0.24,0.08,0,0.04,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GPU SK08 66 Flush + BDX","GPU","SK08","66","MANUAL","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU SK08 66 Flush + BDX","66",0.98,1.2,0.93,1.1000000000000001,0.88,1,0.86,0.99,1.1000000000000001,0.93,0.78,0.88,0.19,0.08,0,0.19,0.09,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GPU SK08 66 Flush + BDX","GPU","SK08","66","ELECTRIC","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU SK08 66 Flush + BDX","66",0.98,1.2,0.93,1.1000000000000001,0.88,1,0.86,0.99,1.1000000000000001,0.93,0.78,0.88,0.19,0.08,0,0.19,0.09,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GPU SK08 76F Flush + BDX","GPU","SK08","76F","MANUAL","Flush + BDX","GPU 76F","GPU 70","ok","GPU","70","GPU SK08 70 Flush + BDX","76",1.2,1.7,1.2,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.93,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GPU SK10 66 Flush + BDX","GPU","SK10","66","MANUAL","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU SK10 66 Flush + BDX","66",0.97,1.2,0.92,1.1000000000000001,0.87,1,0.85,0.98,1.1000000000000001,0.93,0.77,0.88,0.2,0.08,0,0.2,0.09,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.7,2.0499999999999998,0.96,1.41,4.7300000000000004,1.35,0.47,0.66]
["GPU UK08 57 Flush + BDX","GPU","UK08","57","MANUAL","Flush + BDX","GPU 57","GPU 70","ok","GPU","70","GPU UK08 70 Flush + BDX","57",1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.92,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.06,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,1.4020000000000001,1.5,2.1,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.66]
["GPU UK08 66 Flush + BDX","GPU","UK08","66","MANUAL","Flush + BDX","GPU 66","GPU 66","ok","GPU","66","GPU UK08 66 Flush + BDX","66",0.95,1.1000000000000001,0.9,1.1000000000000001,0.85,1,0.83,0.97,1.1000000000000001,0.92,0.76,0.87,0.2,0.08,0,0.2,0.09,0,0.03,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.5,2.1,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.66]
["GPU UK08 76F Flush + BDX","GPU","UK08","76F","MANUAL","Flush + BDX","GPU 76F","GPU 70","ok","GPU","70","GPU UK08 70 Flush + BDX","76",1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.92,1.2,0.14000000000000001,0.05,0,0.14000000000000001,0.05,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"https://base-inies.fr/consultation/infos-produit/42367 ",422,1.4020000000000001,1.5,2.1,1.1600000000000001,1.2,4.7300000000000004,1.39,0.4800000000000002,0.66]
["GTL MK08 66 Flush + BDX","GTL","MK08","66","MANUAL","Flush + BDX","GTL 66","GPL 66","ok","GPL","66","GPL MK08 66 Flush + BDX","66",1.1000000000000001,1.2,0.99,1.1000000000000001,0.94,1.1000000000000001,0.91,1,1.1000000000000001,0.98,0.82,0.92,0.17,0.08,0,0.17,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GTL MK08 70 Flush + BDX","GTL","MK08","70","MANUAL","Flush + BDX","GTL 70","GPL 70","ok","GPL","70","GPL MK08 70 Flush + BDX","70",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.95,1.2,0.22,0.06,0,0.22,0.06,0,0.04,0.09,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.39,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GTL SK08 66 Flush + BDX","GTL","SK08","66","MANUAL","Flush + BDX","GTL 66","GPL 66","ok","GPL","66","GPL SK08 66 Flush + BDX","66",0.97,1.2,0.92,1.1000000000000001,0.87,1,0.85,0.99,1.1000000000000001,0.93,0.77,0.88,0.19,0.08,0,0.19,0.09,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GTL SK08 70 Flush + BDX","GTL","SK08","70","MANUAL","Flush + BDX","GTL 70","GPL 70","ok","GPL","70","GPL SK08 70 Flush + BDX","70",1.2,1.7,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.92,1.2,0.24,0.06,0,0.24,0.06,0,0.05,0.08,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.44,0,0.08,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GTU MK08 66 Flush + BDX","GTU","MK08","66","MANUAL","Flush + BDX","GTU 66","GPU 66","ok","GPU","66","GPU MK08 66 Flush + BDX","66",1.1000000000000001,1.2,1,1.1000000000000001,0.96,1.1000000000000001,0.93,1,1.1000000000000001,0.98,0.84,0.92,0.17,0.08,0,0.17,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.5,1.26,0.60000000000000009,1.2,3.61,0.72,0.37000000000000011,0.56999999999999995]
["GTU SK08 66 Flush + BDX","GTU","SK08","66","MANUAL","Flush + BDX","GTU 66","GPU 66","ok","GPU","66","GPU SK08 66 Flush + BDX","66",0.98,1.2,0.93,1.1000000000000001,0.88,1,0.86,0.99,1.1000000000000001,0.93,0.78,0.88,0.19,0.08,0,0.19,0.09,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.5,1.8,0.96,1.2,4.33,1.1499999999999999,0.44000000000000017,0.64]
["GXU CK04 66 Flush + BDX","GXU","CK04","66","MANUAL","Flush + BDX","GXU 66","GPU 66","ok","GPU","66","GPU CK04 66 Flush + BDX","66",1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.1000000000000001,1,1.1000000000000001,1.2,1,0.92,0.97,0.13,7.0000000000000007E-2,0,0.13,7.0000000000000007E-2,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.27,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,1.08,0.66,0.37000000000000005,0.78,2.31,0.28999999999999998,0.25000000000000006,0.44]
["GXU CK06 66 Flush + BDX","GXU","CK06","66","MANUAL","Flush + BDX","GXU 66","GPU 66","ok","GPU","66","GPU CK06 66 Flush + BDX","66",1.2,1.3,1.1000000000000001,1.2,1.1000000000000001,1.1000000000000001,1,1.1000000000000001,1.2,1,0.91,0.97,0.14000000000000001,7.0000000000000007E-2,0,0.14000000000000001,0.08,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.28999999999999998,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.6120000000000001,1.28,0.78,0.37000000000000005,0.98,2.71,0.36,0.29000000000000004,0.46]
["GXU FK06 66 Flush + BDX","GXU","FK06","66","MANUAL","Flush + BDX","GXU 66","GPU 66","ok","GPU","66","GPU FK06 66 Flush + BDX","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.98,1.1000000000000001,1.2,1,0.87,0.95,0.15,7.0000000000000007E-2,0,0.15,0.08,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.32,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.72199999999999998,1.28,0.92,0.48000000000000004,0.98,2.93,0.47,0.31000000000000005,0.51]
["VFE MK31 57 Flush + BDX","VFE","MK31","57","MANUAL","Flush + BDX","VFE 57","GPL 70","ok","GPL","70","GPL MK31 70 Flush + BDX","57",1.3,1.6,1.2,1.5,1.1000000000000001,1.3,1.1000000000000001,1.3,1.5,1.2,0.97,1.1000000000000001,0.09,0.04,0,0.09,0.05,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.25,0,0.04,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,0.7,0.59,0.60000000000000009,0.41,2.0099999999999998,0.24,0.22999999999999998,0.41]
["VFE MK31 62 Flush + BDX","VFE","MK31","62","MANUAL","Flush + BDX","VFE 62","VFE 62","ok","VFE","62","VFE MK31 62 Flush + BDX","62",1.1000000000000001,1.2,1,1.1000000000000001,0.94,1.1000000000000001,0.92,1,1.1000000000000001,0.96,0.83,0.91,0.18,7.0000000000000007E-2,0,0.18,7.0000000000000007E-2,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.32,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,0.7,0.59,0.60000000000000009,0.41,2.0099999999999998,0.24,0.22999999999999998,0.41]
["VFE MK31 66 Flush + BDX","VFE","MK31","66","MANUAL","Flush + BDX","VFE 66","GPL 66","ok","GPL","66","GPL MK31 66 Flush + BDX","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.98,1.1000000000000001,1.2,1,0.88,0.95,0.12,0.06,0,0.12,7.0000000000000007E-2,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.26,0,0.04,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,0.7,0.59,0.60000000000000009,0.41,2.0099999999999998,0.24,0.22999999999999998,0.41]
["VFE MK31 70 Flush + BDX","VFE","MK31","70","MANUAL","Flush + BDX","VFE 70","GPL 70","ok","GPL","70","GPL MK31 70 Flush + BDX","70",1.3,1.6,1.2,1.5,1.1000000000000001,1.3,1.1000000000000001,1.3,1.5,1.2,0.97,1.1000000000000001,0.16,0.05,0,0.16,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.28000000000000003,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,0.7,0.59,0.60000000000000009,0.41,2.0099999999999998,0.24,0.22999999999999998,0.41]
["VFE MK35 57 Flush + BDX","VFE","MK35","57","MANUAL","Flush + BDX","VFE 57","GPL 70","ok","GPL","70","GPL MK35 70 Flush + BDX","57",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.96,1.1000000000000001,0.11,0.05,0,0.11,0.06,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.31,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.06,0.89,0.60000000000000009,0.76,2.72,0.45,0.28999999999999998,0.51]
["VFE MK35 66 Flush + BDX","VFE","MK35","66","MANUAL","Flush + BDX","VFE 66","GPL 66","ok","GPL","66","GPL MK35 66 Flush + BDX","66",1.1000000000000001,1.2,1,1.2,0.97,1.1000000000000001,0.94,1.1000000000000001,1.2,0.99,0.84,0.93,0.15,7.0000000000000007E-2,0,0.15,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.32,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.06,0.89,0.60000000000000009,0.76,2.72,0.45,0.28999999999999998,0.51]
["VFE MK35 70 Flush + BDX","VFE","MK35","70","MANUAL","Flush + BDX","VFE 70","GPL 70","ok","GPL","70","GPL MK35 70 Flush + BDX","70",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.96,1.1000000000000001,0.2,0.06,0,0.2,0.06,0,0.04,0.09,0,0.13,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.06,0.89,0.60000000000000009,0.76,2.72,0.45,0.28999999999999998,0.51]
["VFE PK31 57 Flush + BDX","VFE","PK31","57","MANUAL","Flush + BDX","VFE 57","GPL 70","ok","GPL","70","GPL PK31 70 Flush + BDX","57",1.3,1.6,1.2,1.5,1.1000000000000001,1.3,1.1000000000000001,1.3,1.5,1.2,0.96,1.1000000000000001,0.09,0.04,0,0.09,0.05,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.27,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,0.7,0.7,0.76200000000000001,0.41,2.34,0.31,0.25999999999999995,0.44]
["VFE PK31 62 Flush + BDX","VFE","PK31","62","MANUAL","Flush + BDX","VFE 62","VFE 62","ok","VFE","62","VFE PK31 62 Flush + BDX","62",1,1.2,0.97,1.1000000000000001,0.91,1,0.89,1,1.1000000000000001,0.94,0.8,0.89,0.19,7.0000000000000007E-2,0,0.19,7.0000000000000007E-2,0,0.03,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,0.7,0.7,0.76200000000000001,0.41,2.34,0.31,0.25999999999999995,0.44]
["VFE PK31 66 Flush + BDX","VFE","PK31","66","MANUAL","Flush + BDX","VFE 66","GPL 66","ok","GPL","66","GPL PK31 66 Flush + BDX","66",1.1000000000000001,1.3,1,1.2,0.99,1.1000000000000001,0.96,1.1000000000000001,1.2,0.99,0.86,0.93,0.13,7.0000000000000007E-2,0,0.13,7.0000000000000007E-2,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.27,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,0.7,0.7,0.76200000000000001,0.41,2.34,0.31,0.25999999999999995,0.44]
["VFE PK31 70 Flush + BDX","VFE","PK31","70","MANUAL","Flush + BDX","VFE 70","GPL 70","ok","GPL","70","GPL PK31 70 Flush + BDX","70",1.3,1.6,1.2,1.5,1.1000000000000001,1.3,1.1000000000000001,1.3,1.5,1.2,0.96,1.1000000000000001,0.17,0.05,0,0.17,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.3,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,0.7,0.7,0.76200000000000001,0.41,2.34,0.31,0.25999999999999995,0.44]
["VFE PK35 57 Flush + BDX","VFE","PK35","57","MANUAL","Flush + BDX","VFE 57","GPL 70","ok","GPL","70","GPL PK35 70 Flush + BDX","57",1.3,1.6,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.94,1.1000000000000001,0.11,0.04,0,0.11,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.32,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.06,1.06,0.76200000000000001,0.76,3.04,0.57999999999999996,0.32000000000000006,0.55000000000000004]
["VFE PK35 62 Flush + BDX","VFE","PK35","62","MANUAL","Flush + BDX","VFE 62","VFE 62","ok","VFE","62","VFE PK35 62 Flush + BDX","62",0.97,1.1000000000000001,0.91,1.1000000000000001,0.87,1,0.84,0.97,1.1000000000000001,0.92,0.77,0.87,0.21,7.0000000000000007E-2,0,0.21,0.08,0,0.04,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.06,1.06,0.76200000000000001,0.76,3.04,0.57999999999999996,0.32000000000000006,0.55000000000000004]
["VFE PK35 66 Flush + BDX","VFE","PK35","66","MANUAL","Flush + BDX","VFE 66","GPL 66","ok","GPL","66","GPL PK35 66 Flush + BDX","66",1,1.2,0.99,1.1000000000000001,0.93,1.1000000000000001,0.91,1,1.1000000000000001,0.96,0.82,0.91,0.16,7.0000000000000007E-2,0,0.16,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.06,1.06,0.76200000000000001,0.76,3.04,0.57999999999999996,0.32000000000000006,0.55000000000000004]
["VFE PK35 70 Flush + BDX","VFE","PK35","70","MANUAL","Flush + BDX","VFE 70","GPL 70","ok","GPL","70","GPL PK35 70 Flush + BDX","70",1.3,1.6,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.94,1.1000000000000001,0.2,0.06,0,0.2,0.06,0,0.04,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.06,1.06,0.76200000000000001,0.76,3.04,0.57999999999999996,0.32000000000000006,0.55000000000000004]
["VFE SK31 57 Flush + BDX","VFE","SK31","57","MANUAL","Flush + BDX","VFE 57","GPL 70","ok","GPL","70","GPL SK31 70 Flush + BDX","57",1.3,1.6,1.2,1.5,1.1000000000000001,1.3,1.1000000000000001,1.3,1.5,1.2,0.95,1.1000000000000001,0.1,0.04,0,0.1,0.05,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.28000000000000003,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,0.7,0.84,0.96,0.41,2.73,0.39,0.29000000000000004,0.46]
["VFE SK31 66 Flush + BDX","VFE","SK31","66","MANUAL","Flush + BDX","VFE 66","GPL 66","ok","GPL","66","GPL SK31 66 Flush + BDX","66",1.1000000000000001,1.2,1,1.1000000000000001,0.97,1.1000000000000001,0.94,1,1.1000000000000001,0.98,0.84,0.92,0.14000000000000001,7.0000000000000007E-2,0,0.14000000000000001,7.0000000000000007E-2,0,0.02,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.28999999999999998,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,0.7,0.84,0.96,0.41,2.73,0.39,0.29000000000000004,0.46]
["VFE SK31 62 Flush + BDX","VFE","SK31","62","MANUAL","Flush + BDX","VFE 62","VFE 62","ok","VFE","62","VFE SK31 62 Flush + BDX","62",1,1.2,0.94,1.1000000000000001,0.89,1,0.87,0.98,1.1000000000000001,0.93,0.78,0.88,0.2,7.0000000000000007E-2,0,0.2,7.0000000000000007E-2,0,0.03,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,0.7,0.84,0.96,0.41,2.73,0.39,0.29000000000000004,0.46]
["VFE SK31 70 Flush + BDX","VFE","SK31","70","MANUAL","Flush + BDX","VFE 70","GPL 70","ok","GPL","70","GPL SK31 70 Flush + BDX","70",1.3,1.6,1.2,1.5,1.1000000000000001,1.3,1.1000000000000001,1.3,1.5,1.2,0.95,1.1000000000000001,0.18,0.05,0,0.18,0.05,0,0.03,0.09,0,0.12,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.32,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,0.7,0.84,0.96,0.41,2.73,0.39,0.29000000000000004,0.46]
["VFE SK35 57 Flush + BDX","VFE","SK35","57","MANUAL","Flush + BDX","VFE 57","GPL 70","ok","GPL","70","GPL SK35 70 Flush + BDX","57",1.2,1.6,1.2,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.93,1.1000000000000001,0.12,0.04,0,0.12,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.06,1.27,0.96,0.76,3.44,0.73,0.3600000000000001,0.56999999999999995]
["VFE SK35 62 Flush + BDX","VFE","SK35","62","MANUAL","Flush + BDX","VFE 62","VFE 62","ok","VFE","62","VFE SK35 62 Flush + BDX","62",0.93,1.1000000000000001,0.88,1,0.83,0.98,0.81,0.95,1,0.9,0.74,0.85,0.23,7.0000000000000007E-2,0,0.23,0.08,0,0.04,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.41,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.06,1.27,0.96,0.76,3.44,0.73,0.3600000000000001,0.56999999999999995]
["VFE SK35 66 Flush + BDX","VFE","SK35","66","MANUAL","Flush + BDX","VFE 66","GPL 66","ok","GPL","66","GPL SK35 66 Flush + BDX","66",1,1.2,0.96,1.1000000000000001,0.91,1,0.88,1,1.1000000000000001,0.95,0.8,0.9,0.17,7.0000000000000007E-2,0,0.17,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.06,1.27,0.96,0.76,3.44,0.73,0.3600000000000001,0.56999999999999995]
["VFE SK35 70 Flush + BDX","VFE","SK35","70","MANUAL","Flush + BDX","VFE 70","GPL 70","ok","GPL","70","GPL SK35 70 Flush + BDX","70",1.2,1.6,1.2,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.93,1.1000000000000001,0.21,0.06,0,0.21,0.06,0,0.04,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.06,1.27,0.96,0.76,3.44,0.73,0.3600000000000001,0.56999999999999995]
["VFE UK31 57 Flush + BDX","VFE","UK31","57","MANUAL","Flush + BDX","VFE 57","GPL 70","ok","GPL","70","GPL UK31 70 Flush + BDX","57",1.3,1.6,1.2,1.5,1.1000000000000001,1.3,1.1000000000000001,1.3,1.5,1.2,0.94,1.1000000000000001,0.1,0.04,0,0.1,0.05,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.28999999999999998,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,0.7,0.98,1.1600000000000001,0.41,3.13,0.47,0.33000000000000007,0.48]
["VFE UK31 62 Flush + BDX","VFE","UK31","62","MANUAL","Flush + BDX","VFE 62","VFE 62","ok","VFE","62","VFE UK31 62 Flush + BDX","62",0.97,1.1000000000000001,0.92,1.1000000000000001,0.87,1,0.85,0.97,1.1000000000000001,0.92,0.77,0.87,0.2,7.0000000000000007E-2,0,0.2,7.0000000000000007E-2,0,0.04,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.37,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,0.7,0.98,1.1600000000000001,0.41,3.13,0.47,0.33000000000000007,0.48]
["VFE UK31 66 Flush + BDX","VFE","UK31","66","MANUAL","Flush + BDX","VFE 66","GPL 66","ok","GPL","66","GPL UK31 66 Flush + BDX","66",1.1000000000000001,1.2,1,1.1000000000000001,0.95,1.1000000000000001,0.92,1,1.1000000000000001,0.97,0.83,0.92,0.14000000000000001,7.0000000000000007E-2,0,0.14000000000000001,7.0000000000000007E-2,0,0.02,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.3,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,0.7,0.98,1.1600000000000001,0.41,3.13,0.47,0.33000000000000007,0.48]
["VFE UK31 70 Flush + BDX","VFE","UK31","70","MANUAL","Flush + BDX","VFE 70","GPL 70","ok","GPL","70","GPL UK31 70 Flush + BDX","70",1.3,1.6,1.2,1.5,1.1000000000000001,1.3,1.1000000000000001,1.3,1.5,1.2,0.94,1.1000000000000001,0.18,0.05,0,0.18,0.05,0,0.03,0.09,0,0.12,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,0.7,0.98,1.1600000000000001,0.41,3.13,0.47,0.33000000000000007,0.48]
["VFE UK35 57 Flush + BDX","VFE","UK35","57","MANUAL","Flush + BDX","VFE 57","GPL 70","ok","GPL","70","GPL UK35 70 Flush + BDX","57",1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.92,1.1000000000000001,0.12,0.05,0,0.12,0.06,0,0.02,0.08,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.06,1.48,1.1600000000000001,0.76,3.84,0.88,0.4,0.59]
["VFE UK35 62 Flush + BDX","VFE","UK35","62","MANUAL","Flush + BDX","VFE 62","VFE 62","ok","VFE","62","VFE UK35 62 Flush + BDX","62",0.9,1.1000000000000001,0.85,1,0.81,0.96,0.79,0.93,1,0.88,0.72,0.84,0.23,7.0000000000000007E-2,0,0.23,0.08,0,0.04,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.42,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.06,1.48,1.1600000000000001,0.76,3.84,0.88,0.4,0.59]
["VFE UK35 66 Flush + BDX","VFE","UK35","66","MANUAL","Flush + BDX","VFE 66","GPL 66","ok","GPL","66","GPL UK35 66 Flush + BDX","66",0.99,1.2,0.94,1.1000000000000001,0.89,1,0.86,0.99,1.1000000000000001,0.94,0.78,0.89,0.17,7.0000000000000007E-2,0,0.17,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.06,1.48,1.1600000000000001,0.76,3.84,0.88,0.4,0.59]
["VFE UK35 70 Flush + BDX","VFE","UK35","70","MANUAL","Flush + BDX","VFE 70","GPL 70","ok","GPL","70","GPL UK35 70 Flush + BDX","70",1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.92,1.1000000000000001,0.22,0.06,0,0.22,0.06,0,0.04,0.08,0,0.13,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.4,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.06,1.48,1.1600000000000001,0.76,3.84,0.88,0.4,0.59]
["VIU MK31 57 Flush + BDX","VIU","MK31","57","FIXED","Flush + BDX","VIU 57","GPU 70","ok","GPU","70","GPU MK31 70 Flush + BDX","57",1.3,1.6,1.2,1.5,1.2,1.3,1.1000000000000001,1.3,1.5,1.2,0.98,1.1000000000000001,0.09,0.04,0,0.09,0.05,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,0.08,0,0.08,0.25,0,0.04,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,0.7,0.59,0.60000000000000009,0.41,2.0099999999999998,0.24,0.22999999999999998,0.41]
["VIU MK31 62 Flush + BDX","VIU","MK31","62","FIXED","Flush + BDX","VIU 62","GIU 62","ok","GIU","62","GIU MK31 62 Flush + BDX","62",1.1000000000000001,1.2,1,1.2,0.99,1.1000000000000001,0.96,1,1.2,0.99,0.86,0.93,0.16,0.06,0,0.16,7.0000000000000007E-2,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.28000000000000003,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,0.7,0.59,0.60000000000000009,0.41,2.0099999999999998,0.24,0.22999999999999998,0.41]
["VIU MK31 66 Flush + BDX","VIU","MK31","66","FIXED","Flush + BDX","VIU 66","GPU 66","ok","GPU","66","GPU MK31 66 Flush + BDX","66",1.2,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.99,1.1000000000000001,1.2,1,0.89,0.95,0.12,7.0000000000000007E-2,0,0.12,7.0000000000000007E-2,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.26,0,0.04,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,0.7,0.59,0.60000000000000009,0.41,2.0099999999999998,0.24,0.22999999999999998,0.41]
["VIU MK35 57 Flush + BDX","VIU","MK35","57","FIXED","Flush + BDX","VIU 57","GPU 70","ok","GPU","70","GPU MK35 70 Flush + BDX","57",1.3,1.7,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.97,1.1000000000000001,0.11,0.05,0,0.11,0.06,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.31,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.06,0.89,0.60000000000000009,0.76,2.72,0.45,0.28999999999999998,0.51]
["VIU MK35 62 Flush + BDX","VIU","MK35","62","FIXED","Flush + BDX","VIU 62","GIU 62","ok","GIU","62","GIU MK35 62 Flush + BDX","62",1.1000000000000001,1.2,0.99,1.1000000000000001,0.93,1.1000000000000001,0.91,1,1.1000000000000001,0.96,0.82,0.91,0.19,7.0000000000000007E-2,0,0.19,7.0000000000000007E-2,0,0.03,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.35,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.06,0.89,0.60000000000000009,0.76,2.72,0.45,0.28999999999999998,0.51]
["VIU MK35 66 Flush + BDX","VIU","MK35","66","FIXED","Flush + BDX","VIU 66","GPU 66","ok","GPU","66","GPU MK35 66 Flush + BDX","66",1.1000000000000001,1.2,1,1.2,0.98,1.1000000000000001,0.95,1.1000000000000001,1.2,0.99,0.86,0.93,0.15,7.0000000000000007E-2,0,0.15,0.08,0,0.03,0.09,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.32,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,0.84200000000000008,1.06,0.89,0.60000000000000009,0.76,2.72,0.45,0.28999999999999998,0.51]
["VIU PK31 57 Flush + BDX","VIU","PK31","57","FIXED","Flush + BDX","VIU 57","GPU 70","ok","GPU","70","GPU PK31 70 Flush + BDX","57",1.3,1.6,1.2,1.5,1.1000000000000001,1.3,1.1000000000000001,1.3,1.5,1.2,0.97,1.1000000000000001,0.09,0.04,0,0.09,0.05,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.27,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,0.7,0.7,0.76200000000000001,0.41,2.33,0.31,0.25999999999999995,0.44]
["VIU PK31 62 Flush + BDX","VIU","PK31","62","FIXED","Flush + BDX","VIU 62","GIU 62","ok","GIU","62","GIU PK31 62 Flush + BDX","62",1.1000000000000001,1.2,1,1.1000000000000001,0.96,1.1000000000000001,0.93,1,1.1000000000000001,0.97,0.84,0.92,0.17,0.06,0,0.17,7.0000000000000007E-2,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.3,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,0.7,0.7,0.76200000000000001,0.41,2.33,0.31,0.25999999999999995,0.44]
["VIU PK31 66 Flush + BDX","VIU","PK31","66","FIXED","Flush + BDX","VIU 66","GPU 66","ok","GPU","66","GPU PK31 66 Flush + BDX","66",1.1000000000000001,1.3,1.1000000000000001,1.2,1,1.1000000000000001,0.97,1.1000000000000001,1.2,0.99,0.87,0.93,0.13,7.0000000000000007E-2,0,0.13,7.0000000000000007E-2,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.27,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,0.7,0.7,0.76200000000000001,0.41,2.33,0.31,0.25999999999999995,0.44]
["VIU PK35 57 Flush + BDX","VIU","PK35","57","FIXED","Flush + BDX","VIU 57","GPU 70","ok","GPU","70","GPU PK35 70 Flush + BDX","57",1.3,1.6,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.95,1.1000000000000001,0.11,0.05,0,0.11,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.32,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.06,1.06,0.76200000000000001,0.76,3.04,0.57999999999999996,0.32000000000000006,0.55000000000000004]
["VIU PK35 62 Flush + BDX","VIU","PK35","62","FIXED","Flush + BDX","VIU 62","GIU 62","ok","GIU","62","GIU PK35 62 Flush + BDX","62",1,1.2,0.95,1.1000000000000001,0.9,1,0.88,0.99,1.1000000000000001,0.94,0.79,0.89,0.2,7.0000000000000007E-2,0,0.2,7.0000000000000007E-2,0,0.03,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.06,1.06,0.76200000000000001,0.76,3.04,0.57999999999999996,0.32000000000000006,0.55000000000000004]
["VIU PK35 66 Flush + BDX","VIU","PK35","66","FIXED","Flush + BDX","VIU 66","GPU 66","ok","GPU","66","GPU PK35 66 Flush + BDX","66",1.1000000000000001,1.2,1,1.1000000000000001,0.94,1.1000000000000001,0.92,1,1.1000000000000001,0.96,0.83,0.91,0.16,7.0000000000000007E-2,0,0.16,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.33,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.004,1.06,1.06,0.76200000000000001,0.76,3.04,0.57999999999999996,0.32000000000000006,0.55000000000000004]
["VIU SK31 57 Flush + BDX","VIU","SK31","57","FIXED","Flush + BDX","VIU 57","GPU 70","ok","GPU","70","GPU SK31 70 Flush + BDX","57",1.3,1.6,1.2,1.5,1.1000000000000001,1.3,1.1000000000000001,1.3,1.5,1.2,0.96,1.1000000000000001,0.1,0.04,0,0.1,0.05,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.28000000000000003,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,0.7,0.84,0.96,0.41,2.73,0.39,0.29000000000000004,0.46]
["VIU SK31 62 Flush + BDX","VIU","SK31","62","FIXED","Flush + BDX","VIU 62","GIU 62","ok","GIU","62","GIU SK31 62 Flush + BDX","62",1.1000000000000001,1.2,1,1.1000000000000001,0.94,1,0.91,1,1.1000000000000001,0.96,0.82,0.91,0.18,7.0000000000000007E-2,0,0.18,7.0000000000000007E-2,0,0.03,0.08,0,0.11,0,0.05,0,0.05,0,0.06,0,0.06,0.32,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,0.7,0.84,0.96,0.41,2.73,0.39,0.29000000000000004,0.46]
["VIU SK31 66 Flush + BDX","VIU","SK31","66","FIXED","Flush + BDX","VIU 66","GPU 66","ok","GPU","66","GPU SK31 66 Flush + BDX","66",1.1000000000000001,1.2,1,1.1000000000000001,0.98,1.1000000000000001,0.95,1,1.1000000000000001,0.98,0.85,0.92,0.14000000000000001,7.0000000000000007E-2,0,0.14000000000000001,7.0000000000000007E-2,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.28999999999999998,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,0.7,0.84,0.96,0.41,2.73,0.39,0.29000000000000004,0.46]
["VIU SK35 57 Flush + BDX","VIU","SK35","57","FIXED","Flush + BDX","VIU 57","GPU 70","ok","GPU","70","GPU SK35 70 Flush + BDX","57",1.2,1.6,1.2,1.5,1.1000000000000001,1.4,1.1000000000000001,1.3,1.5,1.2,0.93,1.1000000000000001,0.12,0.05,0,0.12,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.06,1.27,0.96,0.76,3.44,0.73,0.3600000000000001,0.56999999999999995]
["VIU SK35 62 Flush + BDX","VIU","SK35","62","FIXED","Flush + BDX","VIU 62","GIU 62","ok","GIU","62","GIU SK35 62 Flush + BDX","62",0.97,1.1000000000000001,0.92,1.1000000000000001,0.87,1,0.85,0.97,1.1000000000000001,0.92,0.77,0.87,0.21,7.0000000000000007E-2,0,0.21,0.08,0,0.04,7.0000000000000007E-2,0,0.11,0,0.05,0,0.05,0,0.05,0,0.05,0.38,0,7.0000000000000007E-2,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.06,1.27,0.96,0.76,3.44,0.73,0.3600000000000001,0.56999999999999995]
["VIU SK35 66 Flush + BDX","VIU","SK35","66","FIXED","Flush + BDX","VIU 66","GPU 66","ok","GPU","66","GPU SK35 66 Flush + BDX","66",1,1.2,0.97,1.1000000000000001,0.91,1,0.89,1,1.1000000000000001,0.95,0.8,0.9,0.17,7.0000000000000007E-2,0,0.17,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.34,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.202,1.06,1.27,0.96,0.76,3.44,0.73,0.3600000000000001,0.56999999999999995]
["VIU UK31 57 Flush + BDX","VIU","UK31","57","FIXED","Flush + BDX","VIU 57","GPU 70","ok","GPU","70","GPU UK31 70 Flush + BDX","57",1.3,1.6,1.2,1.5,1.1000000000000001,1.3,1.1000000000000001,1.3,1.5,1.2,0.95,1.1000000000000001,0.1,0.04,0,0.1,0.05,0,0.02,0.09,0,0.11,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.28999999999999998,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,0.7,0.98,1.1600000000000001,0.41,3.13,0.47,0.33000000000000007,0.48]
["VIU UK31 66 Flush + BDX","VIU","UK31","66","FIXED","Flush + BDX","VIU 66","GPU 66","ok","GPU","66","GPU UK31 66 Flush + BDX","66",1.1000000000000001,1.2,1,1.1000000000000001,0.96,1.1000000000000001,0.93,1,1.1000000000000001,0.97,0.84,0.92,0.14000000000000001,7.0000000000000007E-2,0,0.14000000000000001,7.0000000000000007E-2,0,0.02,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.3,0,0.05,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,0.7,0.98,1.1600000000000001,0.41,3.13,0.47,0.33000000000000007,0.48]
["VIU UK35 57 Flush + BDX","VIU","UK35","57","FIXED","Flush + BDX","VIU 57","GPU 70","ok","GPU","70","GPU UK35 70 Flush + BDX","57",1.2,1.6,1.1000000000000001,1.5,1.1000000000000001,1.4,1,1.3,1.5,1.2,0.92,1.1000000000000001,0.12,0.05,0,0.12,0.06,0,0.02,0.09,0,0.11,0,0.06,0,0.06,0,7.0000000000000007E-2,0,7.0000000000000007E-2,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.06,1.48,1.1600000000000001,0.76,3.84,0.88,0.4,0.59]
["VIU UK35 66 Flush + BDX","VIU","UK35","66","FIXED","Flush + BDX","VIU 66","GPU 66","ok","GPU","66","GPU UK35 66 Flush + BDX","66",1,1.2,0.94,1.1000000000000001,0.89,1,0.87,0.99,1.1000000000000001,0.94,0.79,0.89,0.17,7.0000000000000007E-2,0,0.17,0.08,0,0.03,0.08,0,0.11,0,0.06,0,0.06,0,0.06,0,0.06,0.36,0,0.06,0,0,0,0,0,"Pas de FDES en ligne pour la solution choisie",422,1.4020000000000001,1.06,1.48,1.1600000000000001,0.76,3.84,0.88,0.4,0.59]

{"sheet":"climate zones","index":4,"n_rows":37,"n_cols":5,"rows_kept":37,"cut":false,"hidden":true,"merged":[]}
["Lookup","Zone climatique et altitude","Exposition au bruit et usage de la pièce","Pente et orientation","Sws max"]
[{"$f":"B2&\" \"&C2&\" \"&D2","v":"H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m Exposition BR1 - locaux destinés au sommeil Pente < 60°"},"H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m","Exposition BR1 - locaux destinés au sommeil","Pente < 60°",0.25]
[{"$f":"B3&\" \"&C3&\" \"&D3","v":"H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m Exposition BR1 - locaux destinés au sommeil Pente>60° orientation autre que Nord"},"H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m","Exposition BR1 - locaux destinés au sommeil","Pente>60° orientation autre que Nord",0.45]
["H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m Exposition BR1 - locaux destinés au sommeil Pente>60° orientation Nord","H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m","Exposition BR1 - locaux destinés au sommeil","Pente>60° orientation Nord",0.65]
["H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m Exposition BR2 ou BR3 - locaux destinés au sommeil Pente < 60°","H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m","Exposition BR2 ou BR3 - locaux destinés au sommeil","Pente < 60°",0.15]
["H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m Exposition BR2 ou BR3 - locaux destinés au sommeil Pente>60° orientation autre que Nord","H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m","Exposition BR2 ou BR3 - locaux destinés au sommeil","Pente>60° orientation autre que Nord",0.25]
["H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m Exposition BR2 ou BR3 - locaux destinés au sommeil Pente>60° orientation Nord","H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m","Exposition BR2 ou BR3 - locaux destinés au sommeil","Pente>60° orientation Nord",0.45]
["H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m Exposition BR1 - hors locaux destinés au sommeil Pente < 60°","H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m","Exposition BR1 - hors locaux destinés au sommeil","Pente < 60°",0.45]
["H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m Exposition BR1 - hors locaux destinés au sommeil Pente>60° orientation autre que Nord","H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m","Exposition BR1 - hors locaux destinés au sommeil","Pente>60° orientation autre que Nord",0.65]
["H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m Exposition BR1 - hors locaux destinés au sommeil Pente>60° orientation Nord","H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m","Exposition BR1 - hors locaux destinés au sommeil","Pente>60° orientation Nord",1]
["H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m Exposition BR2 ou BR3 - hors locaux destinés au sommeil Pente < 60°","H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m","Exposition BR2 ou BR3 - hors locaux destinés au sommeil","Pente < 60°",0.25]
["H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m Exposition BR2 ou BR3 - hors locaux destinés au sommeil Pente>60° orientation autre que Nord","H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m","Exposition BR2 ou BR3 - hors locaux destinés au sommeil","Pente>60° orientation autre que Nord",0.45]
["H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m Exposition BR2 ou BR3 - hors locaux destinés au sommeil Pente>60° orientation Nord","H2a toutes altitudes ou\nH1a, H1b, H2b altitude > 400 m ou\nH1c, H2c altitude > 800 m","Exposition BR2 ou BR3 - hors locaux destinés au sommeil","Pente>60° orientation Nord",1]
["H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m Exposition BR1 - locaux destinés au sommeil Pente < 60°","H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m","Exposition BR1 - locaux destinés au sommeil","Pente < 60°",0.15]
["H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m Exposition BR1 - locaux destinés au sommeil Pente>60° orientation autre que Nord","H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m","Exposition BR1 - locaux destinés au sommeil","Pente>60° orientation autre que Nord",0.25]
["H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m Exposition BR1 - locaux destinés au sommeil Pente>60° orientation Nord","H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m","Exposition BR1 - locaux destinés au sommeil","Pente>60° orientation Nord",0.45]
["H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m Exposition BR2 ou BR3 - locaux destinés au sommeil Pente < 60°","H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m","Exposition BR2 ou BR3 - locaux destinés au sommeil","Pente < 60°",0.1]
["H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m Exposition BR2 ou BR3 - locaux destinés au sommeil Pente>60° orientation autre que Nord","H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m","Exposition BR2 ou BR3 - locaux destinés au sommeil","Pente>60° orientation autre que Nord",0.15]
["H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m Exposition BR2 ou BR3 - locaux destinés au sommeil Pente>60° orientation Nord","H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m","Exposition BR2 ou BR3 - locaux destinés au sommeil","Pente>60° orientation Nord",0.25]
["H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m Exposition BR1 - hors locaux destinés au sommeil Pente < 60°","H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m","Exposition BR1 - hors locaux destinés au sommeil","Pente < 60°",0.25]
["H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m Exposition BR1 - hors locaux destinés au sommeil Pente>60° orientation autre que Nord","H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m","Exposition BR1 - hors locaux destinés au sommeil","Pente>60° orientation autre que Nord",0.45]
["H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m Exposition BR1 - hors locaux destinés au sommeil Pente>60° orientation Nord","H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m","Exposition BR1 - hors locaux destinés au sommeil","Pente>60° orientation Nord",1]
["H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m Exposition BR2 ou BR3 - hors locaux destinés au sommeil Pente < 60°","H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m","Exposition BR2 ou BR3 - hors locaux destinés au sommeil","Pente < 60°",0.15]
["H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m Exposition BR2 ou BR3 - hors locaux destinés au sommeil Pente>60° orientation autre que Nord","H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m","Exposition BR2 ou BR3 - hors locaux destinés au sommeil","Pente>60° orientation autre que Nord",0.25]
[{"$f":"B25&\" \"&C25&\" \"&D25","v":"H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m Exposition BR2 ou BR3 - hors locaux destinés au sommeil Pente>60° orientation Nord"},"H1a, H1b, H2b altitude <= 400 m ou\nH1c, H2c altitude <= 800 m ou\nH2d, H3 altitude > 400 m","Exposition BR2 ou BR3 - hors locaux destinés au sommeil","Pente>60° orientation Nord",1]
[{"$f":"B26&\" \"&C26&\" \"&D26","v":"H2d ou H3 altitude <= 400 m Exposition BR1 - locaux destinés au sommeil Pente < 60°"},"H2d ou H3 altitude <= 400 m","Exposition BR1 - locaux destinés au sommeil","Pente < 60°",0.1]
["H2d ou H3 altitude <= 400 m Exposition BR1 - locaux destinés au sommeil Pente>60° orientation autre que Nord","H2d ou H3 altitude <= 400 m","Exposition BR1 - locaux destinés au sommeil","Pente>60° orientation autre que Nord",0.15]
["H2d ou H3 altitude <= 400 m Exposition BR1 - locaux destinés au sommeil Pente>60° orientation Nord","H2d ou H3 altitude <= 400 m","Exposition BR1 - locaux destinés au sommeil","Pente>60° orientation Nord",0.25]
["H2d ou H3 altitude <= 400 m Exposition BR2 ou BR3 - locaux destinés au sommeil Pente < 60°","H2d ou H3 altitude <= 400 m","Exposition BR2 ou BR3 - locaux destinés au sommeil","Pente < 60°",0.1]
["H2d ou H3 altitude <= 400 m Exposition BR2 ou BR3 - locaux destinés au sommeil Pente>60° orientation autre que Nord","H2d ou H3 altitude <= 400 m","Exposition BR2 ou BR3 - locaux destinés au sommeil","Pente>60° orientation autre que Nord",0.15]
["H2d ou H3 altitude <= 400 m Exposition BR2 ou BR3 - locaux destinés au sommeil Pente>60° orientation Nord","H2d ou H3 altitude <= 400 m","Exposition BR2 ou BR3 - locaux destinés au sommeil","Pente>60° orientation Nord",0.25]
["H2d ou H3 altitude <= 400 m Exposition BR1 - hors locaux destinés au sommeil Pente < 60°","H2d ou H3 altitude <= 400 m","Exposition BR1 - hors locaux destinés au sommeil","Pente < 60°",0.15]
["H2d ou H3 altitude <= 400 m Exposition BR1 - hors locaux destinés au sommeil Pente>60° orientation autre que Nord","H2d ou H3 altitude <= 400 m","Exposition BR1 - hors locaux destinés au sommeil","Pente>60° orientation autre que Nord",0.25]
["H2d ou H3 altitude <= 400 m Exposition BR1 - hors locaux destinés au sommeil Pente>60° orientation Nord","H2d ou H3 altitude <= 400 m","Exposition BR1 - hors locaux destinés au sommeil","Pente>60° orientation Nord",1]
["H2d ou H3 altitude <= 400 m Exposition BR2 ou BR3 - hors locaux destinés au sommeil Pente < 60°","H2d ou H3 altitude <= 400 m","Exposition BR2 ou BR3 - hors locaux destinés au sommeil","Pente < 60°",0.15]
["H2d ou H3 altitude <= 400 m Exposition BR2 ou BR3 - hors locaux destinés au sommeil Pente>60° orientation autre que Nord","H2d ou H3 altitude <= 400 m","Exposition BR2 ou BR3 - hors locaux destinés au sommeil","Pente>60° orientation autre que Nord",0.25]
["H2d ou H3 altitude <= 400 m Exposition BR2 ou BR3 - hors locaux destinés au sommeil Pente>60° orientation Nord","H2d ou H3 altitude <= 400 m","Exposition BR2 ou BR3 - hors locaux destinés au sommeil","Pente>60° orientation Nord",1]